Consulta: subjectFacets:"Precision agriculture"
Registros recuperados: 240
Data/hora: 16/06/2024 03:13:50

Ciência e Tecnologia: a era das revoluções.
Provedor de dados: 119
Autores: LOPES, M. A.
Oferecer uma mapla visão e debater sobre o papel da agricultura da ciência e das inovações tecnológicas para o aumento da produção de alimentos e promoção do desenvolvimento de forma sustentável.
Tipo: Anais e Proceedings de eventos
Palavras-chave: Agricultura de precisão; Alimento; Segurança alimentar; Políticas públicas; Desenvolvimento econômico; Desenvolvimento sustentável; Automação; Tecnologia; Precision agriculture; Foods; Food safety; Public policy; Economic development; Sustainable development; Automation; Technology.
Ano: 2013
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/996805

Flow and pressure regulation for agricultural sprayers using solenoid valves.
Provedor de dados: 119
Autores: MERCALDI, H. V.; PEÑALOZA, E. A. G.; MARIANO, R. A.; OLIVEIRA, V. A.; CRUVINEL, P. E.
Tipo: Separatas
Palavras-chave: Applications errors; CAN bus; Curved paths.; Precision agriculture; Variable rate application.
Ano: 2017
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1078253

Clustering approaches and ensembles applied in the delineation of management classes in precision agriculture.
Provedor de dados: 119
Autores: SPERANZA, E. A.; CIFERRI, R. R.; CIFERRI, C. D. de A.
Abstract. This paper describes an experiment performed using different approaches for spatial data clustering, aiming to assist the delineation of management classes in Precision Agriculture (PA). These approaches were established from the partitional clustering algorithm Fuzzy c-Means (FCM), traditionally used in this context, and from the hierarchical clustering algorithm HACCSpatial, especially designed for this PA task. We also performed experiments using traditional ensembles approaches from the literature, evaluating their behavior to achieve consensus solutions from individual clusterings obtained from features splitting or running one of the abovementioned algorithms. Results showed some differences between FCM and HACC-Spatial, mainly for the...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Fuzzy c-Means algorithm; Spatial hierarchical clustering algorithm; Agricultura de precisão; Precision agriculture; Cluster analysis; Fuzzy logic; Spatial data.
Ano: 2016
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1079181

A geographic information system for mapping apple quality.
Provedor de dados: 119
Autores: LONGO, D.; BAZZI, L. C.; SOUZA, G. E.; GEBLER, L.; MAGALHÃES, G. S. P.
Technologies related to precision agriculture (AP) have contributed to the development of decision support systems. In this work a tool is presented that allows mapping apple quality indexes georeferenced to transform them into a graphic variable that serves as support for orchard management. The system was developed in Java language, with PostgreSQL database and geographical extension PostGIS. The system has been named "Apple Show" and can analyzed the production areas, mark the points, classify and interpolate them, presenting the results in the form of maps.
Tipo: Parte de livro
Palavras-chave: Decision support system; Geographic Information System; Precision agriculture.
Ano: 2018
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1102323

Integração de ferramentas de SIG e mineração de dados para utilização em atividades de gestão espacialmente diferenciada aplicada na agricultura de precisão.
Provedor de dados: 119
Autores: SPERANZA, E. A.; CIFERRI, R. R.
A agricultura de precisão é uma abordagem agrícola que se utiliza de tecnologias da informação e comunicação para possibilitar uma gestão diferenciada da lavoura voltada para o aumento da produtividade de maneira sustentável, reduzindo os impactos ao meio ambiente a partir da aplicação espacialmente diferenciada de insumos agrícolas e consequentemente proporcionando o aumento do retorno econômico. Um dos conceitos utilizados por essa abordagem é o delineamento de unidades de gestão diferenciada, permitindo tratamentos localizados de acordo com as características do solo e das plantas. Devido ao crescimento da disponibilidade de ferramentas computacionais que podem auxiliar usuários finais, a criação de modelos e arquiteturas acessíveis e capazes de agregar...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Sistemas de informações geográficas; Unidades de gestão diferenciada; Zonas de manejo; Dados espaciais; Mineração de dados; Differentited management units; Management zones; Data mining; Agricultura de precisão; Geographic information systems; Precision agriculture; Spatial data.
Ano: 2017
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1083394

Estratégia de implantação, gestão e funcionamento da Rede Agricultura de Precisão.
Provedor de dados: 119
Autores: INAMASU, R. Y.; BERNARDI, A. C. de C.; NAIME, J. de M.; QUEIROS, L. R.; RESENDE, A. V. de; VILELA, M. de F.; BASSOI, L. H.; PEREZ, N. B.; FRAGALLE, E. P.
Tipo: Parte de livro
Palavras-chave: Condutividade elétrica do solo; Imagem aérea; Cultura anual; Cultura perene; Inovação tecnológica; New technology.; Precision agriculture; Electrical conductivity; Soil; Databases; Annuals; Perennials.
Ano: 2011
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/907456

Soil calcium and pH monitoring sensor system
Provedor de dados: 119
Autores: LEMOS, S. G.; NOGUEIRA, A. R. de A.; TORRE NETO, A.; PARRA, A.; ALONSO, J.
An agrarian sensorial system based on temperature, moisture, and all solid-state ion-selective potentiometric sensors was developed with the objective of monitoring the behavior of H+ and Ca2+ ions in soil and in real conditions, contributing with a new tool that tries to complement the current precision agriculture technology. The evaluation of the sensorial system to pH monitoring presented a good correlation between the results obtained by the system and the standard methodology, allowing us to notice the soil buffer capacity at different soil depths. With regard to calcium, the sensor system also presented an agreement between its results and those obtained by flame atomic absorption spectrometry, using a calibration model based on multiple linear...
Tipo: Separatas
Palavras-chave: In situ soil analysis; Potentiometric sensor; Ph; Calcium; Precision agriculture.
Ano: 2007
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/32922

From visual estimates to fully automated sensor-based measurements of plant disease severity: status and challenges for improving accuracy.
Provedor de dados: 119
Autores: BOCK, C. H.; BARBEDO, J. G. A.; DEL PONTE, E. M.; BOHNENKAMP, D.; MAHLEIN, A. K.
Abstract. The severity of plant diseases, traditionally the proportion of the plant tissue exhibiting symptoms, is a key quantitative variable to know for many diseases and is prone to error. Good quality disease severity data should be accurate (close to the true value). Earliest quantification of disease severity was by visual estimates. Sensor-based image analysis including visible spectrum and hyperspectral and multispectral sensors are established technologies that promise to substitute, or complement visual ratings. Indeed, these technologies have measured disease severity accurately under controlled conditions but are yet to demonstrate their full potential for accurate measurement under field conditions. Sensor technology is advancing rapidly, and...
Tipo: Artigo de periódico
Palavras-chave: Inteligência artificial; Aprendizado de máquina; Dispositivo móvel; Tecnologias digitais; Aprendizado profundo; Precisão; Acurácia; Severidade da doença; Machine learning; Assessment; Sensor; Mobile device; Digital technologies; Deep learning; Phenotyping; Doença de Planta; Precision agriculture; Plant diseases and disorders; Artificial intelligence; Disease severity; Accuracy; Precision.
Ano: 2020
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1122199

Spectral reflectance of satellite images using geostatistics methods to estimate growth and cotton yield.
Provedor de dados: 119
Autores: BRANDAO, Z. N.; GREGO, C. R.; INAMASU, R. Y.; JORGE, L. A. de C.
The objective of this study was the spatial identification of the NDVI index and cotton yield distributions through different crop phenological stages using geostatistical methods in Goiás state, Brazil. The experiment was carried out in a commercial field with 47.4 ha, in 80x80m georeferenced grid with 74 plots. Yield monitor data and multispectral satellite images at 56 m spatial resolution were collected in a rainfed cotton field in two dates to monitor the plant vigor. Satellite images of AWiFS sensor were acquired on 08/02/2011 and 01/04/2011, during the first flowering and fruiting cotton stages, respectively, corresponding to 70 and 120DAE (days after emergence). Measures of canopy reflectance, plant height and leaf nitrogen content were determined...
Tipo: Artigo de periódico
Palavras-chave: Geostatistical analyses.; Precision agriculture; Normalized difference vegetation index.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1001261

Precision and digital agriculture: adoption of technologies and perception of Brazilian farmers.
Provedor de dados: 119
Autores: BOLFE, E. L.; JORGE, L. A. de C.; DEL'ARCO SANCHES, I.; LUCHIARI JUNIOR, A.; COSTA, C. C. da; VICTORIA, D. de C.; INAMASU, R. Y.; GREGO, C. R.; FERREIRA, V. R.; RAMIREZ, A. R.
Abstract: The rapid population growth has driven the demand for more food, fiber, energy, and water, which is associated to an increase in the need to use natural resources in a more sustainable way. The use of precision agriculture machinery and equipment since the 1990s has provided important productive gains and maximized the use of agricultural inputs. The growing connectivity in the rural environment, in addition to its greater integration with data from sensor systems, remote sensors, equipment, and smartphones have paved the way for new concepts from the so-called Agriculture 4.0 or Digital Agriculture. This article presents the results of a survey carried out with 504 Brazilian farmers about the digital technologies in use, as well as current and...
Tipo: Artigo de periódico
Palavras-chave: Agricultura digital; Smart farming; Farmer's attitudes; Digital agriculture; Agricultura de Precisão; Agriculture; Precision agriculture; Brazil.
Ano: 2020
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1128511

Efeito da variabilidade espacial de solos do Vale dos Vinhedos na composição do vinho Merlot - Safra 2012.
Provedor de dados: 119
Autores: MIELE, A.; FLORES, C. A.; FILIPPINI ALBA, J. M.
A importação de vinhos tem dificultado a comercialização de produtos nacionais. Para mitigar este efeito, é necessário aumentar a competitividade do vinho brasileiro, o que pode ser obtido pela redução de custos e melhoria da qualidade. A competitividade pode ser atingida, em parte, com a aplicação de tecnologias de agricultura de precisão. Com este objetivo, estudou-se o efeito de cinco unidades de mapeamento de solos do Vale dos Vinhedos, RS, na composição do vinho Merlot de 2012, avaliando-se 39 variáveis, cujos parâmetros foram submetidos à análise de componentes principais. Três componentes representaram 91,49% da variação total e discriminaram, principalmente, os vinhos elaborados com uvas de videiras cultivadas em Argissolo e Neossolo. Os principais...
Tipo: Parte de livro
Palavras-chave: Merlot; Agricultura de precisao; Viticultura; Manejo do solo; Precision agriculture; Viticulture; Soil management.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/986570

Computação aplicada à agricultura de precisão.
Provedor de dados: 119
Autores: HONDA, B.; JORGE, L. A. de C.
Tipo: Separatas
Palavras-chave: Processamento de imagens; Processamento multiespectral; Multispectral images; Sensoriamento Remoto; Agricultura de Precisão; Remote sensing; Precision agriculture.
Ano: 2013
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/960470

Modelo Digital de Exploração Florestal de Segunda Geração - MODEFLORA II.
Provedor de dados: 119
Autores: FIGUEIREDO, E. O.; PAPA, D. de A.; OLIVEIRA, M. V. N. d'.
Desde 2010, a Embrapa Acre desenvolve estudos com o LIDAR aerotransportado, com objetivo de desenvolver a Segunda Geração do Modelo Digital de Exploração Florestal - Modeflora II. Os procedimentos de manejo de precisão em florestas tropicais ainda apresentam um vasto campo a ser melhorado com a incorporação de técnicas de biometria florestal e escaneamento 3D em larga escala. Assim, os resultados alcançados e os métodos utilizados e adaptados pelo Embrapa Acre não pretendem esgotar o assunto, e sim, continuar um ciclo de avanços iniciados com a silvicultura e manejo de precisão.
Tipo: Parte de livro
Palavras-chave: Geotécnica; Sistema de posicionamento global; Biometria florestal; Forest biometry; Biometría forestal; Manejo florestal; Manejo de precisão; Modelagem 3D; Modeflora II; Embrapa Acre; Rio Branco (AC); Acre; Amazônia Ocidental; Western Amazon; Amazonia Occidental; Manejo forestal; Agricultura de precisión; Análisis estadístico; Geoespatial technology; Inventario forestal; Madera tropical; Sistemas de información geográfica; Sistemas de posicionamiento global; Tecnología geoespacial; Teledetección.; Administração florestal; Inventário florestal; Agricultura de precisão; Essência florestal; Sistema de informação geográfica; Sensoriamento remoto; Análise estatística.; Raio laser; Tropical wood; Forest management; Forest inventory; Precision agriculture; Geographic information systems; Global positioning systems; Remote sensing; Lidar; Statistical analysis; Lásers.
Ano: 2015
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1038719

Estimating soil loss by laminar erosion using precision agriculture computational tools.
Provedor de dados: 119
Autores: KRUG, E. T. S.; GOMES, G. J.; SOUZA, E. G. de; GEBLER, L.; SOBJAK, R.; BAZZI, C. L.
ABSTRACT: The study aimed to identify and evaluate the spatial variability in laminar erosion in areas using precision agriculture tools. Soil data from three properties in the western region of Paraná state, Brazil, were used: one in the municipality of Céu Azul (area A) and two in Serranópolis do Iguaçu (areas B and C). To identify discrepant data (outliers), analysis of the dispersion of quartiles was performed using a box-plot graph. Data normality was verified using the Kolmogorov-Smirnov test. A spatial analysis was performed using AgDataBox-Map software. The parameters of the universal soil loss equation were estimated and used with map algebra to produce a model to identify areas susceptible to erosion. Area A (soil loss estimate = 0-200 t ha-1 per...
Tipo: Artigo de periódico
Palavras-chave: Mapas temáticos; Geoestatística; Equação universal de perda de solo; Agricultura de Precisão; Precision agriculture; Thematic maps; Geostatistics; Universal Soil Loss Equation; Kriging.
Ano: 2022
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1145032

Análise exploratória de dados de monitoramento da dinâmica do gado em uma pastagem natural invadida pelo capim-annoni.
Provedor de dados: 119
Autores: NEVES, M. C.; PEREZ, N. B.; SISTI, R. N.
Abstract: The Precision Agriculture considers spatial variability in the agricultural parcel to increase the efficiency in production process. For this it is necessary to know the behavior of the relevant variables and develop viable strategies for action in system. The application of the Precision Agriculture principles in a livestock system involves a higher degree of difficulty due to the greater number of factors involved and the presence of animal component. Variables such as mobility, trampling, defecations of animals and preferential areas may impact the system and should be considered. The objective of this paper is to perform an exploratory analysis of data from monitoring of animals in an experimental plot of a livestock system, evaluating the...
Tipo: Separatas
Palavras-chave: Estimador de intensidade kernel; Monitoramento; Spacial data; Agricultura de precisão; Pecuária; Sensoriamento remoto; Gado de corte; Pastagem; Capim annoni; Precision agriculture; Remote sensing; Livestock.
Ano: 2015
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1020086

Sensoriamento remoto proximal na pesquisa agropecuária: passos iniciais.
Provedor de dados: 119
Autores: LUIZ, A. J. B.; NEVES, M. C.
Resumo: Após décadas de uso do sensoriamento remoto orbital na agricultura, a possibilidade de uso de imagens obtidas por Aeronaves Remotamente Pilotadas (RPA - Remotely Piloted Aircraft) está mudando o cenário de uso e aplicação das imagens nesse campo. A mudança de escala de trabalho e a limitação atual de bandas disponíveis exige uma nova base de conhecimento sobre aspectos fundamentais nessa área de pesquisa. Esse trabalho, desenvolvido em ambiente controlado, propõe um método não destrutivo (remoto) para estimar a Área Verde Digitalizada (AVD) do capim annoni (Eragrostis plana) e compara seus resultados com os de um aparelho tradicional de medição de área foliar de mesa (LI- 3100). A proposta se baseia no processamento de imagens compostas apenas...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Imagem digital.; Eragrostis plana; Capim annoni; Sensoriamento remoto; Agricultura de Precisão.; Remote sensing; Digital images; Precision agriculture.
Ano: 2019
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1116903

How digital is agriculture in South America? Adoption and limitations.
Provedor de dados: 119
Autores: PUNTEL, L. A.; BOLFE, E. L.; MELCHIORI, R. J. M.; ORTEGA, R.; TISCORNIA, G.; ROEL, A.; SCARAMUZZA, F.; BEST, S.; BERGER, A. G.; HANSEL, D. S. S.; PALACIOS, D. D.; BALBOA, G.
Abstract. A rapidly growing population in a context of land and water scarcity, and climate change has driven an increase in healthy, nutritious, and affordable food demand while maintaining the current cropping area. Digital agriculture (DA) can contribute solutions to meet the demands in an efficient and sustainable way. South America (SA) is one of the main grain and protein producers in the world but the status of DA in the region is unknown. Systematic review of official reports and surveys, literature, and case studies from Brazil, Argentina, Uruguay, and Chile was conducted to address the following objectives: i) quantify adoption of existing DA technologies, ii) identify limitations for DA adoption, iii) summarize existing metrics to benchmark DA...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Agricultura digital; Sustentabilidade; Adoção de tecnologias de agricultura digital; Internet das coisas; Digital agriculture; Sustainability; Adoption; Internet of things; IoT; Agricultura; Agricultura de Precisão; Agriculture; Precision agriculture.
Ano: 2022
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1144364

Computer vision and artificial intelligence in precision agriculture for grain crops: a systematic review.
Provedor de dados: 119
Autores: PATRICIO, D. I.; RIEDER, R.
Tipo: Artigo de periódico
Palavras-chave: Inteligência artificial; Agricultura de Precisão; Precision agriculture; Artificial intelligence; Computer vision.
Ano: 2018
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1099103

Tecnologias desenvolvidas em Agricultura de Precisão.
Provedor de dados: 119
Autores: GREGO, C. R.; SPERANZA, E. A.; RODRIGUES, G. C.; LUCHIARI JUNIOR, A.; VENDRUSCULO, L. G.; RODRIGUES, C. A. G.; INAMASU, R. Y.; VAZ, C. M. P.; RABELLO, L. M.; JORGE, L. A. de C.; ZOLIN, C. A.; FRANCHINI, J. C.; RONQUIM, C. C.
Introdução. Coleta, armazenamento e análise de dados em AP. Identificação da variabilidade espacial do solo. Amostragem de solo. Identificação da variabilidade espacial da cultura. Mapeamento da produtividade. Sensoriamento proximal. Sensoriamento suborbital e remoto. Armazenamento de dados em nuvem. Análise de Dados em AP. Mineração de dados e extração de padrões. Ferramentas de filtragem e limpeza de dados. Geoestatística e interpolação espacial. Delineamento de zonas de manejo. Experimentação onfarm, correlação espacial e recomendações. Aplicações práticas em Agricultura de Precisão. Caracterização da variabilidade espacial dos sistemas de produção de cafés especiais do sul de Minas Gerais. Comportamento espacial e espectral em cana-de-açúcar...
Tipo: Parte de livro
Palavras-chave: Agricultura; Agricultura de Precisão; Agriculture; Precision agriculture.
Ano: 2020
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1126469

Mapeamento preliminar de zonas de manejo em sistema de produção de milho-soja no Cerrado.
Provedor de dados: 119
Autores: VILELA, M. de F.; HURTADO, S. M. C.; RESENDE, A. V. de; CORAZZA, E. J.; MARCHAO, R. L.; OLIVEIRA, C. M. de; GOULART, A. M. C.
Tipo: Parte de livro
Palavras-chave: Fotografia aérea; Variabilidade espacial; Maize; Productivity.; Solo; Cerrado; Produtividade; Condutividade Eletrica.; Precision agriculture; Electrical conductivity; Soil; Soybeans.
Ano: 2011
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/907477

Variabilidade espacial da produtividade da soja e da condutividade elétrica de um Latossolo Bruno.
Provedor de dados: 119
Autores: OLIVEIRA, F. A. de; FRANCHINI, J. C.; DEBIASI, H.
A condutividade elétrica (CE) do solo tem sido utilizada como uma variável que se correlaciona com características do solo. No entanto existem poucas informações sobre sua relação com a produtividade das culturas. O efeito da variabilidade espacial da CE de um Latossolo Bruno sob sistema plantio direto sobre a produtividade da soja foi avaliado em uma área de 18,9 ha localizada em Guarapuava/PR. A CE foi determinada por meio do equipamento Veris 3100®, nas camadas de 0 a 0,3 m e 0 a 0,9 m de profundidade. A produtividade da soja foi determinada com uma colhedora autopropelida de grãos equipada com monitor de colheita. Os dados foram submetidos à análise geoestatística considerando 210 pontos amostrais distribuídos uniformemente pela área. A CE e a...
Tipo: Parte de livro
Palavras-chave: Geoestatística; Soja; Agricultura de precisão; Solo; Soybeans; Geostatistics; Precision agriculture.
Ano: 2011
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/908829

Efeito da variabilidade espacial de solos do Vale dos Vinhedos na composição do vinho Merlot - Safra 2012.
Provedor de dados: 119
Autores: MIELE, A.; FLORES, C. A.; FILIPPINI ALBA, J. M.
A importação de vinhos tem dificultado a comercialização de produtos nacionais. Para mitigar este efeito, é necessário aumentar a competitividade do vinho brasileiro, o que pode ser obtido pela redução de custos e melhoria da qualidade. A competitividade pode ser atingida, em parte, com a aplicação de tecnologias de agricultura de precisão. Com este objetivo, estudou-se o efeito de cinco unidades de mapeamento de solos do Vale dos Vinhedos, RS, na composição do vinho Merlot de 2012, avaliando-se 39 variáveis, cujos parâmetros foram submetidos à análise de componentes principais. Três componentes representaram 91,49% da variação total e discriminaram, principalmente, os vinhos elaborados com uvas de videiras cultivadas em Argissolo e Neossolo. Os principais...
Tipo: Parte de livro
Palavras-chave: Merlot; Agricultura de precisao; Viticultura; Manejo do solo; Precision agriculture; Viticulture; Soil management.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1004688

Sistema para monitoramento da movimentação bovina e aferição dos comportamentos.
Provedor de dados: 119
Autores: LOMBA, L. F. D.; JESUS, L. de; RUBINSZTEJN, H. K. S.; GONDA, L.; PIRES, P. P.
Tipo: Artigo de periódico
Palavras-chave: Pecuária de precisão; Comportamento bovino; Reconhecimento de padrão; Pattern recognition; Precision agriculture; Animal behavior.
Ano: 2017
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1083496

Dissimilarity of parameterized maps generated in geostatistics and the assumption of an automatic software model in precision agriculture.
Provedor de dados: 119
Autores: MALVEZI, K. E. D.; SIBALDELLI, R. N. R.; PEREIRA NETO, O. C.; MORAES, L. A. C.; SAAB, O. J. G. A.; MOREIRA, A.
Título em português: Dissimilaridade de mapas gerados na geoestatística parametrizada e seu pressuposto modelo automático de software na agricultura de precisão.
Tipo: Artigo de periódico
Palavras-chave: Química do Solo; Agricultura de Precisão; Precision agriculture; Soil chemical properties.
Ano: 2020
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1129740

Aplicação de nitrogênio a taxa variável em cultura de trigo: estudo de caso na Unidade Piloto de Agricultura de Precisão de Não-Me-Toque, RS.
Provedor de dados: 119
Autores: PIRES, J. L. F.; CORASSA, G. M.; RAMBO, A. C.; KERBER, L.; PASINATO, A.; DALMAGO, G. A.; SILVA JUNIOR, J. P. da; SANTI, A.; SANTI, A. L.; GUARIENTI, E. M.; CUNHA, G. R. da; STRIEDER, M. L.; FOCHESATTO, E.
O uso de sensores ópticos ativos como ferramenta para a definição da dose de nitrogênio a ser aplicada em cobertura na cultura do trigo é tecnologia disponível e em uso no Brasil. Com o objetivo de realizar o manejo sitio específico da adubação nitrogenada em cobertura na cultura do trigo utilizando-se sensor óptico ativo, foi realizado um estudo de caso na Unidade Piloto da Rede de AP em Não-Me-Toque, RS, na safra 2012. No momento da aplicação de nitrogênio em cobertura, a área foi dividida em dois talhões: um com aplicação a taxa fixa e outro a taxa variável. Foi utilizado equipamento comercial dotado de sensor óptico ativo para aplicação em taxa variável. A área foi monitorada antes e depois da aplicação de nitrogênio por meio de GreenSeeker®. Os...
Tipo: Parte de livro
Palavras-chave: NDVI; Taxa variável; Triticum aestivum L; Variable rate.; Precision agriculture; Wheat.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1006321

Preparação de ambiente colaborativo na internet para a rede de agricultura de precisão liderada pela Embrapa - estudo de caso com a ferramenta de blog WordPress.
Provedor de dados: 119
Autores: BERNARDES, R. M.; QUEIROS, L. R.; SPERANZA, E. A.
Durante a Convenção da Rede de Agricultura de Precisão realizada pela Embrapa em abril de 2010, um grupo de pesquisadores identificou a necessidade de continuar a discussão tendo como mote metadados geoespaciais e também ferramental para análises geoestatísticas, via internet por meio de algum ambiente colaborativo. Havia ainda a preocupação de que esse ambiente colaborativo estivesse em produção o mais rápido possível, de forma que as discussões iniciadas na Convenção não se perdessem com o passar do tempo. Para tanto, foi escolhida a ferramenta Blog com código aberto WordPress - uma vez que é de fácil instalação e configuração - como ambiente que permitisse fomentar as discussões dos pesquisadores. Os primeiros resultados já evidenciam a criação e...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Ambiente colaborativo; WordPress.; Agricultura de Precisão.; Precision agriculture.
Ano: 2010
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/873051

Panicum maximum cv. Tanzânia: climate trends and regional pasture production in Brazil.
Provedor de dados: 119
Autores: PEZZOPANE, J. R. M.; SANTOS, P. M.; EVANGELISTA, S. R. M.; BOSI, C.; CAVALCANTE, A. C. R.; BETTIOL, G. M.; GOMIDE, C. A. de M.; PELLEGRINO, G. Q.
Abstracts: Projected change in forage production under a range of climate scenarios is important for the evaluation of the impacts of global climate change on pasture-based livestock production systems in Brazil. We evaluated the effects of regional climate trends on Panicum maximum cv. Tanzânia production, predicted by agro-meteorological model considering the sum of degree days and corrected by a water availa bility index. Data from Brazilian weather stations (1963-2009) were considered as the current climate (baseline), and future scenarios, based on contrasting scenarios interms of increased temperature and atmospheric CO2 concentrations (high and low increases), were determined for 2013?2040 (2025 scenario) and for 2043-2070 (2055 scenario). Predicted...
Tipo: Artigo de periódico
Palavras-chave: ETA model; Global climate changes; Growing degree days; PRECIS model; Geoprocessamento; Feed crops; Geographical information systems; Agricultura de precisão; Planta forrageira; Balanço hídrico; Impacto ambiental; Sistema de Informação Geográfica; Precision agriculture; Environmental impact; Water balance; Brazil.
Ano: 2016
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1064731

Sistematização do índice de oportunidade na adoção da agricultura de precisão para diferentes sistemas produtivos.
Provedor de dados: 119
Autores: OLIVEIRA, R. P. de; BRANDAO, Z. N.; BERNARDI, A. C. de C.; PEREZ, N. B.; FRANCHINI, J. C.; BENITES, V. de M.; SANTI, A.; GEBLER, L.; BASSOI, L. H.; FILIPPINI ALBA, J. M.; SHIRATSUCHI, L. S.
RESUMO: A caracterização da variação espacial da produção é demanda na adoção da agricultura de precisão. Algumas abordagens buscam estabelecer métricas em apoio a uma gestão eficiente do manejo por sítio-específico. Entre as métricas parametrizadas segundo o ajuste do semi-variograma, o índice de oportunidade de adoção quantifica a variação espacial em função da viabilidade operacional das tecnologias disponíveis. Proposto com base em sistemas de produção de grãos australianos, o modelo foi aplicado no Brasil como ação transversal aos experimentos da Rede de Agricultura de Precisão da Embrapa. O principal objetivo foi avaliar o potencial de uso do índice aplicado a diferentes sistemas produtivos sob condições comuns de monitoramento no Brasil. Este...
Tipo: Separatas
Palavras-chave: Agricultura de precisão; Precision agriculture.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1002031

Uma ferramenta para cadastro e visualização de metadados em Agricultura de Precisão utilizando GeoNetwork.
Provedor de dados: 119
Autores: CORRÊA, P. E. B.; SPERANZA, E. A.; QUEIROS, L. R.
A Rede Agricultura de Precisão (RedeAP) consiste em um sistema que pode ser descrito como uma estratégia de gestão dos dados produzidos nas Unidades Piloto, e é fundamentalmente constituído de três componentes inter-relacionados entre si, sendo eles: Bancos de Dados, Política de Acesso e uso dos Dados, e Aplicação. O componente de Aplicação se trata de um Sistema de Informações Geográficas para a Web baseado no software livre i3Geo com o aplicativo de catalogação de dados geoespaciais GeoNetwork (QUEIROS et al., 2011). A adição de novos registros no catálogo do GeoNetwork pode ser feita utilizando o próprio editor de metadados ou pela ferramenta de importação dos dados no formato XML. Em ambos os casos, o usuário deve ser, no mínimo, registrado como editor...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Sistema de Informações Geográficas; Catalogação de metadados.; Agricultura de Precisão.; Precision agriculture; Geographic information systems.
Ano: 2011
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/921100

Uso de dados do Modelo Digital de Exploração Florestal - Modeflora para modelagem da distribuição potencial de Hura crepitans L. no leste do Acre.
Provedor de dados: 119
Autores: FIGUEIREDO, S. M. de M.; FIGUEIREDO, E. O.
Em razão da pouca disponibilidade de dados de ocorrência de espécies florestais na Amazônia e a necessidade de ampliar o conhecimento da sua distribuição geográfica potencial, foi realizado nesse trabalho a modelagem da distribuição potencial de Hura crepitans L. Os estudos foram desenvolvidos em áreas de planos de manejo florestal, licenciados pelo órgão ambiental estadual, com extensão de 26.187,37 hectares, localizadas nos municípios de Bujari, Capixaba, Senador Guiomard, Sena Madureira e Manuel Urbano, no estado do Acre.
Tipo: Parte de livro
Palavras-chave: Açacu; Sandboxtree; Árbol de habillo; Manejo florestal; Manejo de precisão; Geotécnica; Biometria florestal; Forest biometry; Biometría forestal; Modelagem 3D; Modeflora; Bujari (AC); Senador Guiomard (AC); Capixaba (AC); Amazonia Occidental; Sena Madureira (AC); Manuel Urbano (AC); Acre; Amazônia Ocidental; Western Amazon; Madera forestal; Agricultura de precisión; Inventario forestal; Manejo forestal; Sistemas de información geográfica; Sistemas de posicionamiento global; Teledetección.; Inventário florestal; Essência florestal; Biogeografia; Agricultura de precisão; Sistema de informação geográfica; Sensoriamento remoto.; Administração florestal; Biogeography; Hura crepitans; Geographic information systems; Global positioning systems; Remote sensing.; Precision agriculture; Tropical wood; Forest management; Forest inventory.
Ano: 2015
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1038757

Internet das Coisas.
Provedor de dados: 119
Autores: NARCISO, M. G.; BRONDANI, C.
Introdução. IoT aplicada ao melhoramento genético de precisão. Componentes mais comuns usados em IoT. Protocolo de comunicação LoRa. Exemplo de aplicação na agriculura. Considerações finais.
Tipo: Parte de livro
Palavras-chave: Componentes eletrônicos; Placa eletrônica; Dispositivos; Software embarcado; Obtenção de dados; Protocolo de comunicação; Tecnologia de comunicação; Rastreabilidade; Hardware; Agricultura digital; Melhoramento Genético Vegetal; Agricultura de Precisão; Sensoriamento Remoto; Tecnologia; Precision agriculture; Plant breeding; Remote sensing; Technology; Electronics; Computer software; Computer hardware.
Ano: 2023
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1156142

Nutrient use efficiency in agricultural systems: a brazilian perspective.
Provedor de dados: 119
Autores: BERNARDI, A. C. de C.
Most Brazilian soils are deep, highly weathered, acidic, and of low natural fertility. Many strategies have been developed for building soil fertility using lime and mineral fertilizers, particularly phosphorus (P), potassium (K), and micronutrients to attain higher yields. Brazil currently uses 8% of all the fertilizer produced in the world. The country is fourth among the largest consumers, behind only China, India and the United States. However, there is a big problem: national production is minimal. More than 85% of nutrient sources are imported to meet agricultural demand.
Tipo: Artigo de periódico
Palavras-chave: ILPF; Integrated systems; Enhanced efficiency fertilizers; Fertilizers; Precision agriculture; Soil analysis.
Ano: 2024
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1160855

Desenvolvimento de mosaico de imagens para automatização de processos na fruticultura de precisão.
Provedor de dados: 119
Autores: ANZOLIN, T. B. P.; PAULA FILHO, P. L.; GEBLER, L.; TONIN, P. C.
Abstract?The present work, in progress, aimed to detail the development of automation in the production of perennial fruit crops using image mosaic construction methods. The solution consists of using computer vision techniques based on the open source OpenCV library for image capture and processing, acting as a facilitator in the planning of planting, control and harvesting of apples in orchards with greater qualitative and quantitative performance. Keywords?Precision agriculture; image stitching; agricultural automation. Resumo? O presente trabalho, em andamento, teve por objetivo detalhar o desenvolvimento de automação na produção das culturas de frutas perenes usando métodos de construção de mosaico de imagens. A solução consiste na utilização de...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Fruticultura de precisão; Mosaico de imagens; Automação agrícola; Image stitching; Agricultural automation; Fruticultura; Precision agriculture.
Ano: 2021
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1135623

Banco de dados georeferenciado e sistema de apoio a decisão para a cultura do milho.
Provedor de dados: 119
Autores: NARCISO, M. G.; PEREIRA, D. F.; NÄÄS, I. A.; SOARES, A. F.
Com um banco de dados espaço-temporal, é possível integrar dados referentes a parâmetros físicos, químicos e biológicos do solo, referentes a uma dada cultura, possibilitando ao usuário (produtor) fazer consultas importantes ou simulações. Um sistema de apoio a decisão poderá fornecer para o usuário uma previsão da produtividade esperada para área, considerando o máximo de variáveis relevantes que atuam sobre a planta. Este trabalho tem como objetivo descrever e mostrar a importância de um banco de dados espaço-temporal para a disponibilização de dados sobre a cultura de Milho e o sistema de apoio à decisão Pró-Milho, conforme preceitos da Agricultura de Precisão.
Tipo: Anais e Proceedings de eventos
Palavras-chave: Banco de dados georeferenciado; Sistema de apoio à decisão; Agricultura de precisão; Precision agriculture; Decision support systems.
Ano: 2005
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/9112

Precision viticulture focusing southern Brazil.
Provedor de dados: 119
Autores: FILIPPINI ALBA, J. M.; CRIZEL, G. R.; GIRARDI, C. L.; FLORES, C. A.
There are four main wine regions in Rio Grande do Sul state, Brazil: (1) "Serra Gaúcha"; (2) São Francisco Valley; (3) "Serra do Sudeste" and (4) "Campos de Cima da Serra". The region (1) is the oldest wine region of Brazil, related to Italian immigration in nineteen century. Regions (2), (3) and (4) are newer, showing similarities but soft changes in climate and soil conditions. Precision viticulture (PV) has advanced in these poles in the last 20 years. Different techniques related to precision viticulture in the context of the precision agriculture (PA) network of Embrapa, including soil mapping, physical properties sensors, remote sensing, spectrorradiometry and miscellaneous methods. Results suggest a medium technological development of PA in Brazil,...
Tipo: Artigo de periódico
Palavras-chave: GIS; Mapping; Precision farming; Precision; Precision agriculture; Remote sensing; Soil; Wines.
Ano: 2022
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1150770

Análise das possibilidades e tendências do uso das tecnologias da informação e comunicação em Agricultura de Precisão.
Provedor de dados: 119
Autores: QUEIRÓS, L. R.; LUCHIARI JUNIOR, A.; CAMARGO NETO, J.; MASSRUHÁ, S. M. F. S.; INAMASU, R. Y.; SPERANZA, E. A.; EVANGELISTA, S. R. M.
Resumo: A Agricultura de Precisão (AP) tem em sua concepção a emergência de novas combinações agrotecnológicas baseadas no desenvolvimento e aplicação das tecnologias da informação e comunicação na agricultura. As Tecnologias da Informação e Comunicação (TIC?s) são definidas pela Agência dos Estados Unidos para Cooperação Internacional-USAID como sendo: a combinação de hardware, software e os instrumentos de produção que permitem troca, processamento e manejo da informação e do conhecimento. Então, de acordo com a USAID, as TIC's incluem tecnologias e métodos para armazenar, manejar e processar informação (e.g. computadores, softwares, livros, dispositivos móveis, livrarias digitais e não digitais) e para comunicar a informação (e.g. correio, correio...
Tipo: Parte de livro
Palavras-chave: Tecnologia da informação e comunicação; Computação em nuvem; Computação ubíqua; Sistemas de suporte à decisão; Protocolo de produção; Cloud computing; Agricultural production protocols; Agricultura de precisão; Tecnologia da informação; Precision agriculture; Information technology; Decision support systems.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1000966

Modelo de previsão da produtividade agrícola para auxílio à agricultura de precisão a partir da identificação de padrões freqüentes em base de dados espaço-temporal.
Provedor de dados: 119
Autores: VENDRÚSCULO, L. G.; OLIVEIRA, S. R. de M.
Esta proposta de pesquisa dispõe-se a investigar e propor novos e eficientes modelos de previsão de produtividade agrícola em auxílio à agricultura de precisão a partir de padrões frequentes de dados e consequentes Regras de Associação de dados Espaço-Temporal (RAET).
Tipo: Anais e Proceedings de eventos
Palavras-chave: Produtividade agrícola; Modelo de previsão; Base de dados espaço-temporal.; Agricultura de Precisão.; Precision agriculture; Models; Prediction; Databases.
Ano: 2010
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/876181

Tecnologias desenvolvidas em Agricultura de Precisão.
Provedor de dados: 119
Autores: GREGO, C. R.; SPERANZA, E. A.; RODRIGUES, G. C.; LUCHIARI JÚNIOR, A.; VENDRUSCULO, L. G.; RODRIGUES, C. A. G.; INAMASU, R. Y.; VAZ, C. M. P.; RABELLO, L. M.; JORGE, L. A. de C.; ZOLIN, C. A.; FRANCHINI, J. C.; RONQUIM, C. C.
Introdução. Coleta, armazenamento e análise de dados em AP. Identificação da variabilidade espacial do solo. Amostragem de solo. Identificação da variabilidade espacial da cultura. Mapeamento da produtividade. Sensoriamento proximal. Sensoriamento suborbital e remoto. Armazenamento de dados em nuvem. Análise de Dados em AP. Mineração de dados e extração de padrões. Ferramentas de filtragem e limpeza de dados. Geoestatística e interpolação espacial. Delineamento de zonas de manejo. Experimentação onfarm, correlação espacial e recomendações. Aplicações práticas em Agricultura de Precisão. Caracterização da variabilidade espacial dos sistemas de produção de cafés especiais do sul de Minas Gerais. Comportamento espacial e espectral em cana-de-açúcar...
Tipo: Parte de livro
Palavras-chave: Agricultura; Agricultura de Precisão; Agriculture; Precision agriculture.
Ano: 2020
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1126264

Delineamento de zonas de manejo em cana-de-açúcar a partir de atributos do solo e da cultura e imagens georreferenciadas.
Provedor de dados: 119
Autores: SPERANZA, E. A.; GREGO, C. R.; JORGE, L. A. de C.; RODRIGUES, C. A. G.; LUCHIARI JUNIOR, A.; RONQUIM, C. C.; SANCHES, G. M.
Resumo: Os mapas de zonas de manejo, obtidos a partir de diferentes atributos do solo e da cultura, podem ser utilizados em diferentes atividades realizadas no contexto da agricultura de precisão, tais como aplicação de fertilizantes e corretivos, irrigação e plantio. Este trabalho descreveu o delineamento de zonas de manejo para uma área experimental de cana-de-açúcar, a partir da utilização de dados de atributos do solo e da cultura obtidos por sensoriamento proximal e suborbital em conjunto com algoritmos de agrupamento de dados. Os resultados obtidos mostraram que zonas de manejo delineadas a partir desses atributos são capazes de auxiliar o produtor no tratamento de áreas espacialmente diferenciadas com relação à produtividade.
Tipo: Anais e Proceedings de eventos
Palavras-chave: Aeronave remotamente pilotada; Sensoriamento proximal; Agrupamento de dados; Produtividade da cultura; Drone; Condutividade elétrica aparente; Índice NDVI; Índice NDRE; Red-Edge NDVI; Agricultura de Precisão; Cana de Açúcar; Precision agriculture; Sugarcane; Normalized difference vegetation index.
Ano: 2019
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1118073

Agricultura de precisão em fruticultura.
Provedor de dados: 119
Autores: BASSOI, L. H.; MIELE, A.; REISSER JUNIOR, C.; GEBLER, L.; FLORES, C. A.; FILIPPINI ALBA, J. M.; GREGO, C. R.; TERRA, V. S. S.; TIMM, L. C.; NASCIMENTO, P. dos S.
Os sistemas de produção atualmente existentes na fruticultura brasileira caracterizam-se pela execução de diversas práticas agrícolas durante o ciclo da cultura, tendo como preocupação a quantidade e a qualidade da produção, e a rentabilidade da atividade agrícola. Nesse contexto, cria-se uma oportunidade para a aplicação de agricultura de precisão, como forma de auxiliar a gestão do sistema de produção e a tomada de decisão pelo produtor. Nesse capítulo, são apresentados quatro estudos de caso em que a realização de procedimentos e o uso de ferramentas, característicos de agricultura de precisão, permitem aos produtores e técnicos a compreensão da variabilidade de atributos do solo e da planta e de suas relações, bem como o estabelecimento de zonas...
Tipo: Parte de livro
Palavras-chave: Agricultura de precisao; Fruticultura; Viticultura; Estatística agrícola; Método estatístico; Precision agriculture; Fruit growing; Viticulture; Geostatistics; Agricultural statistics; Multivariate analysis.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1002018

SIG para a gestão vitivinícola no Vale dos Vinhedos, RS
Provedor de dados: 119
Autores: FILIPPINI ALBA, J. M.; FLORES, C. A.; MIELE, A.; VILLANI, L. M.
Processaram-se dados dos atributos físicos e químicos dos solos superficiais de três vinhedos localizados no Vale dos Vinhedos, Bento Gonçalves, RS, de acordo com procedimentos de viticultura de precisão, levantamento de solos e geotecnologias. A aplicação combinada de métodos estatísticos multivariados, geoestatística e SIG permitiu caracterizar três grupos principais de amostras onde os atributos edáficos se mantêm aproximadamente uniformes. A transformação da área ocupada por esses grupos em zonas de manejo dependerá da estratégia produtiva e de mercado da gestão vitícola. Considerando também trabalhos pretéritos, espera-se influenciar a qualidade da uva em cada zona, resultando em vinhos de características específicas com potencial para agregação de...
Tipo: Parte de livro
Palavras-chave: Agricultura de precisao; Sistema de informação; Manejo do solo; Analise estatistica; Precision agriculture; Geographic information systems; Geospatial science and technology; Soil management; Multivariate analysis.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1004692

Definição de zonas de manejo em cana-de-açúcar usando séries temporais de NDVI derivados do satélite Sentinel-2A.
Provedor de dados: 119
Autores: GREGO, C. R.; SPERANZA, E. A.; RODRIGUES, C. A. G.; NOGUEIRA, S. F.; SILVA, G. B. S. da; CIFERRI, R. R.; LUCHIARI JUNIOR, A.
RESUMO. O uso de imagens de satélite gratuitas e de média resolução temporal tem grande aplicação na agricultura de precisão. Este estudo avaliou a evolução de mapas de Índice de Vegetação por Diferença Normalizada (NDVI) obtidos de imagens orbitais do satélite Sentinel-2A, analisados quanto a variabilidade espacial, para auxiliar na identificação de diferentes zonas de manejo para a cana-de-açúcar. Para tanto, uma área de cana-de-açúcar, em Mogi Mirim ( SP), foi analisada durante os anos de 2016 e 2017 utilizando a geoestatística para o zoneamento. Imagens do satélite Sentinel-2A de seis datas foram obtidas e analisadas quanto à variabilidade espacial do NDVI. Houve dependência espacial dos índices de vegetação em todas as datas das imagens obtidas. Os...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Índice de Vegetação por Diferença Normalizada; Geoestatística; Imagem de satélite; Satellite image; Agricultura de Precisão; Cana de Açúcar; Saccharum Officinarum; Sugarcane; Geostatistics; Precision agriculture.
Ano: 2019
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1108752

Amostragem de solo para análises de fertilidade, de manejo e de contaminação.
Provedor de dados: 119
Autores: CHITOLINA, J. C.; PRATA, F.; SILVA, F. C. da; COELHO, A. M.; CASARINI, D. C. P.; MURAOKA, T.; VITTI, A. C.; BOARETTO, A. E.
Amostragem. Causas das variações no solo. Variação vertical. Plano de amostragem: separação das áreas uniformes. Tipos de amostra e parâmetros a serem medidos na amostra. Parâmetros químicos com maior e menor variação. Tamanho das glebas e número de amostras. Local, profundidade e frequência de amostragem. Culturas temporárias. Sistema de cultivo convencional. Sistema de plantio direto. Culturas perenes. Cultura da cana-de-açúcar. Pastagem. Agricultura de precisão. Identificação da variabilidade da fertilidade dos solos. Amostragem de solos. Custos de amostragem, análises de solo e elaboração de mapas. Amostragem de espécies químicas consideradas móveis. Amostragem de metais pesados em áreas contaminadas. Época de coleta das amostras. Equipamentos usados e...
Tipo: Parte de livro
Palavras-chave: Amostragem de solo; Análise de fertilidade; Análise de contaminação; Amostras de solo; Culturas temporárias; Sistema de cultivo convencional; Sistema de plantio direto; Culturas perenes; Análise de espécies químicas móveis; Análise de metais pesados; Agricultura de Precisão; Fertilidade; Pastagem; Solo; Cana de Açúcar; Agriculture; Precision agriculture; Sugarcane.
Ano: 2009
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/256789

Agricultura de precisão em fruticultura.
Provedor de dados: 119
Autores: BASSOI, L. H.; MIELE, A.; REISSER JUNIOR, C.; GEBLER, L.; FLORES, C. A.; FILIPPINI ALBA, J. M.; GREGO, C. R.; TERRA, V. S. S.; TIMM, L. C.; NASCIMENTO, P. dos S.
Os sistemas de produção atualmente existentes na fruticultura brasileira caracterizam-se pela execução de diversas práticas agrícolas durante o ciclo da cultura, tendo como preocupação a quantidade e a qualidade da produção, e a rentabilidade da atividade agrícola. Nesse contexto, cria-se uma oportunidade para a aplicação de agricultura de precisão, como forma de auxiliar a gestão do sistema de produção e a tomada de decisão pelo produtor. Nesse capítulo, são apresentados quatro estudos de caso em que a realização de procedimentos e o uso de ferramentas, característicos de agricultura de precisão, permitem aos produtores e técnicos a compreensão da variabilidade de atributos do solo e da planta e de suas relações, bem como o estabelecimento de zonas...
Tipo: Parte de livro
Palavras-chave: Agricultura de precisao; Fruticultura; Viticultura; Estatística agrícola; Método estatístico; Precision agriculture; Fruit growing; Viticulture; Geostatistics; Agricultural statistics; Multivariate analysis.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/986560

NDVI aplicado em imagens multiespectrais de cafeeiros sadios e cafeeiros infestados com bicho-mineiro.
Provedor de dados: 119
Autores: SANTOS, L. M. dos; FERRAZ, G. A. E. S.; MARIN, D. B.; CARVALHO, M. A. de F.; GUIMARÃES, R. J.; ALECRIM, A. de O.
O Bicho-mineiro (Leucoptera coffeella) é considerado uma praga primária do cafeeiro. O ataque desta praga causa redução da área fotossintética devido a necrose da folha lesionada, além da queda prematura das folhas, prejudicando a produtividade e a longevidade das plantas. Com isso, este trabalho teve como objetivo estudar os valores de Índice de Vegetação (IV) Normalized Difference Vegetation Index (NDVI) aplicado em imagens obtidas com câmera multiespectral de plantas sadias e plantas infestadas com bicho mineiro. Para o processamento das imagens, realizou-se operações aritméticas com as bandas espectrais, utilizando a ?Calculadora Raster?, baseado no uso do IV NDVI. Foram verificados que os valores de NDVI para plantadas infestadas foi próximo dos...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Índice de Vegetação; Agricultura de Precisão; Coffea Arábica; Bicho Mineiro; Praga de Planta; Precision agriculture; Vegetation index; Normalized difference vegetation index; Plant pests.
Ano: 2020
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1143370

Development of an Optoelectronic Sensor for Detecting and Classifying Fruit Fly (Diptera:,Tephritidae) for Use in Real-Time Intelligent Traps.
Provedor de dados: 119
Autores: MORAES, F. S.; NAVA, D. E.; SCHUNEMANN, T.; ROSA, V. S. da.
Tipo: Artigo de periódico
Palavras-chave: Fruit fly; Optoelectronic sensors; Classification of automated insects; Signal processing; Precision agriculture; Pest monitoring.
Ano: 2019
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1120595

Desenvolvimento de um algoritmo baseado em sensores ativos de dossel para recomendação da adubação nitrogenada em taxas variáveis.
Provedor de dados: 119
Autores: SHIRATSUCHI, L. S.; VILELA, M. F.; FERGUSON, R. B.; SHANAHAN, J. F.; ADAMCHUK, V. I.; RESENDE, A. V.; HURTADO, S. C.; CORAZZA, E. J.
Tipo: Parte de livro
Palavras-chave: Sensor óptico; Sensors.; Maize; Milho; Cerrado; Precision agriculture; Fertilizer application; Savanna soils.
Ano: 2011
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/907470

Using ensembles with spatial clustering approaches applied in the delineation of management classes in precision agriculture.
Provedor de dados: 119
Autores: SPERANZA, E. A.; CIFERRI, R. R.
This paper describes experiments performed using diff erent approaches for spatial data clustering, aiming to assist the delineation of management classes in Precision Agriculture (PA). These approaches were established from the partitional clustering algorithm Fuzzy c-Means (FCM), traditionally used in PA, and from the hierarchical clustering algorithm HACC-Spatial, especially designed for PA. We also performed experiments using diff erent clustering ensembles approaches, evaluating their behavior to achieve consensus solutions from individual clusterings obtained from attribute splitting or using exclusively FCM or HACC-Spatial. The achieved results exhibited some diff erences between FCM and HACC-Spatial, mainly for the visualization of management...
Tipo: Artigo de periódico
Palavras-chave: Classes de manejo; Agrupamento de dados espaciais; Ensembles; Cllusterização; Agricultura de Precisão; Precision agriculture; Spatial data; Cluster analysis.
Ano: 2017
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1099223

A review on the use of Unmanned Aerial Vehicles and imaging sensors for monitoring and assessing plant stresses.
Provedor de dados: 119
Autores: BARBEDO, J. G. A.
Abstract: Unmanned aerial vehicles (UAVs) are becoming a valuable tool to collect data in a variety of contexts. Their use in agriculture is particularly suitable, as those areas are often vast, making ground scouting difficult, and sparsely populated, which means that injury and privacy risks are not as important as in urban settings. Indeed, the use of UAVs for monitoring and assessing crops, orchards, and forests has been growing steadily during the last decade, especially for the management of stresses such as water, diseases, nutrition deficiencies, and pests. This article presents a critical overview of the main advancements on the subject, focusing on the strategies that have been used to extract the information contained in the images captured...
Tipo: Artigo de periódico
Palavras-chave: Imagem de sensor; Stress de planta; Drone; Crop; Orchard; Unmanned aerial systems; Agricultura de Precisão; Stress; Precision agriculture; Unmanned aerial vehicles.
Ano: 2019
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1108655

Caracterização espacial de indices de vegetação índice relativo de clorofila em áreas de produção cafés especiais no sul de Minas Gerais.
Provedor de dados: 119
Autores: RODRIGUES, G. C.; GREGO, C. R.; LUCHIARI JUNIOR, A.; SPERANZA, E. A.
RESUMO: A região sul do estado de Minas Gerais é grande produtora de café, principalmente daquele classificado como especial. Aspectos ambientais, entre outros fatores, interferem consideravelmente na produção desse tipo de café, envolvendo fatores como altitude e face de exposição do plantio ao sol. Este trabalho tem como objetivo avaliar a variabilidade espacial em áreas representativas de produção de café arábica (Coffea arabica) classificados como especiais do sul de Minas Gerais quanto aos índices vegetativos e de clorofila para identificar a existência de variabilidade espacial para aplicação da Agricultura de Precisão. Como resultado observou-se variabilidade espacial no NDVI, NDRE e IRC em todos os campos avaliados e trabalhos estão em andamento...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Geoestatística; Variabilidade espacial; Café arábica; Índice de vegetação; Índice relativo de clorofila; Índice de Vegetação da Diferença Normalizada pelo Red-Edge; Spatial variability; Agricultura de Precisão; Café; Coffea Arábica; Precision agriculture; Geostatistics; Vegetation index.
Ano: 2019
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1114194

AgroTIC em agricultura de precisão e automação agrícola.
Provedor de dados: 119
Autores: LUCHIARI JUNIOR, A.; QUEIRÓS, L. R.; CAMARGO NETO, J.; CHAIM, A.
O propósito central desse capítulo é o de diagnosticar e de analisar a situação atual, as tendências evolutivas e as possíveis mudanças das AgroTIC na pesquisa agrícola, na transferência de conhecimento e no desenvolvimento da agricultura brasileira relacionado à Agricultura de Precisão e Automação Agrícola.
Tipo: Parte de livro
Palavras-chave: Tecnologias da informação e comunicação; Agricultura de precisão; Information technology; Precision agriculture.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1010736

Avaliação geral, resultados e perspectivas do uso de agricultura de precisão em culturas anuais.
Provedor de dados: 119
Autores: RESENDE, A. V. de; VILELA, M. de F.
Tipo: Parte de livro
Palavras-chave: Cultura anual; Precision agriculture; Annuals.
Ano: 2011
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/907466

Ambientômica.
Provedor de dados: 119
Autores: GERMANO MARTINS FERREIRA; RESENDE, R. T.; FRITSCHE-NETO, R.; HEINEMANN, A. B.
Introdução. Termos da 'Ambientômica'. O Que é 'Ambiente'? Genética e diversidade ambiental. Ambientômica e as multi-interações genótipos × ambientes. Desenvolvimento de uma rotina de ambientômica. Exemplos de aplicação. Caracterização ambiental. Estudos das normas de reação. Recomendação de cultivares em ambientes de geoprocessamento. Perspectivas. Considerações finais.
Tipo: Parte de livro
Palavras-chave: Multiômicos; Dados ambientais; Ambientipagem; Fatores ambientais; Diversidade ambiental; Genótipos x ambientes; Melhoramento Vegetal; Agricultura de Precisão; Interação Genética; Condição Ambiental; População de Planta; Genética; Precision agriculture; Plant breeding; Gene interaction; Environmental factors; Genetics; Genotype-environment interaction.
Ano: 2023
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1156143

Technologies developed in precision agriculture.
Provedor de dados: 119
Autores: GREGO, C. R.; SPERANZA, E. A.; RODRIGUES, G. C.; LUCHIARI JÚNIOR, A.; VENDRUSCULO, L. G.; RODRIGUES, C. A. G.; INAMASU, R. Y.; VAZ, C. M. P.; RABELLO, L. M.; JORGE, L. A. de C.; ZOLIN, C. A.; FRANCHINI, J. C.; RONQUIM, C. C.
Introduction. Collecting, storing, and analyzing data in PA. Identification of soil spatial variability: Soil sampling; Electrical conductivity. Identification of crop spatial variability: Productivity mapping; Proximal sensing; Suborbital and remote sensing. Cloud data storage: Data analysis in PA: Data mining and pattern extraction; Filtering tools and data cleaning; Geostatistics and spatial interpolation; Outlining management zones; On-farm experiments, spatial correlation, and recommendations. Practical applications in precision agriculture: Characterization of the spatial variability in southern Minas Gerais specialty coffee production systems; Spatial and spectral behavior in sugarcane and its correlation to soil electrical conductivity; PA...
Tipo: Parte de livro
Palavras-chave: Agricultura; Agricultura de Precisão; Agriculture; Precision agriculture.
Ano: 2023
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1156817

Improvement of clay and sand quantification based on a novel approach with a focus on multispectral satellite images.
Provedor de dados: 119
Autores: FONGARO, C. T.; DEMATTÊ, J. A. M.; RIZZO, R.; SAFANELLI, J. L.; MENDES, W. de S.; DOTTO, A. C.; VICENTE, L. E.; FRANCESCHINI, M. H. D.; USTIN, S. L.
Abstract: Soil mapping demands large-scale surveys that are costly and time consuming. It is necessary to identify strategies with reduced costs to obtain detailed information for soil mapping. We aimed to compare multispectral satellite image and relief parameters for the quantification and mapping of clay and sand contents. The Temporal Synthetic Spectral (TESS) reflectance and Synthetic Soil Image (SYSI) approaches were used to identify and characterize texture spectral signatures at the image level. Soil samples were collected (0?20 cm depth, 919 points) from an area of 14,614 km 2 in Brazil for reference and model calibration. We compared different prediction approaches: (a) TESS and SYSI; (b) Relief-Derived Covariates (RDC); and (c) SYSI plus RDC....
Tipo: Artigo de periódico
Palavras-chave: Mapeamento do solo; Imagem de satélite; Sensoriamento Remoto; Satélite; Solo Arenoso; Solo Argiloso; Soil map; Remote sensing; Multispectral imagery; Satellites; Clay soils; Sandy soils; Reflectance spectroscopy; Precision agriculture; Soil degradation.
Ano: 2018
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1114592

Uso do conceito de Internet das Coisas para alertar o produtor sobre a presença de mosca-branca na lavoura.
Provedor de dados: 119
Autores: NARCISO, M. G.; SILVA, K.; LOBO JUNIOR, M.; MENDES, P. S.
Este trabalho descreve o desenvolvimento de uma armadilha automatizada, com ênfase no hardware, usando o conceito de Internet das Coisas (IoT), para detectar a mosca-branca no campo, de forma automatizada, para facilitar o monitoramento da lavoura quanto ao aparecimento desta praga e assim o produtor ou responsável poder tomar decisões sobre o combate desta praga. Uma armadilha comum tem que ser monitorada por uma pessoa, o pragueiro, o qual não tem tempo para monitorar a lavoura a qualquer momento, e sua frequência de avaliação das armadilhas pode ser semanal ou mensal, mas não diária. O sistema desenvolvido monitora a todo momento cada armadilha e envia um alerta ao produtor a qualquer momento.
Tipo: Artigo em anais e proceedings
Palavras-chave: Armadilha; Mosca Branca; Bemisia Tabaci; Agricultura de Precisão; Sensoriamento Remoto; Computer hardware; Computer software; Precision agriculture; Remote sensing; Technology.
Ano: 2023
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1159503

Remote sensing and kriging with external drift to improve sparse proximal soil sensing data and define management zones in precision agriculture.
Provedor de dados: 119
Autores: RODRIGUES, H. M.; CEDDIA, M. B.; VASQUES, G. M.; MULDER, V. L.; HEUVELINK, G. B. M.; OLIVEIRA, R. P. de; BRANDAO, Z. N.; MORAIS, J. P. S.; NEVES, M. L.; TAVARES, S. R. de L.
The precision agriculture scientific field employs increasingly innovative techniques to optimize inputs, maximize profitability, and reduce environmental impacts. Therefore, obtaining a high number of soil samples to make precision agriculture feasible is challenging. This data bottleneck has been overcome by identifying sub-regions based on data obtained through proximal soil sensing equipment. These data can be combined with freely available remote sensing data to create more accurate maps of soil properties. Furthermore, these maps can be optimally aggregated and interpreted for soil heterogeneity through management zones. Thus, this work aimed to create and combine soil management zones from proximal soil sensing and remote sensing data. To this end,...
Tipo: Artigo de periódico
Palavras-chave: Management zones; Proximal soil sensing; Geoestatística; Sensoriamento Remoto; Agricultura de Precisão; Remote sensing; Precision agriculture; Geostatistics.
Ano: 2023
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1159261

Vegetation indices applied to suborbital multispectral images of healthy coffee and coffee infested with coffee leaf miner.
Provedor de dados: 119
Autores: SANTOS, L. M. dos; FERRAZ, G. A. e S.; MARIN, D. B.; CARVALHO, M. A. de F.; DIAS, J. E. L.; ALECRIM, A. de O.; SILVA, M. de L. O. e.
The coffee leaf miner (Leucoptera coffeella) is a primary pest for coffee plants. The attack of this pest reduces the photosynthetic area of the leaves due to necrosis, causing premature leaf falling, decreasing the yield and the lifespan of the plant. Therefore, this study aims to analyze vegetation indices (VI) from images of healthy coffee leaves and those infested by coffee leaf miner, obtained using a multispectral camera, mainly to differentiate and detect infested areas. The study was conducted in two distinct locations: At a farm, where the camera was coupled to a remotely piloted aircraft (RPA) flying at a 3 m altitude from the soil surface; and the second location, in a greenhouse, where the images were obtained manually at a 0.5 m altitude from...
Tipo: Artigo de periódico
Palavras-chave: Agricultura digital; Agricultura de Precisão; Sensoriamento Remoto; Coffea Arábica; Precision agriculture; Remote sensing; Unmanned aerial vehicles.
Ano: 2022
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1143380

A servitização e sua influência no processo de difusão das tecnologias de agricultura de precisão na produção canavieira.
Provedor de dados: 119
Autores: CASAGRANDE, D. J.; TORKOMIAN, A. L. V.
Resumo: Para garantir o aumento da competitividade de seus negócios, as organizações redimensionam, de maneira contínua, mecanismos estratégicos orientados ao estreitamento das relações com seus clientes. Nesse contexto, a servitização surge como um modelo estratégico que visa disponibilizar soluções integradas de produtos e serviços ao mercado. No âmbito das cadeias produtivas agroindustriais, com ênfase para a canavicultura, a combinação de produtos e serviços vem contribuindo de forma expressiva para a expansão mercadológica em nível global. O objetivo deste trabalho foi analisar de que modo as estratégias de servitização podem contribuir para estimular a disseminação de tecnologias de agricultura de precisão (TAPs), no conjunto de atividades produtivas...
Tipo: Artigo de periódico
Palavras-chave: Servitização; Cana de Açúcar; Produto; Agricultura de Precisão; Tecnologia Agrícola; Cane sugar; Sugar products; Technology; Precision agriculture.
Ano: 2021
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1132618

Delineating management zones with different yield potentials in soybean-corn and soybean-cotton production systems.
Provedor de dados: 119
Autores: SPERANZA, E. A.; NAIME, J. de M.; VAZ, C. M. P.; FRANCHINI, J. C.; INAMASU, R. Y.; LOPES, I. de O. N.; QUEIROS, L. R.; RABELLO, L. M.; JORGE, L. A. de C.; CHAGAS, S. das; SCHELP, M. X.; VECCHI, L.
Abstract: The delineation of management zones is one of the ways to enable the spatially differentiated management of plots using precision agriculture tools. Over the years, the spatial variability of data collected from soil and plant sampling started to be replaced by data collected by proximal and orbital sensors. As a result, the variety and volume of data have increased considerably, making it necessary to use advanced computational tools, such as machine learning, for data analysis and decision-making support. This paper presents a methodology used to establish management zones (MZ) in precision agriculture by analyzing data obtained from soil sampling, proximal sensors and orbital sensors, in experiments carried out in four plots featuring...
Tipo: Artigo de periódico
Palavras-chave: Aprendizado de máquina; Variabilidade espacial; Machine learning; Spatial variability; Management Zones; Agricultura de Precisão; Soja; Milho; Algodão; Precision agriculture.
Ano: 2023
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1156255

Sistematização do índice de oportunidade na adoção da agricultura de precisão para diferentes sistemas produtivos.
Provedor de dados: 119
Autores: OLIVEIRA, R. P. de; BRANDAO, Z. N.; BERNARDI, A. C. de C.; PEREZ, N. B.; FRANCHINI, J. C.; BENITES, V. de M.; SANTI, A.; GEBLER, L.; BASSOI, L. H.; FILIPPINI ALBA, J. M.; SHIRATSUCHI, L. S.
A caracterização da variação espacial da produção é demanda na adoção da agricultura de precisão. Algumas abordagens buscam estabelecer métricas em apoio a uma gestão eficiente do manejo por sítio-específico. Entre as métricas parametrizadas segundo o ajuste do semi-variograma, o índice de oportunidade de adoção quantifica a variação espacial em função da viabilidade operacional das tecnologias disponíveis. Proposto com base em sistemas de produção de grãos australianos, o modelo foi aplicado no Brasil como ação transversal aos experimentos da Rede de Agricultura de Precisão da Embrapa. O principal objetivo foi avaliar o potencial de uso do índice aplicado a diferentes sistemas produtivos sob condições comuns de monitoramento no Brasil. Este trabalho...
Tipo: Parte de livro
Palavras-chave: Suporte a decisão; Índice de oportunidade; Variação espacial; Sítio-específico; Agricultura de precisão; Precision agriculture.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1004682

Management zones from proximal soil sensors capture within-field soil property and terrain variations.
Provedor de dados: 119
Autores: VASQUES, G. de M.; RODRIGUES, H. M.; OLIVEIRA, R. P. de; HERNANI, L. C.; TAVARES, S. R. de L.
The objectives are to delineate soil management zones from soil proximal sensor data, and compare soil property values among zones in a 72-ha crop field in southeastern Brazil. Apparent electrical conductivity (aEC) and magnetic susceptibility (aMS), and equivalent Th (eTh) and U (eU) were measured across the field by a Geonics EM38-MK2 and a Medusa MS1200 sensors, respectively. These properties were kriged and used as input for delineating three management zones by fuzzy k-means clustering. Soil properties were measured at 0-10 cm at 72 sites, and their means were compared among the zones. Soil clay, organic C and exchangeable Ca and Mg vary significantly among the zones, according to Brown-Forsythe and Games-Howell tests (p=0.05), while pH, available P...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Gamma radiometrics; Geophysics; Electrical conductivity; Precision agriculture; Geostatistics.
Ano: 2022
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1140033

Ajuste de grades amostrais para o mapeamento da resistência à penetração de um Latossolo Bruno.
Provedor de dados: 119
Autores: DEBIASI, H.; FRANCHINI, J. C.; OLIVEIRA, F. A. de; MACHADO, T. M.
O efeito da intensidade de amostragem na variabilidade espacial da resistência à penetração (RP) de um Latossolo Bruno sob sistema plantio direto foi avaliado em uma área de 18,9 ha localizada em Guarapuava/PR. A RP foi determinada em maio de 2011, por meio de um penetrômetro eletrônico, nas profundidades de 5, 10, 15, 20, 25 e 30 cm. Utilizou-se uma grade amostral de 30 × 30 m, totalizando 210 leituras de RP. Os dados foram submetidos à análise geoestatística, realizada para diferentes intensidades de amostragem, simuladas pela exclusão de pontos amostrais distribuídos uniformemente pela área. Considerando todos os 210 pontos amostrados, a RP apresentou dependência espacial em todas as profundidades avaliadas. Os modelos ajustados para os semivariogramas...
Tipo: Parte de livro
Palavras-chave: Geoestatística; Agricultura de precisão; Compactação do solo; Soil compaction; Precision agriculture; Geostatistics.
Ano: 2011
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/908820

Estudo de caso 8 - nitrogênio, regulador de crescimento e população de plantas em área de produção de algodão nas Fazendas Três Lagoas e Tucunaré, Sapezal, MT.
Provedor de dados: 119
Autores: VAZ, C. M. P.; FRANCHINI, J. C.; SPERANZA, E. A.; INAMASU, R. Y.; JORGE, L. A. de C.; RABELLO, L. M.; LOPES, I. de O. N.; CHAGAS, S. das; SCARIOTE, J. R. C.; SOUZA, M. de; GALBIERI, R.; PIRES JUNIOR, A.
Este trabalho apresenta estudos de caso da experimentação on-farm na cultura do algodão em talhões de produção comercial no Mato Grosso, com avaliação da resposta da produtividade para diferentes doses de nitrogênio em cobertura e diferentes populações de plantas (sementes por metro) em três áreas, e avaliação de regulador de crescimento em duas áreas.
Tipo: Parte de livro
Palavras-chave: Algodoeiro; Experimentação on-farm; Estudos on-farm; Algodão; Agricultura de Precisão; Argila; Nitrogênio; Precision agriculture.
Ano: 2022
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1151270

An impact analysis of pre-processing techniques in spectroscopy data to classify insect-damaged in soybean plants with machine and deep learning methods.
Provedor de dados: 119
Autores: OSCO, L. P.; FURUYA, D. E. G.; FURUYA, M. T. G.; CORRÊA, D. V.; GONÇALVEZ, W. N.; MARCATO JUNIOR, J.; BORGES, M.; MORAES, M. C. B.; MICHEREFF, M. F. F.; AQUINO, M. F. S.; LAUMANN, R. A.; LISENBERG, V.; RAMOS, A. P. M.; JORGE, L. A. de C.
Na publicação: Maria Carolina Blassioli-Moraes.
Tipo: Artigo de periódico
Palavras-chave: Field spectroscopy; Remote sensing; Precision agriculture; Artificial intelligence.
Ano: 2022
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1143293

O melhoramento na era de agricultura de precisão.
Provedor de dados: 119
Autores: RESENDE, R. T.; BRONDANI, C.; CHAVES, L. J.
Neste capítulo, vamos explorar a interseção entre o Melhoramento Genético de plantas e a Agricultura de Precisão, apresentando técnicas e conceitos fundamentais. Abordar a história do melhoramento genético de plantas, culminando na era atual. Faz uma analogia à Equação do Melhorista, relacionando-a com questões contemporâneas do Melhoramento de Precisão. Além disso, apresenta os resultados de uma pesquisa realizada com profissionais da área, investigando suas perspectivas em relação ao Melhoramento de Precisão. Demonstra como a combinação dessas abordagens está transformando a agricultura, impulsionando a sustentabilidade, produtividade e adaptabilidade das plantas cultivadas. O objetivo é auxiliar os melhoristas a otimizarem o processo de seleção,...
Tipo: Parte de livro
Palavras-chave: Inovação genética; Empreendedorismo; Melhoramento Genético Vegetal; Agricultura de Precisão; Historia; Seleção Genética; Variedade Resistente; Comportamento de Variedade; Inovação; Precision agriculture; History; Plant breeding; Plant genetics; Innovation adoption; Entrepreneurship.
Ano: 2023
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1156141

AgroTIC em agricultura de precisão e automação agrícola.
Provedor de dados: 119
Autores: LUCHIARI JUNIOR, A.; QUEIRÓS, L. R.; CAMARGO NETO, J.; CHAIM, A.
O propósito central desse capítulo é o de diagnosticar e de analisar a situação atual, as tendências evolutivas e as possíveis mudanças das AgroTIC na pesquisa agrícola, na transferência de conhecimento e no desenvolvimento da agricultura brasileira relacionado à Agricultura de Precisão e Automação Agrícola.
Tipo: Separatas
Palavras-chave: Tecnologias da informação e comunicação; Agricultura de precisão; Information technology; Precision agriculture.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1040539

Automação de máquinas e implementos agrícolas: eletrônica embarcada, robótica e sistema de gestão de informação.
Provedor de dados: 119
Autores: SOUSA, R. V. de; LOPES, W. C.; INAMASU, R. Y.
Sistemas embarcados. Eletrônica embarcada. Norma Iso11783 - Isobus. Modelo conceitual de integração de informação.
Tipo: Parte de livro
Palavras-chave: Automação de máquinas; Tecnologia da informação; Agricultura de precisão; Information technology; Precision agriculture.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1010739

Organização de dados georreferenciados: estudo de caso - rede de agricultura de precisão.
Provedor de dados: 119
Autores: SPERANZA, E. A.; QUEIROS, L. R.
A grande quantidade de fontes de dados geográficos que vêm surgindo nos últimos anos está gerando a necessidade de construção de modelos conceituais comuns para os Sistemas de Informações Geográficas, de forma a garantir a integração e interoperabilidade entre eles. O presente trabalho apresenta um modelo conceitual para organização de base de dados geográficas da Rede de Agricultura de Precisão idealizada pela Embrapa, utilizando-se de definições relacionadas à metadados e software livre para armazenamento e intercâmbio de dados na rede. Com essas características, vem sendo construída uma Unidade de Sistemas de Informação para a rede, que permitirá a entrada de dados geográficos, tanto em formato vetorial (shapefiles) como em forma de imagens de satélite,...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Dados georreferenciados; Sistemas de Informações Geográficas; Geographic information systems; Databases; Precision agriculture.
Ano: 2010
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/873024

Clorofilômetro no ajuste da adubação nitrogenada em cobertura para o milho de alta produtividade.
Provedor de dados: 119
Autores: HURTADO, S. M. C.; RESENDE, A. V. de; SILVA, C. A. da; CORAZZA, E. J.; SHIRATSUCHI, L. S.
A avaliação do conteúdo relativo de clorofila nas folhas fornece uma medida indireta do estado nutricional das plantas e pode ajudar os agricultores no ajuste da quantidade de nitrogênio (N) a ser aplicada em cobertura no milho. Objetivou-se neste trabalho validar o uso do clorofilômetro na detecção e correção da deficiência de N ao longo do ciclo vegetativo da cultura. O experimento foi conduzido em parcelas estabelecidas numa lavoura comercial, sendo o estado nutricional das plantas monitorado semanalmente com o uso do clorofilômetro. Os tratamentos incluíram uma testemunha (0kg ha-1) e quatro doses de N em cobertura (45, 90, 135 e 180kg ha-1), considerando-se o índice de suficiência de nitrogênio (ISN) de 0,95, o qual foi monitorado com o...
Tipo: Artigo de periódico
Palavras-chave: SPAD; Precision farming.; Nitrogênio; Zea mays; Nutrição vegetal; Agricultura de Precisão.; Precision agriculture; Nitrogen; Nitrogen fertilizers; Corn; Plant nutrition.
Ano: 2011
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/896435

Uso de sensor óptico ativo para caracterização do perfil de NDVI em dosséis de trigo submetidos a diferentes estratégias de manejo.
Provedor de dados: 119
Autores: PIRES, J. L. F.; CORASSA, G. M.; STRIEDER, M. L.; DALMAGO, G. A.; CUNHA, G. R. da; SANTI, A.; SILVA JUNIOR, J. P. da; SANTI, A. L.; SANTOS, H. P. dos; PASINATO, A.; REMOR, C.
Novas tecnologias associadas a sensores remotos têm sido usadas na cultura de trigo. Destaca-se a possibilidade de uso do monitoramento do cultivo em tempo real com indicadores que permitem estimar o vigor, potencial produtivo ou estado nutricional das plantas com base na reflectância do dossel. O uso de sensores ópticos ativos na pesquisa de trigo pode contribuir na caracterização de resposta de genótipos à práticas culturais, com posterior uso como suporte à tomada de decisão de manejo. Nesse sentido, em Passo Fundo, RS, na safra de inverno 2012, utilizou-se o sensor óptico ativo GreenSeeker® para avaliar linhagens de trigo passiveis de lançamento comercial pela Embrapa. Caracterizou-se os padrões de NDVI dos genótipos em ensaios de densidade de...
Tipo: Parte de livro
Palavras-chave: GreenSeeker; DNVI; Triticum aestivum L.; Agricultura de Precisão.; Precision agriculture; Wheat.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1006307

Aplicação do índice de cobertura verde em pastagem de azevém.
Provedor de dados: 119
Autores: NEVES, M. C.; LUIZ, A. J. B.; PEREZ, N. B.; DEIBLER, A.
Resumo: Existe uma crescente oferta de imagens de altíssima resolução espacial, sobretudo a oferecida por plataformas aéreas que operam a baixa altura do solo, como as aeronaves remotamente pilotadas. As características específicas desses dados demandam o desenvolvimento de novos métodos e abordagens. A proposta do Índice de Cobertura Verde visa obter uma medida quantitativa para monitoramento de culturas agrícolas a partir de câmaras fotográficas convencionais, sem a necessidade de uma banda no infravermelho próximo. Este método utiliza a transformação para o espaço de cores HSB (matiz, saturação e brilho) para obter uma relação de pixels com matiz verdes por unidade de área, para aplicação em monitoramento de culturas agrícolas. Neste trabalho,...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Espaço de cor HSB; Aeronaves remotamente pilotadas.; Cobertura vegetal; Azevém; Aerofotogrametria; Reconhecimento Aéreo; Agricultura de Precisão.; Precision agriculture; Aerial photography; Vegetation cover.
Ano: 2019
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1117289

Métodos e ferramentas de interpolação para geração de mapas georreferenciados para irrigação de precisão.
Provedor de dados: 119
Autores: SPERANZA, E. A.; TORRE-NETO, A.; RODRIGUES, E. L.; GREGO, C. R.
Este trabalho teve como objetivo desenvolver um aplicativo computacional capaz de gerar mapas georreferenciados úteis para a tomada de decisão em irrigação de precisão. Para tanto, foram utilizadas as bibliotecas TerraLib e SOMCode, ambas de código aberto e escritas na linguagem C++, desenvolvidas pelo Instituto Nacional de Pesquisas Espaciais (INPE) e pela Embrapa Tabuleiros Costeiros (CPATC), respectivamente. Os dados utilizados para a geração desses mapas foram obtidos por uma grade de sensores de uma unidade piloto da plataforma Irrigap, desenvolvida pela Embrapa Instrumentação Agropecuária (CNPDIA), dados esses referentes a medidas horárias de umidade e temperatura do solo e temperatura do ar. Diferentes métodos de interpolação foram utilizados, com o...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Irrigação de precisão; Mapas temáticos; Instrumentação agropecuária; Mapas georreferenciados; Aplicativo computacional.; Agricultura de Precisão.; Precision agriculture; Georeferencing; Thematic maps; Irrigation.
Ano: 2010
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/873048

Avaliação geral, resultados, perspectivas e uso de ferramentas de agricultura de precisão.
Provedor de dados: 119
Autores: NAIME, J. de M.; CAMARGO NETO, J.; VAZ, C. M. P.
Resumo: A agricultura de Precisão aplica o conceito da espacialização ou da análise da variabilidade espacial dos fatores que influenciam a produção agropecuária. Dessa forma, a AP é bastante dependente de instrumentos que auxiliam na aquisição, tratamento e transmissão dos dados nos campos agrícolas, transformando-os em informações úteis para o manejo sítio específico. Neste projeto componente estão sendo desenvolvidos e adaptados equipamentos, sensores, métodos, programas computacionais e uma plataforma de rede de sensores sem fio, denominadas de ferramentas de AP São apresentados resultados de equipamentos para a medida da matéria orgânica e umidade dos solos e de doenças de plantas; bancada de ensaios para a aplicação de insumos; esfera instrumentada...
Tipo: Parte de livro
Palavras-chave: Equipamentos on-the-go; Rede de sensores sem fio; Sistemas de informações geográficas.; Tecnologia da informação; Sensoriamento remoto; Agricultura de Precisão.; Precision agriculture; Wireless technology; Information technology; Remote sensing; Geographic information systems.
Ano: 2011
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/908527

Delineamento de zonas de manejo para o planejamento de experimentação on-farm na cultura do algodão.
Provedor de dados: 119
Autores: SPERANZA, E. A.; OLIM, G. E. de S.; INAMASU, R. Y.; VAZ, C. M. P.; JORGE, L. A. de C.
RESUMO: O Brasil é atualmente um dos maiores produtores e exportadores mundiais de algodão. O principal desafio dos produtores é a busca contínua do aumento da produtividade, aliado à qualidade do produto final, com foco no aumento da lucratividade e redução de impactos ao meio ambiente, tornando a produção de algodão no país cada vez mais sustentável. Desse modo, se torna cada vez mais necessária a adoção de técnicas de manejo que envolvam a coleta, análise e intervenção com base em dados, como a agricultura de precisão (AP). A subdivisão das áreas de produção em zonas de manejo (ZM) é uma das formas de se iniciar a adoção da AP em uma área de cultivo agrícola. Este trabalho teve como objetivo principal realizar o delineamento de ZM para uma área de...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Análise de Agrupamento; Imageamento Aéreo; Zonas de manejo; Clustering analysis; Aerial Imaging; Yield; Produtividade; Agricultura de Precisão; Precision agriculture.
Ano: 2022
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1148215

Computer vision and image processing for detecting and quantifying whiteflies: a systematic review.
Provedor de dados: 119
Autores: SILVA, J. G. J. da; NARCISO, M. G.; GONÇALVES, C.
A evolucão da agricultura de precisão impulsionou o aumento da produção agrícola e proporcionou o surgimento de grandes desafios em termos de eficiência, segurança alimentar, sustentabilidade e impacto ambiental. Especificamente, o controle de pragas é de suma importância no que tange a saúde das plantações. Este artigo apresenta uma revisão sistemática da literatura, abordando técnicas e métodos de processamento digital de imagens em plantas para a detecção e classificação de pragas, em específico para a praga Mosca Branca. Nesta revisão foram considerados artigos publicados entre 2008 e 2018 indexados por cinco bases de dados científicas. A revisão identificou que as técnicas são bem exploradas, diversificadas e possuem alto desempenho em termos de...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Classificação de imagens; Visão computacional; Agricultura de Precisão; Precision agriculture; Digital images; Computer vision.
Ano: 2019
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1111226

Viabilidade econômica do uso de agricultura de precisão em plantio direto.
Provedor de dados: 119
Autores: GOMIDE, R. L.
Tipo: Parte de livro
Palavras-chave: Viabilidade economica; No-till; Farming precision; Uso; Economic viability.; Agricultura de Precisão; Plantio Direto.; Precision agriculture; Tillage.
Ano: 2001
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/485176

Influência das diferentes faces de exposição ao sol nos índices vegetativos e relativo de clorofila em cafés especiais.
Provedor de dados: 119
Autores: SPERANZA, E. A.; GREGO, C. R.; RODRIGUES, G. C.; LUCHIARI JUNIOR, A.
RESUMO. A cafeicultura tem se destacado no Brasil nos últimos anos, atingindo altos níveis de exportação. Desse modo, a busca por tecnologias que permitam melhorar a produtividade e a qualidade do produto final é uma realidade. Nesse contexto, ferramentas de Agricultura de Precisão (AP) possuem papel estratégico, pois possibilitam ao produtor obter informações georreferenciadas com alta precisão de atributos referentes ao solo e à cultura que podem ser analisadas e transformadas em informações úteis para o manejo da produção. Neste artigo, foi realizado um processo de mineração de dados obtidos em campos experimentais de cafeicultura por meio de sensores proximais que permitem o cálculo de índices de vegetação e de clorofila presente nas plantas. Foram...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Mineração de dados; Sensoriamento Proximal; Zonas de Manejo; Coffee cultivation; Data mining; Proximal Sensing; Management Zones; Cafeicultura; Agricultura de Precisão; Precision agriculture.
Ano: 2019
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1125723

YOLO performance analysis for real-time detection of soybean pests.
Provedor de dados: 119
Autores: TETILA, E. C.; SILVEIRA, F. A. G. da; COSTA, A. B. da; AMORIM, W. P.; ASTOLFI, G.; PISTORI, H.; BARBEDO, J. G. A.
In this work, we evaluated the You Only Look Once (YOLO) architecture for real-time detection of soybean pests.
Tipo: Artigo de periódico
Palavras-chave: Aprendizado profundo; Detecção de objeto; Pragas da soja; Deep learning; Object detection; Soybean pests; Agricultura de Precisão; Glycine Max; Precision agriculture.
Ano: 2024
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1161634

Diagnosis about the perspectives of precision applications of coffee growing technologies in municipalities of Bahia, Brazil.
Provedor de dados: 119
Autores: FAGUNDES, R. B.; BOLFE, E. L.
ABSTRACT. Brazil is the largest coffee producer in the world and precision agriculture (PA) is essential for the efficient management of crops. However, one of the challenges is finding the best way to do it. In this sense, we sought to present in this article a diagnosis on the perspectives of Precision Agriculture technologies applicability in the production of coffee (or Precision Coffee Growing) in some municipalities in Bahia, for greater efficiency, economic and environmental sustainability. To achieve this objective, a virtual document was sent to coffee growers in the state of Bahia. The questionnaire was sent by email in 2021 and the WhatsApp application, reaching 457 producers, 34 of whom, from all productive regions of Bahia, responded. The rate...
Tipo: Artigo de periódico
Palavras-chave: Survey; Questionário; Agricultura de Precisão; Desenvolvimento Rural; Agronegócio; Café; Pesquisa; Precision agriculture; Agribusiness; Rural development; Surveys.
Ano: 2022
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1147793

SIG para a gestão vitivinícola no Vale dos Vinhedos, RS
Provedor de dados: 119
Autores: FILIPPINI ALBA, J. M.; FLORES, C. A.; MIELE, A.; VILLANI, L. M.
Processaram-se dados dos atributos físicos e químicos dos solos superficiais de três vinhedos localizados no Vale dos Vinhedos, Bento Gonçalves, RS, de acordo com procedimentos de viticultura de precisão, levantamento de solos e geotecnologias. A aplicação combinada de métodos estatísticos multivariados, geoestatística e SIG permitiu caracterizar três grupos principais de amostras onde os atributos edáficos se mantêm aproximadamente uniformes. A transformação da área ocupada por esses grupos em zonas de manejo dependerá da estratégia produtiva e de mercado da gestão vitícola. Considerando também trabalhos pretéritos, espera-se influenciar a qualidade da uva em cada zona, resultando em vinhos de características específicas com potencial para agregação de...
Tipo: Parte de livro
Palavras-chave: Agricultura de precisao; Sistema de informação; Manejo do solo; Analise estatistica; Precision agriculture; Geographic information systems; Geospatial science and technology; Soil management; Multivariate analysis.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/986577

Melhoramento de Precisão: aplicações e perspectivas na genética de plantas.
Provedor de dados: 119
O melhoramento na era de agricultura de precisão; Gestão otimizada dos programas; Empreendedorismo e inovação; Ciência de dados; Inteligência artificial; Pesquisa operacional; Internet das coisas; Ambientômica; Fenômica; Genômica; Speed breeding; Edição de genoma.
Tipo: Livros
Palavras-chave: Inteligência artifical; Agricultura de Precisão; Melhoramento Genético Vegetal; Automação; Biotecnologia; Precision agriculture; Plant genetic resources; Artificial intelligence; Agricultural biotechnology.
Ano: 2023
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1155985

Multispectral reflectance and geostatistic methods to estimate leaf nitrogen content and cotton yield.
Provedor de dados: 119
Autores: BRANDÃO, Z. N.; GREGO, C. R.; JORGE, L. A. de C.; MANJOLIN, R. C.
ABSTRACT: Satellite images and geostatistics are useful tools to assess the nutritional status of plants, and thus, understanding the variability of cotton yield in farmers´ fields, within the precision agriculture onfarm experiments. The objective of this study was the spatial identification of the NDVI index and spatial distribution of nitrogen contents and cotton yield through different phenological stages of the crop using geostatistical methods in Goiás state, Brazil. The experiment was carried out in a commercial field with 47.4 ha, in 80x80m georeferenced grid with 74 plots. Yield monitor data and multispectral satellite images at 56 m spatial resolution were collected in a rainfed cotton field in two dates to monitor the plant vigor, as well as...
Tipo: Parte de livro
Palavras-chave: Variabilidade espacial de nutrientes; Índice de vegetação da diferença normalizada; Análises geoestatísticas; Métodos geoestatísticos; Reflectancia multiespectral; Nitrogênio foliar; Algodoeiro; Nutrients spatial variability; Geostatistical analysis; Agricultura de Precisão; Algodão; Precision agriculture; Normalized difference vegetation index; Cotton.
Ano: 2022
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1145001

Correlation between vegetation indexes generated at Vitis Vinifera L. and soil, plant and production parameters for emergency application in decision making.
Provedor de dados: 119
Autores: SANTOS, M. da S.; GEBLER, L.; SEBEM, E.
Correlation between proximal sensing techniques and laboratory results of qualitative variables plus agronomic attributes was evaluated of a 3,0 ha vineyard in the county of Muitos Capões, Northeast of Rio Grande do Sul State, Brazil, in Vitis vinifera L. at 2017/2018 harvest, aiming to evaluate the replacement of conventional laboratory analysis in viticulture by Vegetation Indexes, at situations were laboratory access are unavailable. Based on bibliographic research, looking for vegetative indexes developed or used for canopy reflectance analysis on grapevines and whose working bands were within the spectral range provided by the equipment used, a total of 17 viable candidates were obtained. These chosen vegetation indices were correlated, through...
Tipo: Artigo de periódico
Palavras-chave: Vegetation indexes; Precision agriculture; Remote sensing.
Ano: 2022
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1137381

Improving coffee yield interpolation in the presence of outliers using multivariate geostatistics and satellite data.
Provedor de dados: 119
Autores: SILVA, C. de O. F.; GREGO, C. R.; MANZIONE, R. L.; OLIVEIRA, S. R. de M.
the objective of this study was to evaluate the use of remotely sensed data as auxiliary variables in the block cokriging (BCOK) modeling of coffee yield characterized by the presence of outliers.
Tipo: Artigo de periódico
Palavras-chave: Cokrigagem; Variograma; Agricultura digital; Dados de satélite; Geoestatística; Coffee yield; Cokriging; Variogram; Digital agriculture; Café; Coffea Arábica; Agricultura de Precisão; Sensoriamento Remoto; Precision agriculture; Remote sensing; Geostatistics.
Ano: 2024
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1161056

Tecnologias desenvolvidas em Agricultura de Precisão.
Provedor de dados: 119
Autores: GREGO, C. R.; SPERANZA, E. A.; RODRIGUES, G. C.; LUCHIARI JÚNIOR, A.; VENDRUSCULO, L. G.; RODRIGUES, C. A. G.; INAMASU, R. Y.; VAZ, C. M. P.; RABELLO, L. M.; JORGE, L. A. de C.; ZOLIN, C. A.; FRANCHINI, J. C.; RONQUIM, C. C.
Introdução. Coleta, armazenamento e análise de dados em AP. Identificação da variabilidade espacial do solo. Amostragem de solo. Identificação da variabilidade espacial da cultura. Mapeamento da produtividade. Sensoriamento proximal. Sensoriamento suborbital e remoto. Armazenamento de dados em nuvem. Análise de Dados em AP. Mineração de dados e extração de padrões. Ferramentas de filtragem e limpeza de dados. Geoestatística e interpolação espacial. Delineamento de zonas de manejo. Experimentação onfarm, correlação espacial e recomendações. Aplicações práticas em Agricultura de Precisão. Caracterização da variabilidade espacial dos sistemas de produção de cafés especiais do sul de Minas Gerais. Comportamento espacial e espectral em cana-de-açúcar...
Tipo: Parte de livro
Palavras-chave: Agricultura; Agricultura de Precisão; Agriculture; Precision agriculture.
Ano: 2020
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1126562

Análise de correspondência: uma ferramenta útil na interpretação de mapas de produtividade.
Provedor de dados: 119
Autores: CARVALHO, J. R. P. de; VIEIRA, S. R.; MORAN, R. C. C. P.
O objetivo do presente trabalho foi apresentar a Análise de Correspondência como um método estatístico multivariado que pode ajudar na interpretação de mapas de produtividade. Para tal, levantou-se a hipótese de a utilização de mapas de produtividade, para delimitar regiões homogêneas no campo, depender da estabilidade espacial e temporal desta variável, tornando-se preocupante seu uso indiscriminado como ferramenta de informação preditiva. Quatro mapas de produtividade foram usados neste trabalho, relativos a amostras coletadas de componentes de produção para arroz em 1994, milho em 1995, algodão em 1996 e milho em 1998, em uma malha com 110 pontos, espaçados de 10 x 10 m, da estação experimental do Instituto Agronômico de Campinas em Votuporanga (SP). Os...
Tipo: Artigo de periódico
Palavras-chave: Variabilidade espacial; Variabilidade temporal; Análise exploratória; Dados categorizados; Método estatístico multivariado; Agricultura de Precisão; Precision agriculture; Statistical analysis.
Ano: 2002
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/41

Agricultura de precisão em fruticultura.
Provedor de dados: 119
Autores: BASSOI, L. H.; MIELE, A.; REISSER JUNIOR, C.; GEBLER, L.; FLORES, C. A.; FILIPPINI ALBA, J. M.; GREGO, C. R.; TERRA, V. S. S.; TIMM, L. C.; NASCIMENTO, P. dos S.
Os sistemas de produção atualmente existentes na fruticultura brasileira caracterizam-se pela execução de diversas práticas agrícolas durante o ciclo da cultura, tendo como preocupação a quantidade e a qualidade da produção, e a rentabilidade da atividade agrícola. Nesse contexto, cria-se uma oportunidade para a aplicação de agricultura de precisão, como forma de auxiliar a gestão do sistema de produção e a tomada de decisão pelo produtor. Nesse capítulo, são apresentados quatro estudos de caso em que a realização de procedimentos e o uso de ferramentas, característicos de agricultura de precisão, permitem aos produtores e técnicos a compreensão da variabilidade de atributos do solo e da planta e de suas relações, bem como o estabelecimento de zonas...
Tipo: Parte de livro
Palavras-chave: Agricultura de precisao; Fruticultura; Viticultura; Estatística agrícola; Método estatístico; Precision agriculture; Fruit growing; Viticulture; Geostatistics; Agricultural statistics; Multivariate analysis.
Ano: 2014
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1004685

Uso de imagens de sensoriamento remoto para identificação de variabilidade espacial em Agricultura de Precisão.
Provedor de dados: 119
Autores: SPERANZA, E. A.; ANTUNES, J. F. G.; INAMASU, R. Y.
Resumo. A Agricultura de Precisão (AP) tem como principal objetivo aumentar o retorno econômico de uma lavoura, considerando o uso racional de insumos agrícolas a partir da identificação da variabilidade espacial dos atributos do solo e da cultura. Dentre esses atributos, aqueles que permitem a geração de mapas referentes a biomassa vegetal presente em alguns estágios de crescimento da lavoura, como o Índice de Vegetação por Diferença Normalizada (NDVI) que indica a presença e o vigor da vegetação, podem auxiliar de maneira significativa na identificação da variabilidade espacial da área de cultivo. Este trabalho descreve um experimento para verificação da correlação espacial entre imagens de sensoriamento remoto em diferentes resoluções espaciais, em uma...
Tipo: Anais e Proceedings de eventos
Palavras-chave: Biomassa vegetal; Correlação espacial; Resolução espacial; Vegetal biomass; Spatial correlation; Spatial resolution; Sensoriamento Remoto; Agricultura de Precisão; Remote sensing; Precision agriculture; Normalized difference vegetation index.
Ano: 2018
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1099230

Aplicando Mineração de Imagens na Agricultura de Precisão.
Provedor de dados: 119
Autores: RODRIGUES, D. DE C.; ROCHA, M. L.; TREVISAN, D. M. DE Q.; JORGE, L. A. de C.; FERREIRA, E. J.; OSCO, L. P.; BARBOSA, R. M.
RESUMO: Análise de imagens de plantações estão consolidados no mercado da agricultura de precisão. Nesse sentido, a utilização de técnicas de processamento de imagem, mineração de imagem e inteligência artificial são ferramentas fundamentais. Podendo aplicar essas técnicas de maneira individual ou em conjunto. Um problema comum em análises de imagens é que pequenas mudanças na iluminação e no momento de tirar fotos podem influenciar como as técnicas computacionais identificam seus elementos. O custo é muito alto ou mesmo inviável para identificar ou segmentar uma imagem de forma universal. Sendo assim, é necessário um ponto de partida solido para guiar as técnicas existentes. Este estudo apresenta um experimento utilizando técnicas de mineração de imagens,...
Tipo: Artigo de periódico
Palavras-chave: Mineração de Dados; Mineração de Imagem; Regras de Associação; Data Mining; Image Mining; Association Rules; Agricultura de Precisão; Precision agriculture.
Ano: 2021
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1138150

Delineation of irrigation management zones in a Quartzipsamment of the brazilian Semiarid region.
Provedor de dados: 119
Autores: OLDONI, H.; BASSOI, L. H.
The objective of this work was to delineate irrigation management zones using geostatistics and multivariate analysis in different combinations of physical and hydraulic soil properties, as well as to determine the optimal number of management zones in order to avoid overlaping. A field experiment was carried out in a Quartzipsamment, for two years, in an irrigated orchard of table grape, in the Senador Nilo Coelho Irrigation Scheme, in the municipality of Petrolina, in the state of Pernanbuco, Brazil. Soil samples were collected for the determination of soil physico-hydraulic properties. A portable meter was used to measure soil apparent electrical conductivity. Spatial distribution maps were generated using ordinary kriging. Management zones for five...
Tipo: Artigo de periódico
Palavras-chave: Fuzzy c-means; Irrigation planning; Soil apparent electrical conductivity; Spatial variability; Geoestatística; Planejamento da irrigação; Condutividade elétrica aparente do solo; Variabilidade espacial; Semiárido; Agricultura de precisão; Solo; Geostatistics; Precision agriculture.
Ano: 2016
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1061546

Biometric characteristics and canopy reflectance association for early-stage sugarcane.
Provedor de dados: 119
Autores: ROCHA, M. G. da; BARROS, F. M. M. de; OLIVEIRA, S. R. de M.; AMARAL, L. R. do.
ABSTRACT: Knowing the spatial variability of sugarcane biomass in the early stages of development may help growers in their management decision-making. Proximal canopy sensing is a promising technology that can identify this variability but is limited to quantifying plant-specific parameters. In this study, we evaluated whether biometric variables integrated with canopy reflectance data can assist in the generation of models for early-stage sugarcane biomass prediction. To substantiate this assertion, four sugarcane-producing fields were measured with an active crop canopy sensor and 30 sampling plots were selected for manually quantifying chlorophyll content, plant height, stalk number and aboveground biomass. We determined that Random Forest and Multiple...
Tipo: Artigo de periódico
Palavras-chave: Floresta aleatória; Índice de vegetação; Mineração de dados; Precision farming; Random forest; Vegetation indices; Data mining; Canopy sensor; Biomassa; Cana de Açúcar; Agricultura de Precisão; Biomass; Sugarcane; Precision agriculture; Vegetation index.
Ano: 2019
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/1110823

Agricultura de precisão para a sustentabilidade de sistemas produtivos do agronegócio brasileiro.
Provedor de dados: 119
Autores: INAMASU, R. Y.; BERNARDI, A. C. de C.; VAZ, C. M. P.; NAIME, J. de M.; QUEIROS, L. R.; RESENDE, A. V. de; VILELA, M. de F.; JORGE, L. A. de C.; BASSOI, L. H.; PEREZ, N. B.; FRAGALLE, E. P.
Tipo: Parte de livro
Palavras-chave: Sensoriamento remoto; Precision agriculture; Remote sensing.
Ano: 2011
URL: http://www.alice.cnptia.embrapa.br/alice/handle/doc/907451

Development of artificial sugarcane seed CP-54 from three cultivars (cv MEX 69-290; cv MEX 68-P-23; cv. CP 72-2086) using polymers in Tabasco, Mexico
Provedor de dados: 109
Autores: Álvarez-Sánchez,Geiner F; Arias-de la Cruz,Heidi L; Salgado-García,Sergio; Córdova-Sánchez,Samuel; Ortiz-Laurel,Hipólito; Castelán-Estrada,Mepivoseth; García-de la Cruz,Rubén; Castañeda-Ceja,Raúl.
Abstract Precision mechanized sowing of sugarcane has been delayed due to germination failures caused in sowing process by pieces of sugarcane, generating economic losses by reducing production. The aim of this study was to evaluate different polymers and cultivars of sugarcane to elaborate artificial seed CP-54, seed germination and quality of sugarcane plants. An experiment was carried out in two stages in experimental field of the Colegio de Postgraduados Campus Tabasco, Mexico. Results indicate that the best physical stage of artificial seed CP-54 was obtained in Mex 69-290, Mex 68-P-23 and CP 72-2086 cultivars encapsulated with starch polymers and sodium alginate. Artificial seed CP-54 germination was 100 and 84% encapsulated with starch and alginate...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Encapsulation; Precision agriculture; Saccharum spp.; Seed germination; Buds; Sugarcane response.
Ano: 2018
URL: http://www.scielo.org.co/scielo.php?script=sci_arttext&pid=S0120-28122018000100094

Weed-removal system based on artificial vision and movement planning by A* and RRT techniques
Provedor de dados: 1
Autores: Solaque Guzmán, Leonardo Enrique; Acevedo, Marianne Lorena Romero; Guevara, Adriana Riveros.
The recent exploration of autonomous robotics tasks in agro-industry has permitted the integration of theories of artificial vision and mobile robotics with tasks in precision agriculture. Artificial vision allows for the classification of weeds and crops from images of plantations. With 3D-image processing systems, the location of the weeds is determined, and then the movement of the tool responsible for eradication is proposed. This article presents the solution for finding weeds within a crop field using classifiers and the integration of a 3D-vision system that builds a point cloud featuring the plants to safeguard, the weeds and the free space using Zed technology. With this information, search techniques such as A* (A star) and RRT (Rapidly exploring...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mobile robotics; Precision agriculture; Weed recognition; Weed removal; Trajectory planning.
Ano: 2019
URL: http://periodicos.uem.br/ojs/index.php/ActaSciAgron/article/view/42687

Soil penetration resistance mapping quality: effect of the number of subsamples
Provedor de dados: 1
Autores: Pias, Osmar Henrique de Castro; Cherubin, Maurício Roberto; Basso, Claudir José; Santi, Antônio Luis; Molin, José Paulo; Bayer, Cimélio.
There is no consensus in the literature regarding how many subsamples are needed to perform accurate on-farm soil penetration resistance (SPR) mapping. Therefore, the objective of this study was to define the number of subsamples per sampling point needed to quantify the SPR. The experiment was performed in a 4.7 ha area and employed a 50 × 50 m grid system (18 sampling points). The SPR was evaluated using a digital penetrometer in two different years with 1, 2, 3, 4, 5, 6, 9, 12, and 15 subsamples per sampling point. The SPR maps produced with increasing numbers of subsamples were compared to the reference maps (15 subsamples) using the relative deviation coefficient and Pearson´s linear correlation. A reduction in the number of subsamples promoted an...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil compaction; Sampling protocol; Precision agriculture; Microvariability.; Soil compaction; Sampling protocol; Precision agriculture; Microvariability; Física do solo.
Ano: 2018
URL: http://periodicos.uem.br/ojs/index.php/ActaSciAgron/article/view/34989

Correlação linear e espacial entre a produtividade do feijoeiro e atributos físicos de um LATOSSOLO VERMELHO Distroférrico de Selvíria, Estado de Mato Grosso do Sul - DOI: 10.4025/actasciagron.v31i1.6641
Provedor de dados: 1
Autores: Martins, Mariana Ventura; UNESP; Carvalho, Morel de Passos e; UNESP; Andreotti, Marcelo; UNESP; Montanari, Rafael; UNESP.
Os atributos físicos do solo têm se mostrado de grade interesse para a agricultura contemporânea, uma vez que refletem decisivamente sobre a produtividade vegetal. Em 2006, no campus da Faculdade de Engenharia de Ilha Solteira, Unesp, analisou-se a produtividade do feijoeiro (PG) no sistema plantio direto irrigado, a resistência mecânica do solo à penetração (RP), a densidade do solo (DS) e as umidades gravimétrica (UG) e volumétrica (UV) em profundidade, num LATOSSOLO VERMELHO Distroférrico. O objetivo foi determinar as correlações lineares e espaciais, entre os atributos estudados, visando selecionar um indicador da qualidade física do solo de boa representatividade para a PG. Foi instalada a malha, para a coleta de dados contendo 135 pontos amostrais,...
Palavras-chave: 5.02.01.07-7 Solos Florestais manejo do solo; Qualidade física do solo; Plantio direto; Agricultura de precisão; Phaseolus vulgaris. soil management; Soil physical quality; No-tillage; Precision agriculture; Phaseolus vulgaris.
Ano: 2009
URL: http://periodicos.uem.br/ojs/index.php/ActaSciAgron/article/view/6641

A sampling plan and spatial distribution for site-specific control of Sphenophorus levis in sugarcane
Provedor de dados: 1
Autores: Pavlu, Franz Arthur; Molin, José Paulo.
Sphenophorus levis has become a major pest of sugarcane plantations in Brazil, causing significant losses in productivity. Few studies have been conducted on the spatial distribution of this pest in the field, which is essential for the development of sampling plans. We aimed to characterize the spatial distribution of S. levis in sugarcane, defining a reliable, practical and feasible sampling plan, as well as generating application maps for production areas, allowing for comparison of the consumption of inputs in a conventional system with site-specific application. The study was conducted in areas around Piracicaba, Brazil. First, we conducted sampling to evaluate the best sampling density to characterize the spatial dependence. The results showed that...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: 5.03.01.00-4 eostatistics; Site-specific application; Precision agriculture; Entomology; Soil pests; Sugarcane weevil Máquinas e Implementos Agrícolas.
Ano: 2016
URL: http://periodicos.uem.br/ojs/index.php/ActaSciAgron/article/view/28599

Espacialização de perdas e da qualidade do feijão em colheita semimecanizada - DOI: 10.4025/actasciagron.v32i2.3240
Provedor de dados: 1
Autores: Souza, Cristiano Márcio Alves de; Universidade Federal da Grande Dourados; Bottega, Eduardo Leonel; Universidade Federal de Viçosa; Vilela, Fábio Velloso; Universidade Federal da Grande Dourados; Rafull, Leidy Zulys Leyva; Universidade Federal da Grande Dourados; Queiroz, Daniel Marçal de; Universidade Federal de Viçosa.
O objetivo deste trabalho foi analisar o efeito da distribuição espacial do teor de água dos grãos e da produtividade do feijoeiro sobre as perdas e a qualidade do produto durante o processo de arranquio, recolhimento, trilha e separação em uma recolhedora-trilhadora. O trabalho foi realizado em uma área de 35 ha sob pivô central. Foi determinado o teor de água dos grãos no arranquio e no recolhimento, a produtividade total e líquida da lavoura, a velocidade de trabalho da máquina, a quantidade de grãos perdidos no arranquio, no recolhimento e na trilha e separação e a porcentagem de matéria estranha e própria do feijoeiro presente no produto. As perdas de grãos e a qualidade do produto colhido apresentaram elevada variação de seus valores na área,...
Palavras-chave: 5.01.03.02-4 grãos; Impurezas; Agricultura de precisão Mecanização Agrícola grain; Impurity; Precision agriculture.
Ano: 2010
URL: http://periodicos.uem.br/ojs/index.php/ActaSciAgron/article/view/3240

Soil penetration resistance mapping quality: effect of the number of subsamples
Provedor de dados: 1
Autores: Pias, Osmar Henrique de Castro; Cherubin, Maurício Roberto; Basso, Claudir José; Santi, Antônio Luis; Molin, José Paulo; Bayer, Cimélio.
There is no consensus in the literature regarding how many subsamples are needed to perform accurate on-farm soil penetration resistance (SPR) mapping. Therefore, the objective of this study was to define the number of subsamples per sampling point needed to quantify the SPR. The experiment was performed in a 4.7 ha area and employed a 50 × 50 m grid system (18 sampling points). The SPR was evaluated using a digital penetrometer in two different years with 1, 2, 3, 4, 5, 6, 9, 12, and 15 subsamples per sampling point. The SPR maps produced with increasing numbers of subsamples were compared to the reference maps (15 subsamples) using the relative deviation coefficient and Pearson´s linear correlation. A reduction in the number of subsamples promoted an...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil compaction; Sampling protocol; Precision agriculture; Microvariability. soil compaction; Sampling protocol; Precision agriculture; Microvariability Física do solo.
Ano: 2018
URL: http://periodicos.uem.br/ojs/index.php/ActaSciAgron/article/view/34989

Weed-removal system based on artificial vision and movement planning by A* and RRT techniques
Provedor de dados: 1
Autores: Solaque Guzmán, Leonardo Enrique; Acevedo, Marianne Lorena Romero; Guevara, Adriana Riveros.
The recent exploration of autonomous robotics tasks in agro-industry has permitted the integration of theories of artificial vision and mobile robotics with tasks in precision agriculture. Artificial vision allows for the classification of weeds and crops from images of plantations. With 3D-image processing systems, the location of the weeds is determined, and then the movement of the tool responsible for eradication is proposed. This article presents the solution for finding weeds within a crop field using classifiers and the integration of a 3D-vision system that builds a point cloud featuring the plants to safeguard, the weeds and the free space using Zed technology. With this information, search techniques such as A* (A star) and RRT (Rapidly exploring...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mobile robotics; Precision agriculture; Weed recognition; Weed removal; Trajectory planning.
Ano: 2019
URL: http://periodicos.uem.br/ojs/index.php/ActaSciAgron/article/view/42687

Environment simulator for studying automatic crop farming
Provedor de dados: 111
Autores: Oksanen, Timo; Hakojärvi, M.; Maksimow, T.; Aspiala, A.; Hautala, M.; Visala, A.; Ahokas, J.
Agricultural machines capable of utilizing variable rate application technology are tackling spatial variability in agricultural fields.  Agricultural field robots are the next step in technology, robots which are capable of utilizing sensor and actuating technologies without human contact and operate only areas of interest.  However, agricultural field robots are still under research.  Robots are just one part of the next generation of crop farming having more advanced tools to do the work which currently requires humans.  The next generation of crop farming, in the vision of the authors, is based on automation, which incorporates stationary and moving sensors systems, robots, model based decision making, automated operation planning which adapts to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Robots; Crop growth models; Soil water models; Precision agriculture; Environment simulation; Decision making; Operation planning.
Ano: 2014
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/2604

Solutions for fast development of precision agriculture in Iran
Provedor de dados: 111
Autores: Bagheri, Nikrooz -; Bordbar, Marzieh.
A descriptive survey method was carried out to assess to effective factors on precision agriculture (PA) adoption and to find out practical solutions for development of PA in Iran.  The research population included 450 people from agricultural specialists, experts, researchers.  A sample of 117 was constituted using proportional stratified sampling based on the Cochran formula.  Data were collected using questionnaire.  The questionnaire was validated by a panel of experts, and the reliability index was established by a Cronbach's coefficient.  Computed Cronbach’s alpha score obtained 81%.  All survey data were analyzed using the Statistical Package for Social Sciences (SPSS 16.0).  The most important solutions for development of PA in Iran were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural extension; Precision agriculture; Agricultural management adoption; Factor analysis; Precision agriculture; Solution.
Ano: 2014
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/2716

Performance evaluation of a variable rate sprayer by artificial neural network models
Provedor de dados: 111
Autores: Bagheri, Nikrooz -.
To evaluate the performance of a variable rate boom sprayer, an artificial neural network (ANN) was employed. To model output flow of nozzles, 727 nets by four neural net models, namely, linear, MLP, RBF and GRNN were tested. For each nozzle, 45, 22 and 23 experimental data were used for train, verification and test, respectively. The results indicated that RBF model was selected as the best by regression ratio of 0.198 and R2 of 0.98. To investigate the capability of RBF model in prediction of nozzles flow, statistical analysis was used. Based on the results, average value of R2 for statistical and RBF models were 0.98 and 0.99, respectively. So, the average value of CV for RBF and statistical models were 18.96% and 19.05%, respectively. From the results,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Mechanics of agricultural engineering ANN; Control system; Precision agriculture; Sprayer; VRA.
Ano: 2014
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/2861

Last generation instrument for agriculture multispectral data collection
Provedor de dados: 111
Autores: Marinello, Francesco.
In recent years, the acquisition and analysis of multispectral data are gaining a growing interest and importance in agriculture.  On the other hand, new technologies are opening up for the possibility of developing and implementing sensors with relatively small size and featuring high technical performances.  Thanks to low weights and high signal to noise ratios, such sensors can be transported by different types of means (terrestrial as well as aerial vehicles), giving new opportunities for assessment and monitoring of several crops at different growing stages or health conditions.  The choice and specialization of individual bands, within the electromagnetic spectrum ranging from the ultraviolet to the infrared, plays a fundamental role in the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Sensors wavelengths  vegetation indices  multiband imaging  synchronized  measurement.
Ano: 2017
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/3939

Spatial variability of microbial biomass and organic matter labile pools in a haplic planosol soil
Provedor de dados: 53
Autores: Loureiro,Diego Campana; De-Polli,Helvécio; Ceddia,Marcos Bacis; Aquino,Adriana Maria de.
The objective of this work was to study the spatial variability of soil microbial biomass (SMB) and labile soil organic matter pools (labile SOM), under different management systems and plant cover. The experiment was conducted in a Haplic Planosol soil on an Integrated Agroecological Production System (SIPA), in Seropédica, Rio de Janeiro. The evaluated management systems were: alley cropping, pasture, and bush garden, the late one was used as reference area. Three grids of regular spacing of 2.5 x 2.5 meters were used for sampling, consisting of 25 georeferenced points each, where soil samples were taken at 0-10 cm depth. The following labile constituents of soil organic matter were determined: free light fraction (FLF), water soluble C and N, C and N of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Organic carbon; Geoestatistic; Glomalin; Precision agriculture.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0006-87052010000500010

Non-invasive spectral detection of the beneficial effects of Bradyrhizobium spp. and plant growth-promoting rhizobacteria under different levels of nitrogen application on the biomass, nitrogen status, and yield of peanut cultivars
Provedor de dados: 53
Autores: Elsayed,Salah; Elhoweity,Mohamed; El-Hendawy,Salah; Schmidhalter,Urs.
ABSTRACT High-throughput phenotyping using spectral reflectance measurements offers the potential to provide more information for making better-informed management decisions at the crop canopy level in real time. The aim of this study was to investigate the suitability of hyperspectral reflectance measurements of the crop canopy for the assessment of biomass, nitrogen concentration, nitrogen uptake, relative chlorophyll contents, and yield in 2 peanut cultivars, Giza 5 and Giza 6. Peanuts were grown under field conditions and subjected to 3 doses of nitrogen fertilizer with or without the application of 2 bio-fertilizers, Bradyrhizobium spp. or plant growth-promoting rhizobacteria. Simple linear regression of normalized difference spectral indices and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biofertilizer; Phenomics; Phenotyping; Precision agriculture; Spectral reflectance.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0006-87052017000200189

Sampling grids for monitoring Euschistus heros infestation in soybean
Provedor de dados: 53
Autores: Pias,Osmar Henrique de Castro; Cherubin,Maurício Roberto; Berghetti,Juliano; Kuss,Cassiano Carlos; Santi,Antônio Luis; Basso,Claudir José.
ABSTRACT Euschistus heros is one the most important pest insect in soybean fields in Brazil. Therefore, site-specific management applied for controlling E. heros can result in economic and environmental benefits. However, sampling protocols for assessing spatialtemporal variability of this soybean pest and, then, for guiding a more sustainable pest management, were still unknown. Thus, the objective of this study was to compare the efficiency of sampling grid sizes for monitoring the spatial variability of E. heros infestation along the soybean reproductive stages. Nine sampling campaigns were carried out using the beating sheet method, from R2 to R7 soybean phenological stages. It was used a sampling grid of 10 × 10 m, totaling 338 points in an soybean...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Neotropical brown stink bug; Pest sampling protocol; Spatio-temporal variability; Precision agriculture.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0006-87052017000300386

Hyperspectral remote sensing to assess the water status, biomass, and yield of maize cultivars under salinity and water stress
Provedor de dados: 53
Autores: Elsayed,Salah; Darwish,Waleed.
ABSTRACT Spectral remote sensing offers the potential to provide more information for making better-informed management decisions at the crop canopy level in real time. In contrast, the traditional methods for irrigation management are generally time-consuming, and numerous observations are required to characterize them. The aim of this study was to investigate the suitability of hyperspectral reflectance measurements of remote sensing technique for salinity and water stress condition. For this, the spectral indices of 5 maize cultivars were tested to assess canopy water content (CWC), canopy water mass (CWM), biomass fresh weight (BFW), biomass dry weight (BDW), cob yield (CY), and grain yield (GY) under full irrigation, full irrigation with salinity...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Precision agriculture; Precision phenotyping; Spectral indices.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0006-87052017000100062

Quantifying Nitrate Leaching in Irrigated Wheat with Different Nitrogen Fertilization Strategies in an Alfisol
Provedor de dados: 117
Autores: Claret M,Marcelino; Urrutia P,Roberto; Ortega B,Rodrigo; Best S,Stanley; Valderrama V,Natalia.
Consumption of water contaminated with nitrates is associated with important health effects such as methemoglobinemia and gastric cancer. Intensive agriculture, which uses large quantities of N fertilizer, is the main source of nitrates in water systems. There are several strategies to reduce leaching and increase Nitrogen Use Efficiency (NUE). An experiment was conducted with spring wheat (Triticum aestivum L.) under sprinkler irrigation (center pivot) to determine if adjusted N applications using precision agriculture tools and plant demand resulted in a lower groundwater nitrate load. Evaluated treatments were: produced fertilization (Pr), precision agriculture (Pa), chlorophyll meter (Sm), and control without N (W/N). The ceramic capsule methodology...
Tipo: Journal article
Palavras-chave: Nitrates; Precision agriculture; Chlorophyll meter; Wheat.
Ano: 2011
URL: http://www.scielo.cl/scielo.php?script=sci_arttext&pid=S0718-58392011000100018

Effect of Agricultural Intervention on the Spatial Variability of some Soils Chemical Properties in the Eastern Plains of Colombia
Provedor de dados: 117
Autores: Camacho-Tamayo,Jesús H; Luengas,Carlos A; Leiva,Fabio R.
Growing demand for food exerts pressure on natural resources and may lead to the expansion of agricultural frontiers in developing countries. Most of this pressure appears in tropical zones, in native savannahs, with naturally infertile soils prone to degradation. Crop management in these regions is based on generalized estimates, leaving aside the inherent soil variability, leading to low production efficiency and high risk of environmental damage. This study aims at determining the spatial variability of some chemical properties, including organic carbon, pH, exchangeable acidity, exchangeable aluminum, P, Ca, Mg, K and Na for two Oxisols with different levels of agricultural intervention, in Puerto Lopez, Colombia, in order to identify guidelines for...
Tipo: Journal article
Palavras-chave: Geostatistics; Kriging; Soil management; Precision agriculture; Kriging.
Ano: 2008
URL: http://www.scielo.cl/scielo.php?script=sci_arttext&pid=S0718-58392008000100005

Spatial variability of soil acidity attributes and the spatialization of liming requirement for corn
Provedor de dados: 64
Autores: Hurtado,Sandro Manuel Carmelino; Silva,Carlos Alberto; Resende,Álvaro Vilela de; Von Pinho,Renzo Garcia; Inácio,Euzelina dos Santos Borges; Higashikawa,Fábio Satoshi.
In Brazil, technicians, in most cases, ignore the aspects related to the spatial variability of the soil acidity attributes when liming requirement is calculated. The objective of this study was to validate the liming practice, evaluating the presence of spatial variability of the soil acidity attributes and the existence of areas with differentiated liming requirement, which were calculated by different methods. The experiment was carried out in an area cultivated with corn under conventional management and irrigation. The soil (0-0.2 m) was sampled in a conventional way (composite soil sample) and in a systematic scheme, by use of a grid sampling. In sequence to the soil fertility attributes analysis, it was calculated the liming requirement, according...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Geostatistics; Zea mays (L); Liming application zones.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1413-70542009000500022

Multispectral aerial images for the evaluation of maize crops
Provedor de dados: 64
Autores: Hoss,Douglas Felipe; Luz,Gean Lopes da; Lajús,Cristiano Reschke; Moretto,Marcos Antônio; Tremea,Geraldo Antonio.
ABSTRACT The combination of multispectral aerial images and computational processing is emerging as one of the solutions used in precision agriculture to observe the nutritional status of plants. The objective of this study is therefore to associate the nitrogen content and dry weight of the aerial part of maize plants (DW) with the vegetation indices obtained by multispectral aerial images (NDVIA and NDREA), and with the SPAD index and the Greenseeker NDVI, in the vegetative stage V6. To this end, randomized blocks in a factorial scheme of 6x4 (six nitrogen doses at the base and four different flight altitudes) were used, with three replications. The collected data was submitted to ANOVA with the F test (p = 0,05) and subsequent regression analysis. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays; Precision agriculture; Nitrogen; Computational processing.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1413-70542020000100216

Optimization of sample design sizes and shapes for regionalized variables using simulated annealing
Provedor de dados: 118
Autores: Guedes,Luciana P.C; Uribe-Opazo,Miguel A; Ribeiro Junior,Paulo J.
The spatial variability of structures in regionalized variables are defined with the aid of geostatistical techniques, which facilitate the estimation of values for these variables in unsampled localizations and generate thematic maps to be used in decision making for localized treatments in the area under study. The quality of these maps depends on the trustworthiness of these estimates that can be modified with the choice for the sample design. The objective of this work was to establish an optimal size and shape of the sample designs in order to enhance the efficiency of sampling plans for the prediction of space dependent variables. These designs were obtained with the use of a stochastic search method called Simulated Annealing. This method is based...
Tipo: Journal article
Palavras-chave: Geostatistics; Interpolation; Precision agriculture; Spatial variability.
Ano: 2014
URL: http://www.scielo.cl/scielo.php?script=sci_arttext&pid=S0718-16202014000100004

Profit maps for precisión agriculture
Provedor de dados: 118
Autores: Bazzi,Claudio L; Souza,Eduardo G; Khosla,Raj; Uribe-Opazo,Miguel A; Schenatto,Kelyn.
During the last few years, yield maps have become economically feasible for farmers due to technological advances in precision agriculture. However, evidence of yield profitability is still uncertain, and variability in yield has seldom been correlated to variability in profits. Differently from yield maps, profit maps can supply additional information about the economic return for each particular area of a field. The objective of the present work was to study how management decisions can be facilitated by transforming yield-map datasets into profit maps and the importance of the selection of interpolator type. Yield and profit maps were generated for each data set (three soybean fields and one corn field) using the inverse of the distance (ID), the...
Tipo: Journal article
Palavras-chave: Precision agriculture; Profit map; Profitability map.
Ano: 2015
URL: http://www.scielo.cl/scielo.php?script=sci_arttext&pid=S0718-16202015000300007

Effects of storage on vis-NIR-SWIR reflectance spectra of Mombasa grass leaf samples
Provedor de dados: 65
Autores: Tavares,Tiago Rodrigues; Fiorio,Peterson Ricardo; Seixas,Hugo Tameirão; Garcia,Amparo Cisneiros; Barros,Pedro Paulo da Silva.
ABSTRACT: Vis-NIR-SWIR reflectance spectra of leaf samples, collected in the laboratory, allow the calibration of predictive models to quantify their physicochemical attributes in a practical manner and without producing chemical residues. This technique should enable the development of management strategies for intensification of pasture use. However, spectral analysis performed in the laboratory may be affected by the deterioration of plant material during transport from the field to the lab, so storage methods are necessary. This research aimed to evaluate the effects of different storage methods on the spectral response of Mombasa grass leaves. Three methods were evaluated: (i) artificially refrigerated environment, (ii) humid environment, and (iii)...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Diffuse reflectance spectroscopy; Hyperspectral sensors; Forage; Precision agriculture.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782020000300401

Productivity of soybean in management zones with application of different sowing densities
Provedor de dados: 65
Autores: Camicia,Rafaela Greici da Motta; Maggi,Marcio Furlan; Souza,Eduardo Godoy de; Bazzi,Claudio Leones; Konopatzki,Evandro André; Michelon,Gabriela Karoline; Pinheiro,José Bruno Santos.
ABSTRACT:  The present study aimed to assess the efficiency of sowing at variable rates for soybean cultivation in two management zones (MZs) which were defined based on stable attributes and correlated with productivity using the Fuzzy C-means clustering algorithm and the kriging interpolation.Seeding was carried out in the 2015/2016 and 2017/2018 crops with a variation of 20% of seeds and crop row spacing of 0.70m. In each MZ, 8 plots with higher and lower seed density were established. Productivity was measured using a harvest monitor connected to a harvester. Data were filtered and submitted to descriptive analysis. Productivity maps were generated using the inverse square distance interpolation for each seeding density. In the MZ with the highest...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Grain production; Management zones.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782018001200201

Diagnosis de nitrógeno en chile de agua identificada por reflectancia.
Provedor de dados: 32
Autores: San Juan Martínez, Erwin.
El diagnóstico oportuno del estado nutrimental de los cultivos en la agricultura de precisión es de suma importancia y vitalidad; por lo que cada vez se hacen más necesarias técnicas que permitan conocer el estado nutrimental del cultivo de forma rápida, precisa y confiable. Es por ello que el presente trabajo tuvo como objetivo determinar la concentración de nitrógeno foliar en chile de agua mediante reflectancia, dicha característica se obtuvo por medio de equipos como: radiómetro (CROPSCAN), escáner de escritorio y cámara fotográfica digital, de igual forma se determinó un índice de verdor utilizando el medidor portátil SPAD Minolta 502 y, la concentración de nitrógeno foliar por el método Kjeldahl. A partir de esas mediciones y con el programa Curve...
Palavras-chave: Agricultura de precisión; Firmas espectrales; Nutriente; Precision agriculture; Spectral signatures; Nitrogen content; Edafología; Maestría.
Ano: 2014
URL: http://hdl.handle.net/10521/2285

Broadcast distribution uniformity of fertilizer with centrifugal spreaders used in variable rate application
Provedor de dados: 70
Autores: CUNHA,JOÃO P. A. R.; SOARES FILHO,ROMEU.
ABSTRACT The quality of fertilizer distribution process is important to the success of agriculture. This research aimed to study the distribution uniformity of fertilizers with spreaders capable of performing variable rate. Evaluations were carried out in different farms, in the Southwest region of the State of Goiás, Brazil. 13 longitudinal and transversal distribution profiles with 11 centrifugal spreaders were evaluated: five with limestone, two with gypsum, two with magnesium oxide, one with monoammonium phosphate (MAP), one with super simple phosphate (SS), one with chloride potassium (KCl) and one with formulated fertilizer (02-20-20). The collectors and the form of distribution followed the ASABE S341.3 standard (2006). The broadcasted distribution...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertilizer distribution; Broadcast spreaders; Precision agriculture.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500928

ESTIMATION OF MAIZE BIOMASS USING UNMANNED AERIAL VEHICLES
Provedor de dados: 70
Autores: Calou,Vinícius B. C.; Teixeira,Adunias dos S.; Moreira,Luis C. J.; Rocha Neto,Odílio C. da; Silva,José A. da.
ABSTRACT Unmanned aerial vehicles (UAVs) are a promising tool for technology development and transfer and for the economic success of the agricultural sector. The objective of this study is to assess the validity of biomass estimation in a commercial maize plantation using aerial images obtained by a UAV. The proposed methodology involved analyzing images acquired in scheduled flights, processing orthophoto (georeferenced image) data, evaluating digital terrain elevation models, and assessing the quality of dense point clouds. Data were collected using two cameras, one with a 16-megapixel flat lens and the other with a 12-megapixel fish-eye lens coupled to a UAV, at two flight altitudes (30 and 60 meters) over hybrid maize (AG1051) crop irrigated by center...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Structure from Motion; Unmanned aerial vehicles; Zea mays L.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600744

SOIL ATTRIBUTES AND WHEAT PERFORMANCE IN A GEOREFERENCED SEED PRODUCTION FIELD
Provedor de dados: 70
Autores: Gadotti,Gizele I.; Corrêa,Marciabela F.; Navroski,Renan; Nadal,Ariele P.; Schuch,Luis O. B.
ABSTRACT The aim of this research was to study the linear correlations and spatial distribution between soil attributes and productivity and physiological quality of wheat seeds. Soil samples were collected at georeferenced points in an area of 41 ha with a rectangular grid of 100 × 100 m to determine soil fertility. Grain productivity, number of ears m-2, protein content, and physiological seed quality were assessed. The results were submitted to Pearson's correlation analysis, descriptive statistics, and geostatistics. Phosphorus content presented a high spatial variability, with a coefficient of variation of 97.79%. Protein content, number of ears, and SMP index presented low values of coefficient of variation, indicating their low spatial variability....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Fertility; Seed quality; Triticum aestivum L.; Spatial variability.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400624

Auger-type granular fertylizer distributor: matemathical model and dynamic simulation
Provedor de dados: 70
Autores: Garcia,Angel P.; Cappelli,Nelson L.; Umezu,Claudio K.
The objective of this study was to model mathematically and to simulate the dynamic behavior of an auger-type fertilizer applicator (AFA) in order to use the variable-rate application (VRA) and reduce the coefficient of variation (CV) of the application, proposing an angular speed controller θ' for the motor drive shaft. The input model was θ' and the response was the fertilizer mass flow, due to the construction, density of fertilizer, fill factor and the end position of the auger. The model was used to simulate a control system in open loop, with an electric drive for AFA using an armature voltage (V A) controller. By introducing a sinusoidal excitation signal in V A with amplitude and delay phase optimized and varying θ' during an operation cycle, it is...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Seeder fertilizer drill; Modeling; Precision agriculture.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100016

SPATIAL AUTOCORRELATION OF PHYSICAL ATTRIBUTES OF AN OXISOL
Provedor de dados: 70
Autores: Oliveira,Job T. de; Oliveira,Rubens A. de; Cunha,Fernando F. da; Santos,Eduardo S. dos.
ABSTRACT Studies that seek to identify a smaller number of soil attributes that represent others can generate less expenditure of time and financial resources for monitoring cultivated areas. Thus, this study aimed to analyze the spatial distribution and spatial autocorrelation of physical attributes of an Oxisol (Latossolo Vermelho Amarelo, Brazilian Soil Classification System). The evaluated attributes consisted of soil density (SD), total porosity (TP), free porosity (FP), field capacity (FC), permanent wilt point (PW), and total water availability (TW). Semivariogram adjustments and semivariance estimates were performed to characterize the structure and magnitude of the spatial dependence of soil attributes. The attributes were distributed on thematic...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Spatial dependence; Geostatistics; Moran index.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200255

POSITION ERRORS IN SOWING IN CURVED AND RECTILINEAR ROUTES USING AUTOPILOT
Provedor de dados: 70
Autores: Santos,Adão F. dos; Correa,Lígia N.; Gírio,Lucas A. S.; Paixão,Carla S. S.; Silva,Rouverson P. da.
ABSTRACT The use of automatic routing significantly increases the yield and quality of agricultural operations and reduces the overlap rates between the mechanized set passes during the operation. The objective of this study was to analyse the quality of peanut sowing using automatic routing in two paths, curved and rectilinear, based on the error of parallelism and execution error, through statistical process control. The maps used came from an area of peanut seed production, in the city of Luzitânia, São Paulo, Brazil. The sowing was carried out by the execution of a project elaborated in CAD software that, for its elaboration, was taken into consideration the working width of the seeder-fertilizer, as well as the spacing of the crop. The CenterPoint RTX...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Peanut; GNSS; Parallelism; RTX.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400568

SPATIAL VARIABILITY IN LEAF ANALYSIS AND PRODUCTIVITY OF FERTIRRIGATED AÇAÍ
Provedor de dados: 70
Autores: Ribeiro,Felipe O.; Fernandes,Antonio R.; Matos,Gilson S. B. de; Lindolfo,Marcelo M.; Guedes,Rafael S.; Rodrigues,Graziele R.
ABSTRACT This study aimed to define management zones (MZs) for fertirrigated açaí cultivation, based on spatial variability of the foliar nutrients and productivity data. The work was carried out in an area of 5.75 ha of a 7-year crop, with 80 georeferenced sample points. Fresh fruit productivity and nutrient (N, P, K, Ca, Mg, S, B, Cu, Fe, Mn, and Zn) contents were determined. The average contents of macronutrients were considered adequate for adult açaí plants, and their spatial dependence associated with fruit productivity allowed the representation of their distributions through maps of variability. Through multivariate analysis, three main components were highlighted. These components explained 51.5 % of the total variability of the data, where PC1...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Amazon; Management zones; Multivariate analysis; Nutrient contents; Precision agriculture.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600800

EFFECT OF HEIGHT, TILT AND TWIST ANGLES OF AN ACTIVE REFLECTANCE SENSOR ON NDVI MEASUREMENTS
Provedor de dados: 70
Autores: Stocker,Vinícius; Souza,Eduardo G. de; Johann,Jerry A.; Beneduzzi,Humberto M.; Silva,Franciléia de O. e.
ABSTRACT The application of nitrogen (N) fertilizer is complex and expensive, so its correct management has financial and environmental benefits. The use of optical proximity sensors is a promising technique. However, the movement of the agricultural machinery or of the person carrying the sensor will result in height differences and/or different tilt and twist angles with respect to the canopy. We considered whether these variations would affect the reflectance measurement. In this study, we took normalized difference vegetation index (NDVI) readings of a wheat canopy, to which 90 kg ha-1 of urea had been applied in stage 5, and observed the NDVI in stages 6, 8 and 10.5. We also tested soybeans, to which 90 kg ha-1 of urea had been applied in stage R1,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitrogen fertilization; Precision agriculture; GreenSeeker; NDVI.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800096

Experimental evaluation of the performance of a wireless sensor network in agricultural environments
Provedor de dados: 70
Autores: Roccia,Clerivaldo; Teruel,Bárbara; Alves,Elaine C. de S.; Arnold,Francisco; Bravo-Roger,Leonardo; Moretti,Angelo; Gonçalves,Marcos S.
The aim of this study was to perform an experimental study to evaluate the proper operation distance between the nodes of a wireless sensor network available on the market for different agricultural crops (maize, physic nut, eucalyptus). The experimental data of the network performance offers to farmers and researchers information that might be useful to the sizing and project of the wireless sensor networks in similar situations to those studied. The evaluation showed that the separation of the nodes depends on the type of culture and it is a critical factor to ensure the feasibility of using WSN. In the configuration used, sending packets every 2 seconds, the battery life was about four days. Therefore, the autonomy may be increased with a longer...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Maize (Zea mays L); Physic nut (Jatropha curcas); Eucalyptus (Eucalyptus grandis); Precision agriculture; Zigbee technology.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600018

Management zones definition using soil chemical and physical attributes in a soybean area
Provedor de dados: 70
Autores: Bazzi,Claudio L.; Souza,Eduardo G.; Uribe-Opazo,Miguel A.; Nóbrega,Lúcia H. P.; Rocha,Davi M.
Several equipments and methodologies have been developed to make available precision agriculture, especially considering the high cost of its implantation and sampling. An interesting possibility is to define management zones aim at dividing producing areas in smaller management zones that could be treated differently, serving as a source of recommendation and analysis. Thus, this trial used physical and chemical properties of soil and yield aiming at the generation of management zones in order to identify whether they can be used as recommendation and analysis. Management zones were generated by the Fuzzy C-Means algorithm and their evaluation was performed by calculating the reduction of variance and performing means tests. The division of the area into...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Spatial variability; Fuzzy clustering; Management zones; Autocorrelation; Cross-correlation.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500007

PERFORMANCE OF HELICAL METERING MECHANISMS IN THE APPLICATION OF MICROGRANULAR FERTILIZER
Provedor de dados: 70
Autores: Spagnolo,Roger T.; Rosa,David P. da; Pinho,Marivan da S.; Schiavon,Cheiner S.; Schmechel,Diego K.
ABSTRACT The use of microgranular fertilizers is currently increasing, with low application rates as an obstacle in the mechanization. This study aimed to verify the performance of helical metering mechanisms using microgranular fertilizer. Four different fertilizer-metering mechanisms were tested at two pre-established dose rates (35 and 50 kg ha−1) and seven longitudinal angles (−15°, −10°, −5°, 0°, +5°, +10°, and +15°). The experiment was carried out according to Brazilian standards. The results showed that the longitudinal inclination affects the actual fertilizer dose in all tested metering systems. Metering mechanisms with a helicoid with longitudinal and lateral overflow presented a similar dose, according to the variation of the longitudinal...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural equipment; Longitudinal inclination; Precision agriculture.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400481

Management zones in agriculture acording to the soil and landscape variables
Provedor de dados: 70
Autores: Delalibera,Hevandro C.; Weirich Neto,Pedro H.; Nagata,Noemi.
The study of spatial variability of soil and plants attributes, or precision agriculture, a technique that aims the rational use of natural resources, is expanding commercially in Brazil. Nevertheless, there is a lack of mathematical analysis that supports the correlation of these independent variables and their interactions with the productivity, identifying scientific standards technologically applicable. The aim of this study was to identify patterns of soil variability according to the eleven physical and seven chemical indicators in an agricultural area. It was used two multivariate techniques: the hierarchical cluster analysis (HCA) and the principal component analysis (PCA). According to the HCA, the area was divided into five management zones: zone...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Multivariate analysis; Precision agriculture; Spatial variability.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600021

MANAGEMENT CLASS DELIMITATION IN A SOYBEAN CROP USING ORBITAL IMAGES
Provedor de dados: 70
Autores: Zanella,Marco A.; Queiroz,Daniel M. de; Valente,Domingos S. M.; Pinto,Francisco de A. de C.; Santos,Nerilson T.
ABSTRACT The delimitation of management classes is critical for successful precision agriculture. This process involves choosing the variables to use and analyzing the spatial variability of the variables. Thus, the objective of this study was to analyze the correlation between management class maps generated from orbital images and yield maps. A 95-hectare area of rainfed grain was evaluated. Yield maps were obtained for the 2015/2016 and 2016/2017 soybean crops. Orbital images were used from two dates for each crop to generate vegetation index maps. The spatial correlation between the vegetation indices and the yield maps was obtained using a bivariate Moran index. The delineated management classes were compared using the Kappa index. This study...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Vegetation index; Yield map.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500676

GPS receivers for georeferencing of spatial variability of soil attributes
Provedor de dados: 70
Autores: Rosalen,David L; Rodrigues,Marcos S; Chioderoli,Carlos A; Brandão,Flavia J. C; Siqueira,Diego S.
The characterization of the spatial variability of soil attributes is essential to support agricultural practices in a sustainable manner. The use of geostatistics to characterize spatial variability of these attributes, such as soil resistance to penetration (RP) and gravimetric soil moisture (GM) is now usual practice in precision agriculture. The result of geostatistical analysis is dependent on the sample density and other factors according to the georeferencing methodology used. Thus, this study aimed to compare two methods of georeferencing to characterize the spatial variability of RP and GM as well as the spatial correlation of these variables. Sampling grid of 60 points spaced 20 m was used. For RP measurements, an electronic penetrometer was used...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; GNSS; Compaction; Soil water content.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600013

Determination of management zones from normalized and standardized equivalent produtivity maps in the soybean culture
Provedor de dados: 70
Autores: Suszek,Grazieli; Souza,Eduardo G. de; Uribe-Opazo,Miguel A.; Nobrega,Lucia H. P.
Through the site-specific management, the precision agriculture brings new techniques for the agricultural sector, as well as a larger detailing of the used methods and increase of the global efficiency of the system. The objective of this work was to analyze two techniques for definition of management zones using soybean yield maps, in a productive area handled with localized fertilization and other with conventional fertilization. The sampling area has 1.74 ha, with 128 plots with site-specific fertilization and 128 plots with conventional fertilization. The productivity data were normalized by two techniques (normalized and standardized equivalent productivity), being later classified in management zones. It can be concluded that the two methods of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thematic map; Precision agriculture; Geostatistics; Soybean.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500007

SPECTRAL VEGETATION INDEXES APPLIED TO NITROGEN SUFFICIENCY INDEX: A STRATEGY WITH POTENTIAL TO INCREASE NITROGEN USE EFFICIENCY ON TOMATO CROP
Provedor de dados: 70
Autores: Oliveira,Thiago F.; Pinto,Francisco A. C.; Silva,Derly J. H.
ABSTRACT The tomato crop is one of the most demanding of nitrogen fertilizers. This element on soil has an elevated mobility that can represent danger to the environment and reduces its efficiency. Therefore, the purpose of this study was to evaluate the methodology for recommending nitrogen fertilizer for tutored tomatoes with a variable rate based on nitrogen sufficiency index. The treatments consisted of a reference plot and five treatments with the nitrogen sufficiency index calculated on spectral indexes NDVI, GNDVI, MCARI, PSSRa and the SPAD value. The productivity was evaluated considering the fruits size and viability. The descriptors of quality, color, soluble solids, total acidity, titratable acidity and flavor were also evaluated. All the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fruit quality; Precision agriculture; Tomato nutrition; Variable rate fertilization.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100118

COMPARING A SINGLE-SENSOR CAMERA WITH A MULTISENSOR CAMERA FOR MONITORING COFFEE CROP USING UNMANNED AERIAL VEHICLES
Provedor de dados: 70
Autores: Gomes,Amanda P. A.; Queiroz,Daniel M. de; Valente,Domingos S. M.; Pinto,Francisco de A. de C.; Rosas,Jorge T. F.
ABSTRACT There exist two options for digital cameras that can capture the near-infrared (NIR) band. Conventional red–green–blue (RGB, visible bands) cameras with a single sensor provide NIR band visibility based on the removal of the internal NIR-blocking filter. Alternatively, multisensor cameras exist that have a specific sensor for each band. The modified RGB cameras are of a lower price. In this context, the objective of this study was to compare the performance of a modified RGB camera with that of a multisensor camera for obtaining the normalized difference vegetation index (NDVI) in an area with coffee cultivations. A multispectral camera with five sensors and another camera with only one sensor were used. The NDVI of the coffee field was also...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; UAV; Radiometric calibration; Modified RGB camera.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100087

SAMPLING DENSITY FOR CHARACTERIZING THE PHYSICAL QUALITY OF A SOIL UNDER COFFEE CULTIVATION IN SOUTHWESTERN MINAS GERAIS
Provedor de dados: 70
Autores: Silvero,Nélida E. Q.; Marques Júnior,José; Siqueira,Diego S.; Gomes,Romário P.; Costa,Milene M. R.
ABSTRACT The elaboration of maps to characterize the spatial variability of soil attributes assists in the strategic planning and decision making of agricultural managers. Precision and accuracy of maps are related to the ideal sampling density to characterize the variability pattern. This study was conducted with the aim of identifying the sampling density to represent the variability of soil physical quality using attributes with different magnitudes of variation in an area cultivated with coffee. Three approaches were used to find the most adequate sampling density (geostatistical analysis, percentage of error associated with the sampling density, and coefficient of variation). A total of 145 soil samples were collected at a depth of 0-0.20 m at the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Coffea arabica; Sampling error; Geostatistics.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500718

CONTRIBUTION OF SOIL ATTRIBUTES AND MORPHOLOGICAL VARIABLES TO YIELD OF IRRIGATED GARLIC
Provedor de dados: 70
Autores: Oliveira,Job T. de; Oliveira,Rubens A. de; Furtado Junior,Marconi R.
ABSTRACT This study aimed to investigate relationships between the soil attributes that most affect garlic yield, which can be useful to choose a new area for the growing of this vegetable. We also aimed to study the effects of irrigation deficit at bulb formation stage (cloves) on final garlic quality and yield. The variables evaluated were garlic yield, irrigation, nitrogen, lateral shoot growing, plant water potential, bulb volume, leaf area index, soil electrical conductivity, soil mechanical resistance to penetration, and volumetric soil moisture content. Initially, the Pearson's correlation was estimated for the phenological indexes, and a correlation network was used to graphically express the results and to correct multicollinearity between...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Allium sativum L.; Path analysis; Precision irrigation; Precision agriculture.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200215

Management zones using fuzzy clustering based on spatial-temporal variability of soil and corn yield
Provedor de dados: 70
Autores: Rodrigues,Marcos S.; Corá,José E.
Clustering soil and crop data can be used as a basis for the definition of management zones because the data are grouped into clusters based on the similar interaction of these variables. Therefore, the objective of this study was to identify management zones using fuzzy c-means clustering analysis based on the spatial and temporal variability of soil attributes and corn yield. The study site (18 by 250-m in size) was located in Jaboticabal, São Paulo/Brazil. Corn yield was measured in one hundred 4.5 by 10-m cells along four parallel transects (25 observations per transect) over five growing seasons between 2001 and 2010. Soil chemical and physical attributes were measured. SAS procedure MIXED was used to identify which variable(s) most influenced the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Management zone analyst; Precision agriculture; Soil pH; Tropical soils; Zea mays L.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300470

Redundant variables and the quality of management zones
Provedor de dados: 70
Autores: Ricardo,Sobjak; Souza,Eduardo G. de; Bazzi,Claudio L.; Uribe-Opazo,Miguel A.; Betzek,Nelson M.
ABSTRACT Precision agriculture (PA) allows farmers to identify and address variations in an agriculture field. Management zones (MZs) make PA more feasible and economical. The most important method for defining MZs is a fuzzy C-means algorithm, but selecting the variable for use as the input layer in the fuzzy process is problematic. BAZZI et al. (2013) used Moran’s bivariate spatial autocorrelation statistic to identify variables that are spatially correlated with yield while employing spatial autocorrelation. BAZZI et al. (2013) proposed that all redundant variables be eliminated and that the remaining variables would be considered appropriate on the MZ generation process. Thus, the objective of this work, a study case, was to test the hypothesis that...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Spatial correlation; Relative efficiency.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100078

CORRELATIONS AMONG VEGETATION INDICES AND PEANUT TRAITS DURING DIFFERENT CROP DEVELOPMENT STAGES
Provedor de dados: 70
Autores: Carneiro,Franciele M.; Furlani,Carlos E. A.; Zerbato,Cristiano; Menezes,Patricia C. de; Gírio,Lucas A. da S.
ABSTRACT Active optical sensors have been widely used for the spatial and temporal monitoring of peanut culture because they are accurate, non-destructive methods for rapidly obtaining data. The objective of this study was to determine the optimal stage of crop growth for collecting sensor readings based on correlations between quality indicators. In addition, we compared vegetation indices (Normalized Difference Vegetation Index [NDVI], Normalized Difference Red-Edge Index, [NDRE], and Inverse Ratio Vegetation Index, [IRVI]) by monitoring temporal variability in the peanut crop in order to determine which of them obtained the best reading quality throughout the process. The experiment was performed on the 2016/17 crop in the agricultural area of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Remote sensing; Arachis hypogaea L.; Control charts; Precision agriculture.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800033

Spatial variability of yield and other parameters associated with pear trees
Provedor de dados: 70
Autores: Konopatzki,Marcia R. S.; Souza,Eduardo G.; Nóbrega,Lúcia H. P.; Uribe-Opazo,Miguel A.; Suszek,Grazieli.
In the last few years, precision agriculture has become commonly used with many crops, particularly cereals, and there is also interest in precision horticulture. Pear is a seasonal fruit and well appreciated by Brazilian people, although it is mostly imported. Brazilian farmers are nowadays trying to increase pear production. Thus, this research aimed at mapping the yield of pear trees in order to study the spatial variability of yield as well as its comparison with spatial variability of soil and plant attributes. The experimental field had 146 pear trees, variety 'Pêra d'água', distributed on a 1.24 ha. Four harvests were performed according to the fruit ripening and from each tree; only the ripe fruits were harvested. In each harvest, all the fruits...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Thematic maps; Horticulture.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200018

TEMPORAL VARIABILITY IN ACTIVE REFLECTANCE SENSOR-MEASURED NDVI IN SOYBEAN AND WHEAT CROPS
Provedor de dados: 70
Autores: Beneduzzi,Humberto M.; Souza,Eduardo G.; Bazzi,Claudio L.; Schenatto,Kelyn.
ABSTRACT: Optimization of N management is one of the great challenges to be overcome in grain production, as it is directly related to productivity and can also cause environmental damage. Precision agriculture aims to solve this problem by applying nitrogen fertilizer at varying rates. Reflectance sensors are instruments capable of estimating N needs in various crops, including grain crops. However, it is not clear how these sensors perform under varying solar radiation and cloud cover, due to a lack of research on their temporal variability. Thus, this study examined the temporal variability of the NDVI (normalized difference vegetation index), as measured by an active reflectance sensor, in both soybean and wheat crops. The NDVI data were collected...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Remote sensing; Vegetation index; NDVI.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400771

PRODUCTIVITY OF CORN HYBRIDS IN RELATION TO SOWING OVERLAP
Provedor de dados: 70
Autores: Farias,Marcelo S. de; Dagios,Ravel F.; Santi,Antônio L.; Cherubin,Maurício R.
ABSTRACT The automatic control of section shut-off in seed drills minimizes seeding overlap and can reduce productivity losses, especially in responsive crops such as corn. In that context, this study evaluated the effect of sowing overlap on the grain yield and productivity of three corn hybrids. A DB-50 precision seed drill, with 33 rows equipped with a 16-row automatic section control, was used in this experiment. A randomized block design was applied to test three corn hybrids under two sowing conditions (without sowing overlap - WOSO; and with sowing overlap - WSO), with four replications. The analyzed variables were the number of plants per hectare, the number of cobs per hectare, cob length, the number of grains per cob, the thousand grain weight,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays; Precision agriculture; Section control; Plant population.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400489

Soil sampling intensity and spatial distribution pattern of soils attributes and corn yield in no-tillage system
Provedor de dados: 70
Autores: Rodrigues,Marcos S.; Corá,José E.; Fernandes,Carolina.
Taking into account that the sampling intensity of soil attributes is a determining factor for applying of concepts of precision agriculture, this study aims to determine the spatial distribution pattern of soil attributes and corn yield at four soil sampling intensities and verify how sampling intensity affects cause-effect relationship between soil attributes and corn yield. A 100-referenced point sample grid was imposed on the experimental site. Thus, each sampling cell encompassed an area of 45 m² and was composed of five 10-m long crop rows, where referenced points were considered the center of the cell. Samples were taken from at 0 to 0.1 m and 0.1 to 0.2 m depths. Soil chemical attributes and clay content were evaluated. Sampling intensities were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geostatistics; Precision agriculture; Zea mays.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500005

SPATIAL VARIABILITY OF IRRIGATED COMMON BEAN YIELD CORRELATED WITH THE FERTILITY OF A SANDY SOIL
Provedor de dados: 70
Autores: Oliveira,Job T. de; Roque,Cassiano G.; Teodoro,Paulo; Montanari,Rafael.
ABSTRACT The common bean is widely cultivated in Brazil. In the 2016–2017 growing season, an experiment was carried out in a Typic Quartzipsamment (or Neossolo Quartzarênico) soil in the municipality of Cassilândia, MS, Brazil, with the aim of characterizing specific aspects of soil management, using a linear and spatial correlation between the irrigated yield of common beans and the chemical properties of the soil. Soil samples were collected from layers at depths 0.00–0.10 and 0.10–0.20 m, within a grid of 117 georeferenced points. A data analysis was carried out using statistical and geostatistical techniques. A multiple regression analysis showed that about 31% of the grain yield variability of the irrigated common bean crop could be attributed to the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Geostatistics; Soil management; Irrigation; (Phaseolus vulgaris L.).
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500645

Prototype for soil mechanical resistance measurement with chisel plow automated control
Provedor de dados: 70
Autores: MACHADO,THIAGO M.; LANÇAS,KLÉBER P.
ABSTRACT In Brazil, there are several available models and systems to measure soil compaction; however, the data generated by such equipment have to be processed and interpreted, making the process expensive. Our study aimed to evaluate a prototype of instrumented rods to identify soil compacted layers and control chiseling depth, and compared it to a conventional system at a fixed depth of 0.35 m. In order to compare them, we assessed the following parameters: hourly fuel consumption, operational fuel consumption, drawbar power, average power, average speed, slipping, tractor effective field capacity and response time. Our results showed that mechanical chiseling at variable depths reduced in 26% the operational fuel consumption and increased in 14% the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Soil compaction; Chiseling.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400646

ASSEMBLY OF A REMOTELY PILOTED AIRCRAFT OF LOW COST APPLIED TO AGRICULTURE
Provedor de dados: 70
Autores: Cunha,João P. A. R. Da; Sirqueira Neto,Matheus A.
ABSTRACT: The remotely piloted aircraft (RPA) have great applicability in agriculture. Although it is a technology that has been developed for many years, in the field of agriculture it passed unnoticed for a long time. The high cost of acquisition is still a limiting factor for small and medium-sized farmers. In this way, this study had as objective to develop a low cost RPA for agriculture application. In the present study, the development and the assembly of an RPA prototype of a quadcopter type is presented, consisting of four engines and of vertical propulsion, capable of moving without human intervention, that is, autonomous flight, applied to agriculture and low cost investment. In it was boarded a data control and processing system collected from...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Quadcopters; RPA.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601268

Amostragem de solo em plantio direto para aplicação em agricultura de precisão.
Provedor de dados: 14
Autores: CARVALHO, J. R. P. de.
O objetivo deste estudo seria a comparação das diversas técnicas estatísticas disponíveis, visando o estudo da amostragem de solo para plantio direto. Com a formação de bases de dados digitais e melhores métodos para coleção de dados e análise geoestatfstica, estudos mais detalhados podem ser realizados sobre a variação dos solos e suas conseqüências.
Tipo: Folhetos
Palavras-chave: Pedometria; Amostragem de solo; Geoestatística; Pedometric; Agricultura de Precisão; Plantio Direto; Soil sampling; No-tillage; Geostatistics; Precision agriculture.
Ano: 1999
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/7537

Técnicas inovadoras de melhoramento de precisão.
Provedor de dados: 14
Autores: NEPOMUCENO, A. L.
Tipo: Artigo na mídia
Palavras-chave: Agricultura de Precisão; Biotecnologia; Inovação; Precision agriculture; Biotechnology; Innovation adoption.
Ano: 2018
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1107315

Agricultura irrigada: potencialidade do semiárido.
Provedor de dados: 14
A Vitivinicultura no Semiárido; A Mangicultura no Semiárido; Outras frutíferas no Semiárido; Novos cultivos de frutíferas no Semiárido; A Olericultura no Semiárido; Perspectivas para o futuro da Agricultura irrigada no Semiárido.
Tipo: Fascículos de periódicos
Palavras-chave: Agricultura de baixo carbono; Semiárido; Agricultura irrigada; Fruticultura irrigada; Vinho tropical; Suco de uva; Certificação do Vale São Francisco; Agricultura; Irrigação; Fruticultura; Viticultura; Manga; Citricultura; Olericultura; Mudança Climática; Economia da Produção; Desenvolvimento Socio-Econômico; Agriculture; Precision agriculture; Tropical agriculture; Sustainable agriculture; Fruit products; Fruit wines; Fruiting; Tropical and subtropical fruits; Irrigation; Irrigation management; Social impact; Social environment; Agricultural economics.
Ano: 2015
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1098479

Greenhouse Gas and Animal Agriculture Conference: proceedings of the 7th GGAA - august 4th to 8th, Iguassu Falls/Brazil.
Provedor de dados: 14
The Greenhouse Gas and Animal Agriculture Conference (GGAA) is the premier international conference summarising the collective state of scientific knowledge on greenhouse gas abatement strategies and production systems adaptation needs for the livestock sector. The gathering features leading scientists and policymakers reviewing the current state of knowledge and presenting significant new developments in policy, measurement, modelling, mitigation and adaptation efforts associated with greenhouse gases from animal agriculture. The Conference takes place every 3 years, moving from continent to continent at each edition. The first conference, GGAA2003, was held in Japan with 200 delegates from 20 countries. Five subsequent GGAA conferences have been...
Tipo: Livros
Palavras-chave: Gás de efeito estufa; Baixo carbono; Agricultura de Precisão; Precision agriculture; Greenhouse gases.
Ano: 2019
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1116059

Agricultura de precisão em fruticultura.
Provedor de dados: 14
Autores: BASSOI, L. H.; MIELE, A.; REISSER JUNIOR, C.; GEBLER, L.; FLORES, C. A.; FILIPPINI ALBA, J. M.; GREGO, C. R.; TERRA, V. S. S.; TIMM, L. C.; NASCIMENTO, P. dos S.
Os sistemas de produção atualmente existentes na fruticultura brasileira caracterizam-se pela execução de diversas práticas agrícolas durante o ciclo da cultura, tendo como preocupação a quantidade e a qualidade da produção, e a rentabilidade da atividade agrícola. Nesse contexto, cria-se uma oportunidade para a aplicação de agricultura de precisão, como forma de auxiliar a gestão do sistema de produção e a tomada de decisão pelo produtor. Nesse capítulo, são apresentados quatro estudos de caso em que a realização de procedimentos e o uso de ferramentas, característicos de agricultura de precisão, permitem aos produtores e técnicos a compreensão da variabilidade de atributos do solo e da planta e de suas relações, bem como o estabelecimento de zonas...
Tipo: Parte de livro
Palavras-chave: Geoestatística; Análise multivariada; Agricultura de precisao; Fruticultura; Viticultura; Estatística agrícola; Método estatístico; Maçã; Pêssego; Uva; Precision agriculture; Fruit growing; Viticulture; Geostatistics; Agricultural statistics; Multivariate analysis.
Ano: 2014
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1008274

Repositório de Recursos de Informação da Rede de Agricultura de Precisão da Embrapa (Rede AP): manual do usuário: Versão 1.0.
Provedor de dados: 14
Autores: SPERANZA, E. A.; QUEIROS, L. R.
Perfis de Acesso e Administração. Acesso ao Repositório. Repositório de Dados. Visualizar Dados Georreferenciados. Catalogação de Metadados.
Tipo: Livros
Palavras-chave: Ferramenta computacional; Metadados geoespaciais; Agricultura de Precisão; Precision agriculture.
Ano: 2012
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/952782

Geoestatística aplicada a agricultura de precisão.
Provedor de dados: 14
Autores: GREGO, C. R.; OLIVEIRA, R. P. de; VIEIRA, S. R.
A agricultura de precisão se baseia na aplicação de tecnologias de maneira localizada de acordo com a variabilidade espacial, a qual a geoestatística está diretamente relacionada. Geoestatística é uma ferramenta que utiliza o conceito de variáveis regionalizadas na avaliação de variabilidade espacial por meio da extração e organização espacial dos dados disponíveis de acordo com a semelhança entre pontos vizinhos georreferenciados. Não se limita apenas em obter um modelo de dependência espacial, pretende também estimar valores nos locais não amostrados. O objetivo do capítulo é apresentar os conceitos básicos da ferramenta geoestatística e como ela pode ser aplicada em agricultura de precisão. Para tanto procurou-se abordar a conceituação da...
Tipo: Parte de livro
Palavras-chave: Mapas precisos; Variabilidade espacial; Georreferenciamento; Manejo localizado; Agricultura de precisão; Precision agriculture.
Ano: 2014
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1004020

Procedimentos metodológicos utilizados na compilação de dados do Modeflora para construção de mapas dinâmicos no cartão microSD para uso no GPS.
Provedor de dados: 14
Autores: FIGUEIREDO, E. O.; HALK, T. de M.; PAPA, D. de A.; CUNHA, R. M da; CASSOL, H. L. G.
O planejamento da exploração florestal em florestas tropicais, realizada com técnicas de precisão recomendadas pelo Modelo Digital de Exploração Florestal (Modeflora), permite significativas vantagens. Porém, para que o planejamento da exploração florestal seja executado com precisão e agilidade pelas equipes de campo, é necessário que todas as informações estejam consolidadas num mapa dinâmico. Para que todas as informações fiquem consolidadas num único conjunto de mapas dinâmicos, há necessidade de compilar os dados em um formato de arquivo digital (IMG), o qual é reconhecido pelos receptores GPS e navegadores automotivos. Este trabalho demonstra os Procedimentos metodológicos utilizados na compilação de dados do Modeflora para construção de mapas...
Tipo: Folhetos
Palavras-chave: Manejo florestal; Manejo de precisão; Geotécnica; Modelagem 3D; Sistema de posicionamento global; Biometria florestal; Forest biometry; Biometría forestal; Modeflora; Teledetección; Sistemas de posicionamiento global; Sistemas de información geográfica; Manejo forestal; Inventario forestal; Geoespatial technology; Agricultura de precisión; Tecnología geoespacial; Administração florestal; Sensoriamento remoto; Sistema de informação geográfica; Agricultura de precisão; Inventário florestal; Forest management; Precision agriculture; Remote sensing; Global positioning systems; Forest inventory; Geographic information systems.
Ano: 2010
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/877753

Gestão de recursos de informação em Agricultura de Precisão.
Provedor de dados: 14
Autores: QUEIROS, L. R.; SPERANZA, E. A.; BETTIOL, G. M.; FILIPPINI ALBA, J. M.; BERNARDI, A. C. de C.; INAMASU, R. Y.; GREGO, C. R.; RABELLO, L. M.
Diante da natureza multidisciplinar das pesquisas agrícolas, em especial as pesquisas em Agricultura de Precisão, da crescente produção de dados digitais em diferentes formatos e padrões, e da necessidade crescente de recuperação com qualidade e intercâmbio desses dados, torna-se necessário o estabelecimento de estratégias para sua gestão. Dentre essas estratégias, destaca-se a definição clara das normalizações e dos padrões de metadados a serem adotados.
Tipo: Folhetos
Palavras-chave: Metadados; Organização da informação; Agricultura de Precisão; Base de Dados; Databases; Precision agriculture.
Ano: 2011
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/903343

Estratégia de implantação, gestão e funcionamento da Rede Agricultura de Precisão.
Provedor de dados: 14
Autores: INAMASU, R. Y.; BERNARDI, A. C. de C.; NAIME, J. de M.; QUEIROS, L. R.; RESENDE, Á. V. de; VILELA, M. de F.; BASSOI, L. H.; PEREZ, N. B.; FRAGALLE, E. P.
Resumo: A globalização da produção para a alimentação requer proteção, gestão e precisão. O cenário contemporâneo da agricultura brasileira. O cenário atual da agricultura brasileira caminha para uma produção eficiente, com proteção ao meio ambiente. A economia em escala global evidenciou o protagonismo do Brasil, especialmente nesta época, quando há um aumento no consumo mundial de alimentos e a necessidade de produzir energia renovável. O País possui terras, condições climáticas e tecnologia para ajudar a suprir a si e a outras nações com alimento e energia renovável. Para isso, também necessita melhorar sua competitividade em áreas como a pecuária e silvicultura e produtos como o trigo e o algodão, sem perder a perspectiva da sustentabilidade. E a...
Tipo: Parte de livro
Palavras-chave: Banco de dados; Inovação tecnológica; Condutividade elétrica do solo; Imagem aérea; New technology; Agricultura de Precisão; Precision agriculture; Databases.
Ano: 2011
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/908516

Estudo de caso 1 - técnicas de agricultura de precisão para criação de zonas de manejo usando sensores proximais e software R na Fazenda Pamplona, Cristalina, GO.
Provedor de dados: 14
Autores: OLIVEIRA, R. P. de; BRANDAO, Z. N.; RODRIGUES, H. M.
O objetivo geral deste trabalho foi avaliar três técnicas de delineamento de ZMs, tendo como foco a melhoria da produtividade do algodoeiro em um sistema de produção comercial. As três técnicas de obtenção das ZMs aqui utilizadas foram: 1) a partir da combinação de dados de EM38® e MDE; 2) a partir do primeiro componente da análise de componentes principais (PCA), utilizando os dados de EM38® e MDE; e 3) usando mapas espacializados de alguns atributos do solo, coletados em campo após a medição com o sensor EM38. Foram mapeados, para este trabalho, os teores de areia e argila, bem como nutrientes como: N, P, K, Ca, e Mg, obtidos de amostras compostas e medidas em laboratório. O mapa de produtividade do algodoeiro, obtido durante a colheita, foi utilizado...
Tipo: Parte de livro
Palavras-chave: Modelo Digital de Elevação; Zona de Manejo; Sensoriamento Proximal; Sistema de Produção; Algodão; Manejo; Agricultura de Precisão; Mapa; Product system; Precision agriculture; Digital elevation models; Cotton.
Ano: 2022
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1151214

Modelo Digital de Exploração Florestal - MODEFLORA.
Provedor de dados: 14
Autores: PAPA, D. de A.
O Modelo Digital de Exploração Florestal (Modeflora) é uma inovação tecnológica, na área de manejo de precisão, que integra o Sistema de Posicionamento Global (GPS), o Sistema de Informação Geográfica (SIG) e o Sensoriamento Remoto (SR) para planejar, executar e monitorar as atividades de manejo florestal com alta precisão. O uso desses recursos permite representar previamente no computador os aspectos espaciais da realidade florestal. Informações como localização das árvores e nascentes, igarapés, áreas de preservação permanente (APPs), curvas de nível, pontos barométricos e relevo compõem o banco de dados do plano de manejo. Como resultado, o Modelo Digital de Exploração Florestal gera um microzoneamento da área de manejo florestal com escala de até 1,15...
Tipo: Artigo na mídia
Palavras-chave: Geotécnica; Manejo florestal; Manejo de precisão; Modelagem 3D; Sistema de posicionamento global; Modeflora; Forest biometry; Biometría forestal; Biometria florestal; Sistemas de posicionamiento global; Agricultura de precisión; Inventario forestal; Manejo forestal; Sensoriamiento remoto; Sistemas de información geográfica; Tecnología geoespacial; Administração florestal; Sistema de informação geográfica; Agricultura de precisão; Inventário florestal; Sensoriamento remoto; Geospatial technology; Precision agriculture; Forest inventory; Forest management; Geographic information systems; Remote sensing; Global positioning systems.
Ano: 2016
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1055181

Armazenamento e recuperação de dados georreferenciados de condutividade elétrica do solo na Rede de Agricultura de Precisão da Embrapa.
Provedor de dados: 14
Autores: SPERANZA, E. A.; QUEIROS, L. R.; RABELLO, L. M.; GREGO, C. R.; BRANDÃO, Z. N.
Resumo: Este trabalho descreve a implantação de uma ferramenta para armazenamento em uma base de dados espacial de informações georreferenciadas de condutividade elétrica do solo obtidas em campo. A partir dos dados coletados, mapas são gerados para suporte à tomada de decisão em agricultura de precisão. Este trabalho utilizou coletas de dados realizadas em uma área de plantio de cana-de-açúcar em Mogi Mirim, SP no âmbito do projeto da Rede de Agricultura de Precisão da Embrapa (Rede AP).
Tipo: Parte de livro
Palavras-chave: Dados georreferenciados; Condutividade elétrica do solo; Base de dados geoespacial; Georreferenciamento; Agricultura de Precisão; Spatial data; Georeferencing; Precision agriculture.
Ano: 2011
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/908523

Uso de imagens aéreas obtidas com drones em sistemas de produção de soja.
Provedor de dados: 14
Autores: FRANCHINI, J. C.; BALBINOT JUNIOR, A. A.; JORGE, L. A. de C.; DEBIASI, H.; DIAS, W. P.; GODOY, C. V.; OLIVEIRA JUNIOR, A. de; CORREA, F. B.; OLIVEIRA, M. C. N. de.
Tipo: Folhetos
Palavras-chave: Reconhecimento Aéreo; Equipamento Agrícola; Agricultura de Precisão; Soja; Produção Agrícola; Agricultural machinery and equipment; Precision agriculture; Soybeans.
Ano: 2018
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1103613

Modeflora: modelo digital de exploração florestal.
Provedor de dados: 14
Autores: PAPA, D. de A.; FIGUEIREDO, E. O.
O Modelo Digital de Exploração Florestal (Modeflora) é uma inovação tecnológica, na área de manejo florestal sustentável, que integra o Sistema de Posicionamento Global (GPS), o Sistema de Informação Geográfica (SIG) e o Sensoriamento Remoto (SR) para planejar, executar e monitorar as atividades de manejo com alta precisão. O uso desses recursos permite representar previamente no computador os aspectos espaciais da realidade florestal. Informações como localização das árvores e nascentes, igarapés, APP, curvas de nível, pontos barométricos e relevo compõem o banco de dados do plano de manejo. Como resultado, o Modelo Digital de Exploração Florestal gera um microzoneamento da área de manejo florestal com escala de até 1:15 metros. Com isso é possível fazer...
Tipo: Folders
Palavras-chave: Geotécnica; Manejo florestal; Manejo de precisão; Biometria florestal; Forest biometry; Biometría forestal; Sistema de posicionamento global; Modelagem 3D; Modeflora; Inventario forestal; Sistemas de información geográfica; Sistemas de posicionamiento global; Tecnología geoespacial; Agricultura de precisión; Geoespatial technology; Manejo forestal; Teledetección; Administração florestal; Inventário florestal; Agricultura de precisão; Sistema de informação geográfica; Sensoriamento remoto; Forest management; Forest inventory; Precision agriculture; Geographic information systems; Global positioning systems; Remote sensing.
Ano: 2011
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1005198

Coeficientes técnicos para o inventário e manejo florestal com emprego do Modelo Digital de Exploração Florestal (MODEFLORA).
Provedor de dados: 14
Autores: FIGUEIREDO, E. O.; LIMA, Q. S. de.
Devido à crescente demanda por informações sobre os coeficientes técnicos do Modelo Digital, esta publicação apresenta os principais coeficientes técnicos envolvidos no inventário florestal, abertura de estradas e pátios, abate de árvores, arraste de toras e carregamento.
Tipo: Folhetos
Palavras-chave: Geotécnica; Manejo florestal; Manejo de precisão; Biometría forestal; Sistema de posicionamento global; Modelagem 3D; Modeflora; Biometria florestal; Forest biometry; Inventario forestal; Teledetección; Insumos agrícolas; Geoespatial technology; Análisis económico; Agricultura de precisión; Tecnología geoespacial; Sistemas de posicionamiento global; Sistemas de información geográfica; Manejo forestal; Sistema de informação geográfica; Agricultura de precisão; Administração florestal; Inventário florestal; Sensoriamento remoto; Insumo; Análise econômica; Geographic information systems; Precision agriculture; Forest inventory; Forest management; Farm inputs; Economic analysis; Remote sensing; Global positioning systems.
Ano: 2008
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/511370

Estimativa da biomassa de milho por imagens RGB de drones.
Provedor de dados: 14
Autores: ANDRADE JUNIOR, A. S. de; LOPES, A. da S.; BASTOS, E. A.; CARDOSO, M. J.; SOUSA, R. C. M. de.
A biomassa é um parâmetro agronômico estratégico utilizado para indicar o status de crescimento da cultura, por causa dos efeitos das práticas de manejo agrícola. A metodologia convencional para se obter a biomassa ocorre por métodos destrutivos, que requerem a colheita manual das plantas, pesagem e secagem em estufa, inviabilizando as medidas em grandes áreas de produção. Como alternativa, recomendam-se técnicas de sensoriamento remoto com imagens aéreas adquiridas por drones, com boa precisão, economia de tempo e mão de obra. O estudo teve como objetivo a proposição e validação de modelos de estimativa da biomassa seca de plantas de milho, usando-se a altura das plantas extraída de modelos digitais de superfície (CSM) gerados de imagens aéreas de câmera...
Tipo: Folhetos
Palavras-chave: Estrutura de planta; UAV; CSM; Sensoriamento Remoto; Agricultura de Precisão; Zea Mays; Precision agriculture; Plant architecture.
Ano: 2021
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1137276

Modelagem da hidrografia em planos de manejo e critérios para definição de árvores em APP pelo Modeflora.
Provedor de dados: 14
Autores: FIGUEIREDO, E. O.; MOURA, D. C. de S.; FIGUEIREDO, S. M. de M.; PAPA, D. de A.
Novas tecnologias, sendo advindas do geoprocessamento e do sensoriamento remoto, vêm sendo desenvolvidas a fim de auxiliar no processo de delimitação das APPs e demarcação das árvores. No entanto, faltam estudos para investigar e comprovar sua eficácia. Não há registro de trabalhos, publicados no Brasil, que utilizem diferentes metodologias na definição de APPs para avaliá-las. O presente trabalho teve como objetivo propor uma metodologia precisa para o mapeamento de áreas de preservação permanente e definição de árvores protegidas e exploráveis na região de influência das APPs, comprovando a sua aplicabilidade nos PMFS.
Tipo: Folhetos
Palavras-chave: Código Florestal; Área de proteção ambiental; Área de Preservação Permanete (APP); Geotécnica; Manejo florestal; Embrapa Acre; Forest biometry; Sistema de posicionamento global; Modeflora; Modelagem 3D; Manejo de precisão; Biometria florestal; Western Amazon; Amazônia Ocidental; Acre; Rio Branco (AC); Biometría forestal; Sistemas de posicionamiento global; Mapeamento; Agricultura de precisión; Cubierta (plantas); Inventario forestal; Ley ambiental; Manejo forestal; Sistemas de información geográfica; Teledetección; Agricultura de precisão; Inventário florestal; Administração florestal; Sensoriamento remoto; Sistema de informação geográfica; Hidrografia; Vegetação; Cartografia; Hidrologia; Precision agriculture; Forest management; Canopy; Environmental law; Cartography; Remote sensing; Global positioning systems; Geographic information systems; Forest inventory; Hydrology.
Ano: 2009
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/852921

Inovações e avanços radicais que definirão o nosso futuro.
Provedor de dados: 14
Autores: LOPES, M. A.
Apresenta possíveis avanços radicais e inovações para as próximas duas décadas, com base no relatório 100 radical innovation breakthroughs for the future, produzido com foco na União Europeia. O estudo poderá servir de referência na definição de estratégias em outras partes do globo, além de orientar reflexão e debate acerca das implicações econômicas, sociais e éticas decorrentes das próximas ondas de inovação. O Brasil pode, por exemplo, avaliar a importância potencial de cada uma dessas inovações diante de sua realidade maturidade e força relativa do seu sistema de educação, pesquisa e inovação, gerando referências úteis para o fortalecimento de políticas e estímulos, em sintonia com os tempos desafiadores à frente.
Tipo: Artigo na mídia
Palavras-chave: Objetivos de Desenvolvimento Sustentável (ODS); Tecnologias da informação e da comunicação; Inovação tecnológica; Tecnologia da Informação; Inovação; Agricultura de Precisão; Precision agriculture; Communications technology.
Ano: 2019
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1123778

Compilação de dados do Modeflora para construção de mapas dinâmicos em MicroSD na plataforma GPS Garmin 78.
Provedor de dados: 14
Autores: FIGUEIREDO, E. O.; PAPA, D. de A.; OLIVEIRA, M. V. N. d'.
Para que as equipes de exploração florestal executem o planejamento florestal de acordo com as boas práticas e técnica do manejo de precisão se faz necessário a adoção dos procedimentos descritos nesta publicação. Com isso será possível a obtenção de mapas dinâmicos no formato IMG para inserção em cartões de memória de receptores GPS.
Tipo: Folhetos
Palavras-chave: Geotécnica; Manejo florestal; Manejo de precisão; Modelagem 3D; Sistema de posicionamento global; Geoprocessamento; GPS Garmin 78; Modeflora; Biometria florestal; Biometría forestal; Forest biometry; Tecnología geoespacial; Agricultura de precisión; Geoespatial technology; Inventario forestal; Manejo forestal; Sensoriamiento remoto; Sistemas de información geográfica; Sistemas de posicionamiento global; Sensoriamento remoto; Administração florestal; Sistema de informação geográfica; Inventário florestal; Agricultura de precisão; Forest management; Precision agriculture; Geographic information systems; Remote sensing; Global positioning systems; Forest inventory.
Ano: 2016
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1052878

Execução e monitoramento das operações de campo.
Provedor de dados: 14
Autores: FIGUEIREDO, E. O.; BRAZ, E. M.; OLIVEIRA, M. V. N. d'.
A grande vantagem do Modelo Digital de Exploração Florestal (Modeflora) é a compatibilidade da modelagem da realidade de campo com o planejamento do manejo e, principlamente, a facilidade de execução do planejamento pelos operários florestais.
Tipo: Parte de livro
Palavras-chave: Geotécnica; Manejo florestal; Manejo de precisão; Sistema de posicionamento global; Modelagem 3D; Modeflora; Biometria florestal; Forest biometry; Biometría forestal; Agricultura de precisión; Geoespatial technology; Inventario forestal; Manejo forestal; Sistemas de información geográfica; Sistemas de posicionamiento global; Tecnología geoespacial; Teledetección; Administração florestal; Inventário florestal; Agricultura de precisão; Sistema de informação geográfica; Sensoriamento remoto; Forest management; Forest inventory; Precision agriculture; Geographic information systems; Global positioning systems; Remote sensing.
Ano: 2007
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/503868

Manejo de precisão em florestas tropicais: modelo digital de exploração florestal.
Provedor de dados: 14
Esta publicação procura fornecer aos profissionais da engenharia florestal, as principais etapas de campo e escritório para construção do modelo digital de exploração e manejo florestal. As etapas foram selecionadas e descritas de modo que um profissional da área com conhecimento básico de sistema de informação geográfica (GIS) possa planejar os trabalhos de campo e obter um mapa de exploração florestal com a apropriação das coordenadas verdadeiras de todas as árvores, detalhes da hidrografia, relevo e curvas de nível e, ainda, executar a exploração florestal com receptores GPS e navegadores veiculares.
Tipo: Livros
Palavras-chave: Geotécnica; Manejo florestal; Manejo de precisão; Sistema de posicionamento global; Modelagem 3D; Modeflora; Biometria florestal; Forest biometry; Biometría forestal; Sistemas de posicionamiento global; Agricultura de precisión; Geoespatial technology; Inventario forestal; Manejo forestal; Sistemas de información geográfica; Tecnología geoespacial; Teledetección; Inventário florestal; Administração florestal; Sistema de informação geográfica; Agricultura de precisão; Sensoriamento remoto; Global positioning systems; Remote sensing; Forest management; Forest inventory; Precision agriculture; Geographic information systems.
Ano: 2007
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/501879

Metodologia para sugestão de grades amostrais mínimas para monitoramento da variabilidade espacial de videiras.
Provedor de dados: 14
Autores: SPERANZA, E. A.; GREGO, C. R.; GEBLER, L.
Resumo - Na fruticultura, onde as áreas de produção são muito pequenas quando comparadas com as culturas de grãos, a representatividade de uma grade de amostras ideal para a aplicação da geoestatística é muito densa com relação ao que é utilizado na agricultura de precisão (AP) tradicional, o que torna a amostragem uma atividade extremamente cara ao produtor. Assim, metodologias que pretendem propor um número mínimo de amostras necessárias para o estabelecimento de atividades voltadas a AP, considerando a representação satisfatória da variabilidade espacial da área e o custo da coleta de dados e análise são importantes para tomadas de decisão com relação ao manejo. Este trabalho teve como objetivo principal estabelecer uma metodologia, baseada em análise...
Tipo: Folhetos
Palavras-chave: Geoestatística; Análise de agrupamento; Vitivinicultura; Videira; Uva; Viticulture; Precision agriculture; Geostatistics; Cluster analysis.
Ano: 2021
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1137878

Estudo de caso 7 - imagens aéreas na avaliação do vigor e estimativa de produtividade do algodoeiro na Fazenda Pamplona, Cristalina, GO.
Provedor de dados: 14
Autores: BRANDAO, Z. N.; GREGO, C. R.; ZONTA, J. H.
O objetivo deste trabalho foi avaliar a capacidade de índices de vegetação obtidos através de imagens do satélite Sentinel-2, por imagens aéreas de alta resolução e imagens RGB obtidas em VANTs, na estimativa da produtividade do algodoeiro no cerrado de Goiás, monitorando o vigor das plantas através da variabilidade espacial de dois IVs, o MPRI (Modified Photochemical Reflectance Index) e o NDVI (Normalized Difference Vegetation Index) em diferentes estádios fenológicos.
Tipo: Parte de livro
Palavras-chave: Algodoeiro; Índice de vegetação; Modified Photochemical Reflectance Index; Veículos aéreos não-tripulados; Agricultura de Precisão; Vegetation index; Normalized difference vegetation index; Precision agriculture; Unmanned aerial vehicles.
Ano: 2022
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1151323

Potencial de uso das tecnologias de agricultura e pecuária de precisão e automação.
Provedor de dados: 14
Autores: BERNARDI, A. C. de C.; LUCHIARI JUNIOR, A.; PEREZ, N. B.; INAMASU, R. Y.
Tipo: Folhetos
Palavras-chave: Pecuária; Agricultura de Precisão; Tecnologia; Automação; Precision agriculture; Technology.
Ano: 2017
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1069365

Sistematização do índice de oportunidade na adoção da agricultura de precisão para diferentes sistemas produtivos.
Provedor de dados: 14
Autores: OLIVEIRA, R. P. de; BRANDAO, Z. N.; BERNARDI, A. C. de C.; PEREZ, N. B.; FRANCHINI, J. C.; BENITES, V. de M.; SANTI, A.; GEBLER, L.; BASSOI, L. H.; FILIPPINI ALBA, J. M.; SHIRATSUCHI, L. S.
A caracterização da variação espacial da produção é demanda na adoção da agricultura de precisão. Algumas abordagens buscam estabelecer métricas em apoio a uma gestão eficiente do manejo por sítio-específico. Entre as métricas parametrizadas segundo o ajuste do semi-variograma, o índice de oportunidade de adoção quantifica a variação espacial em função da viabilidade operacional das tecnologias disponíveis. Proposto com base em sistemas de produção de grãos australianos, o modelo foi aplicado no Brasil como ação transversal aos experimentos da Rede de Agricultura de Precisão da Embrapa. O principal objetivo foi avaliar o potencial de uso do índice aplicado a diferentes sistemas produtivos sob condições comuns de monitoramento no Brasil. Este trabalho...
Tipo: Parte de livro
Palavras-chave: Sistema produtivo; Variação espacial; Agricultura de precisão; Precision agriculture.
Ano: 2014
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1008275

Sistematização do índice de oportunidade na adoção da agricultura de precisão para diferentes sistemas produtivos.
Provedor de dados: 14
Autores: OLIVEIRA, R. P. de; BRANDAO, Z. N.; BERNARDI, A. C. de C.; PEREZ, N. B.; FRANCHINI, J. C.; BENITES, V. de M.; SANTI, A.; GEBLER, L.; BASSOI, L. H.; FILIPPINI ALBA, J. M.; SHIRATSUCHI, L. S.
A caracterização da variação espacial da produção é demanda na adoção da agricultura de precisão. Algumas abordagens buscam estabelecer métricas em apoio a uma gestão eficiente do manejo por sítio-específico. Entre as métricas parametrizadas segundo o ajuste do semi-variograma, o índice de oportunidade de adoção quantifica a variação espacial em função da viabilidade operacional das tecnologias disponíveis. Proposto com base em sistemas de produção de grãos australianos, o modelo foi aplicado no Brasil como ação transversal aos experimentos da Rede de Agricultura de Precisão da Embrapa. O principal objetivo foi avaliar o potencial de uso do índice aplicado a diferentes sistemas produtivos sob condições comuns de monitoramento no Brasil. Este trabalho...
Tipo: Parte de livro
Palavras-chave: Suporte a decisão; Índice de oportunidade; Variação espacial; Sítio-específico; Agricultura de precisão; Precision agriculture.
Ano: 2014
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1004023

Uso de imagens orbitais e suborbitais na caracterização da variabilidade espacial da produtividade.
Provedor de dados: 14
Autores: BRANDAO, Z. N.; OLIVEIRA, R. P. de; SANA, R. S.; SOFIATTI, V.; ZONTA, J. H.; MEDEIROS, J. da C.
Imagens de satélites fornecem dados para gerenciamento de áreas florestadas e culturas com estimativa da produtividade no mundo inteiro. O objetivo desse trabalho foi avaliar a capacidade de índices de vegetação obtidos através de imagens do satélite Landsat-5 e por imagens aéreas de alta resolução na estimativa da produtividade do algodoeiro no cerrado de Goiás. Estimativas do índice de área foliar e medições da altura das plantas também foram realizadas nessas datas. Ao final do mês de abril foram adquiridas imagens aéreas de alta resolução da área de estudo. Índices de vegetação foram obtidos com os dados de refletância das imagens de satélite e aérea. Os resultados mostram que os dados de refletância multiespectral atingiram níveis significativos de...
Tipo: Parte de livro
Palavras-chave: Fotografias aéreas; Imagens de satélite; Variabilidade espacial; Índices de vegetação; Agricultura de precisão; Precision agriculture.
Ano: 2014
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1004025

Agricultura de precisão para a sustentabilidade de sistemas produtivos do agronegócio brasileiro.
Provedor de dados: 14
Autores: INAMASU, R. Y.; BERNARDI, A. C. de C.; VAZ, C. M. P.; NAIME, J. de M.; QUEIROS, L. R.; RESENDE, A. V. de; VILELA, M. de F.; JORGE, L. A. de C.; BASSOI, L. H.; PEREZ, N. B.; FRAGALLE, E. P.
O início da agricultura de precisão (AP) teve foco em máquinas dotadas de receptores GPS (Global Positioning System) e mapas de produtividade. Talvez, devido à essa fase, estabeleceu-se no Brasil, um senso comum de que o tema AP é uma área do conhecimento relacionada à sofisticação das máquinas agrícolas por meio de eletrônicas embarcadas e sistemas computacionais complexos, apesar do impacto final objetivar a sustentabilidade do agronegócio. A comunidade acadêmica, por sua vez, priorizou trabalhos iniciais voltados ao desenvolvimento de máquinas e equipamentos, por entender que ali estavam os principais desafios.
Tipo: Parte de livro
Palavras-chave: Agricultura de Precisão; Sensoriamento Remoto; Precision agriculture; Remote sensing.
Ano: 2011
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/908112

Agricultura de precisão pode melhorar o gerenciamento da produção de uva de mesa.
Provedor de dados: 14
Autores: BASSOI, L. H.
o uso de um monitoramento detalhado do cultivo de uva de mesa pode auxiliar o gerenciamento da produção no Vale do São Francisco, no Nordeste brasileiro. Uma pesquisa realizada pela Embrapa Semiárido mostra que a aplicação da chamada agricultura de precisão (AP) pode revelar diferentes situações em uma mesma área de produção, permitindo que seja realizado um manejo mais adequado. A AP é uma forma de gerenciamento das atividades agrícolas que leva em consideração as variações que as plantas e o solo apresentam em diferentes partes da área de cultivo ao longo do ciclo de produção.
Tipo: Artigo na mídia
Palavras-chave: Uva de mesa; Uva; Agricultura de Precisão; Produção; Precision agriculture.
Ano: 2012
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/919310

AGRICULTURA de precisão.
Provedor de dados: 14
Esta tecnologia tem como objetivo básico aumentar a eficiência da agricultura com redução dos impactos ambientais.
Tipo: Folders
Palavras-chave: Agricultura de Precisão; Tecnologia; Precision agriculture.
Ano: 2001
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/985930

MODEFLORA: Modelo Digital de Exploração Florestal.
Provedor de dados: 14
Autores: FIGUEIREDO, E. O.
Esta publicação apresenta o MODEFLORA, Modelo Digital de Exploração Florestal.
Tipo: Folhetos
Palavras-chave: Geotécnica; Manejo florestal; Modeflora; Biometría forestal; Manejo de precisão; Sistema de posicionamento global; Modelagem 3D; Biometria florestal; Forest biometry; Agricultura de precisión; Teledetección; Tecnología geoespacial; Sistemas de posicionamiento global; Sistemas de información geográfica; Manejo forestal; Inventario forestal; Geoespatial technology; Administração florestal; Inventário florestal; Agricultura de precisão; Sensoriamento remoto; Sistema de informação geográfica; Global positioning systems; Remote sensing; Precision agriculture; Forest inventory; Forest management; Geographic information systems.
Ano: 2008
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/631386

Processamento digital e aprendizado de máquina de imagens aéreas obtidas por aeronaves remotamente pilotadas (RPA) para estimar percentual de cobertura do solo por gramíneas perenes em pomar de citros.
Provedor de dados: 14
Autores: CARVALHO, R. da S.; CARVALHO, J. E. B. de.
A presente metodologia digital tem como objetivo estimar o percentual de cobertura do solo com gramíneas (Urochloa spp.) nas entrelinhas de pomares de citros para fins de pesquisa. Esse processo metodológico digital, combina ferramentas de processamento de imagens aéreas de aeronaves remotamente pilotadas (RPA) e softwares livres de código aberto Fiji ImageJ e Weka (Waikato Environment for Knowledge Analysis), sendo que este último utiliza algoritmos de última geração e técnicas de inteligência artificial (IA) da subárea de aprendizado de máquina (supervisionado). Utilizou-se o método preditivo de classificação de árvore de decisão tendo como algoritmo classificador Random Forest, que é acionado no software Fiji ImageJ a partir do plugin TWS (Trainable...
Tipo: Folhetos
Palavras-chave: Tecnologia digital; Drone; Inteligência artificial; Processamento digital; Agricultura; Equipamento; Cobertura do Solo; Cobertura Vegetal; Fruta Cítrica; Citricultura; Agricultura de Precisão; Agriculture; Drums (equipment); Equipment; Ground cover plants; Vegetation cover; Citrus fruits; Artificial intelligence; Precision agriculture.
Ano: 2022
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1146298

Compactação do solo e produtividade da cultura da soja em área irrigada no Cerrado.
Provedor de dados: 14
Autores: SÁ, M. A. C. de; SHIRATSUCHI, L. S.; FRANZ, C. A. B.; SANTOS JÚNIOR, J. de D. G. dos.
RESUMO: A compactação do solo foi avaliada e correlacionada com a produtividade de soja irrigada (safra 2006) sob plantio direto em dois solos: Latossolo Vermelho Amarelo textura média (LV) e Neossolo Quartzarênico (RQ) na região de Luis Eduardo Magalhães, Bahia, Brasil. Ensaios de campo e laboratório para determinação do Índice de Cone (IC) foram conduzidos, sendo ajustados modelos de IC em função de (conteúdo de água volumétrico), Ds (densidade do solo) e argila. Ensaios de laboratório proporcionaram modelos com R2 mais elevados. Para caracterização da compactação do solo com base no IC, é importante estabelecer as relações matemáticas entre IC e atributos do solo, como Ds e teor de argila. Tanto o LV quanto o RQ sob Cerrado apresentaram valores mais...
Tipo: Folhetos
Palavras-chave: Índice de cone; Soil mechanical resistance; Soil mapping; Agricultura de Precisão; Compactação do Solo; Glycine Max; Mapa; Manejo do Solo; Soja; Precision agriculture; Soybeans; Soil management.
Ano: 2007
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/572302

Multispectral remote sensing for site-specific nitrogen fertilizer management
Provedor de dados: 86
Autores: Bagheri,Nikrooz; Ahmadi,Hojjat; Alavipanah,Seyed Kazem; Omid,Mahmoud.
The objective of this work was to evaluate the use of multispectral remote sensing for site-specific nitrogen fertilizer management. Satellite imagery from the advanced spaceborne thermal emission and reflection radiometer (Aster) was acquired in a 23 ha corn-planted area in Iran. For the collection of field samples, a total of 53 pixels were selected by systematic randomized sampling. The total nitrogen content in corn leaf tissues in these pixels was evaluated. To predict corn canopy nitrogen content, different vegetation indices, such as normalized difference vegetation index (NDVI), soil-adjusted vegetation index (Savi), optimized soil-adjusted vegetation index (Osavi), modified chlorophyll absorption ratio index 2 (MCARI2), and modified triangle...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aster; Nitrogen content; Near infrared; Multispectral response; Precision agriculture; Vegetation indices.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2013001000011

Delineation of irrigation management zones in a Quartzipsamment of the Brazilian semiarid region
Provedor de dados: 86
Autores: Oldoni,Henrique; Bassoi,Luís Henrique.
Abstract The objective of this work was to delineate irrigation management zones using geostatistics and multivariate analysis in different combinations of physical and hydraulic soil properties, as well as to determine the optimal number of management zones in order to avoid overlaping. A field experiment was carried out in a Quartzipsamment, for two years, in an irrigated orchard of table grape, in the Senador Nilo Coelho Irrigation Scheme, in the municipality of Petrolina, in the state of Pernanbuco, Brazil. Soil samples were collected for the determination of soil physico-hydraulic properties. A portable meter was used to measure soil apparent electrical conductivity. Spatial distribution maps were generated using ordinary kriging. Management zones for...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuzzy c-means; Geostatistics; Irrigation planning; Precision agriculture; Soil apparent electrical conductivity; Spatial variability.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2016000901283

On-the-go tropical soil sensing for pH determination using ion-selective electrodes
Provedor de dados: 86
Autores: Silva,Fernanda Cristina de Souza; Molin,José Paulo.
Abstract: The objective of this work was to assess the performance of an antimony ion-selective electrode (ISE) sensor system, using manual and automatic operating modes, for measuring the potential of hydrogen (pH), in real time, in Oxisols with different characteristics. Samples were manually collected and sent to a laboratory for determination of pH in water and calcium chloride, whose values were used as references. Another set of samples was also automatically collected using a commercial equipment, and readings were performed in manual mode. The performance parameters of the sensor system were calculated and evaluated. Part of the soil samples was used to assess the degree of influence of moisture in determining pH. Calibration lines were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Direct soil sensing; Precision agriculture; Real-time mapping.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2018001101189

Sugarcane response to nitrogen rates, measured by a canopy reflectance sensor
Provedor de dados: 86
Autores: Rosa,Hugo José Andrade; Amaral,Lucas Rios do; Molin,José Paulo; Cantarella,Heitor.
Abstract:The objective of this work was to evaluate whether a canopy sensor is capable of estimating sugarcane response to N, as well as to propose strategies for handling the data generated by this device during the decision-making process for crop N fertilization. Four N rate-response experiments were carried out, with N rates varying from 0 to 240 kg ha-1. Two evaluations with the canopy sensor were performed when the plants reached average stalk height of 0.3 and 0.5 m. Only two experiments showed stalk yield response to N rates. The canopy sensor was able to identify the crop response to different N rates and the relationship of the nutrient with sugarcane yield. The response index values obtained from the canopy sensor readings were useful in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: NDVI; Nitrogen fertilization; Optical sensor; Precision agriculture; Proximal sensing.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2015000900840

Soil chemical attributes restricting grain yield in Oxisols under no-tillage system
Provedor de dados: 86
Autores: Corassa,Geomar Mateus; Santi,Antônio Luís; Silva,Vanderlei Rodrigues da; Baron,Felipe Arthur; Reimche,Geovane Boschmann; Fioresi,Dejales; Flora,Diandra Pinto Della.
Abstract: The objective of this work was to identify soil chemical attributes restricting grain yield in Oxisols under the no-tillage system, using directed soil sampling. High, medium, and low yield zones were defined in two agricultural fields using historical yield data of several crops. The yield zones were defined based on the harvest maps of the following crops: corn in 2008/2009, white oat in 2009, and corn in 2012/2013 in field I, with 117.70 ha; and corn in 2009/2010, soybean in 2010/2011, and wheat in 2012 in field II, with 107.30 ha. Soil sampling points were georeferenced in each yield zone, where samples were collected at eight soil depths, spaced 0.05 m apart, totaling 80 variables. Low yields were associated with low cation exchange...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Organic matter; Precision agriculture; Site-specific management; Soil fertility; Soil sampling; Yield zones.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2018001101203

Spatial variability of soil physical attributes in integrated production systems in the Amazon region
Provedor de dados: 86
Autores: Feitosa,Izabela de Lima; Passos,Alexandre Martins Abdão dos; Cipriani,Henrique Nery; Oliveira,Marcelo Silva de; Marcolan,Alaerto Luiz; Vasques,Gustavo Mattos.
Abstract: The objective of this work was to analyze the spatial variability of soil physical attributes in integrated production systems and its relationship with the growth and yield of a corn (Zea mays) crop intercropped with palisade grass (Urochloa brizantha). The experiment was carried out in an integrated crop-livestock (ICL) system and in an integrated crop-livestock-forestry (ICLF) system, in a Plinthic Hapludox. The ICLF system was managed in alleys between eucalyptus (Eucalyptus spp.) rows, spaced at 18, 30, and 42 m. Corn grain and forage yields were positively correlated with soil clay and moisture contents, whereas grain yield was negatively correlated with soil penetration resistance. The lowest corn plant heights and grain yields were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eucalyptus; Urochloa brizantha; Agronomic efficiency; Precision agriculture; Soil compaction; Soil variability.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2019000100600

Correlation of physical and chemical attributes of soil with sugarcane yield
Provedor de dados: 86
Autores: Cerri,Domingos Guilherme Pellegrino; Magalhães,Paulo Sérgio Graziano.
The objective of this work was to evaluate the correlation between sugarcane yield and some physical and chemical attributes of soil. For this, a 42‑ha test area in Araras, SP, Brazil, was used. Soil properties were determined from samples collected at the beginning of the 2003/2004 harvest season, using a regular 100x100 m grid. Yield assessment was done with a yield monitor (Simprocana). Correlation analyses were performed between sugarcane yield and the following soil properties: pH, pH CaCl2, N, C, cone index, clay content, soil organic matter, P, K, Ca, Mg, H+AL, cation exchange capacity, and base saturation. Correlation coefficients were respectively ‑0.05, ‑0.29, 0.33, 0.41, ‑0.27, 0.22, 0.44, ‑0.24, trace, ‑0.06, 0.01, 0.32, 0.14, and 0.04....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum officinarum; Precision agriculture; Soil sampling; Spatial variation; Variation structure.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2012000400018

Infestation maps and spatial stability of main weed species in maize culture
Provedor de dados: 87
Autores: Calha,I.M.; Sousa,E.; González-Andújar,J.L.
A study on the spatial distribution of the major weeds in maize was carried out in 2007 and 2008 in a field located in Golegã (Ribatejo region, Portugal). The geo-referenced sampling focused on 150 points of a 10 x 10 m mesh covering an area of 1.5 ha, before herbicide application and before harvest. In the first year, 40 species (21 botanical families) were identified at seedling stage and only 22 during the last observation. The difference in species richness can be attributed to maize monoculture favouring reduction in species number. Three of the most representative species were selected for the spatial distribution analysis: Solanum nigrum, Chenopodium album and Echinochloa crus-galli. The three species showed an aggregated spatial pattern and spatial...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geo-statistics; Kriging; Precision agriculture; Chenopodium album; Echinochloa crus-galli; Solanum nigrum.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-83582014000200004

Weed mapping using a machine vision system
Provedor de dados: 87
Autores: Silva Junior,M.C.; Pinto,F.A.C.; Queiroz,D.M.; Gómez-Gil,J.; Navas-Gracia,L.M.
Weed mapping is a useful tool for site-specific herbicide applications. The objectives of this study were (1) to determine the percentage of land area covered by weeds in no-till and conventionally tilled fields of common bean using digital image processing and geostatistics, and (2) to compare two types of cameras. Two digital cameras (color and infrared) and a differential GPS were affixed to a center pivot structure for image acquisition. Sample field images were acquired in a regular grid pattern, and the images were processed to estimate the percentage of weed cover. After calculating the georeferenced weed percentage values, maps were constructed using geostatistical techniques. Based on the results, color images are recommended for mapping the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Geostatistic; Common bean.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-83582012000100025

Phytosociological variability of weeds in soybean field
Provedor de dados: 87
Autores: Santi,A.L.; Bona,S.D.; Lamego,F.P.; Basso,C.J.; Eitelwein,M.T.; Cherubin,M.R.; Kaspary,T.E.; Ruchel,Q.; Gallon,M.
Understanding spatial distribution of weeds in the crop enables to perform localized herbicide applications, increasing the technical and economic efficiency of operations and reducing environmental impacts. This work aimed to characterize the spatial and phytosociological variability of weeds occurring in soybean commercial field. It was conducted in an agricultural area located at the municipality of Boa Vista das Missões - RS, during the 2010/2011 harvest season. The area, that had been managed under no-tillage with soybean monoculture (summer) for five years, was divided in regular squares of 50 x 50 m (0.25 ha), totalizing 356 points. For species identification, 0.5 x 0.5 m sample squares were used. During the survey, 1,739 individuals were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Spatial distribution; Importance index value; Variable rate application.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-83582014000100005

Selection of Grids for Weed Mapping
Provedor de dados: 87
Autores: Camicia,R.F.M.; Maggi,M.F.; Souza,E.G.; Jadoski,S.O.; Camicia,R.G.M.; Menechini,W.
This study aimed to assess the degree of similarity presented by thematic maps generated by different sampling grids of weed plants in a commercial agricultural area of 7.95 hectares. Monocotyledons and dicotyledons were counted on the 2012/2013 and 2013/2014 harvests, before soybean planting, in the fallow period after wheat harvest, in both years. A regular grid of 10 x 10 m was produced to sample the invasive plants, used as reference, and the counting was done in 1 m² of each sample point, totaling 795 samples in each year, compared to regular grids of 30 and 50 m, generated from the data exclusion of the standard grid. Twenty-two composite soil samples were taken at a depth of 0-20 cm to correlate soil properties with weeds occurrence. For the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Sample grids; Weeds.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-83582015000200365

2009 PRECISION AGRICULTURAL SERVICES DEALERSHIP SURVEY RESULTS
Provedor de dados: 31
Autores: Whipker,   Linda D.; Akridge,   Jay T.
In the spring of 2009, Crop Life magazine and Purdue University’s Center for Food and Agricultural Business conducted a survey of crop input dealers for the 14th consecutive year. In February, a questionnaire was mailed to 2500 Crop Life retail crop input dealership readers across the US. (See Appendix I to this report for a copy of the questionnaire.) A total of 258 questionnaires were returned, with 241 being usable. This provided an effective response rate of 9.6 percent, the lowest response rate in the 14 year history of the project. (In prior years, response rates have ranged from a high of 38 percent in 1996 to a low of 11 percent in 2001 and 2008.) Consistent with previous surveys, dealerships were asked questions about the types of precision...
Tipo: Working or Discussion Paper
Palavras-chave: Precision agriculture; Geographic information systems (GIS); Crop input dealer; Variable rate application; Site-specific agriculture; Technology adoption.; Agribusiness; Q13; O30; L84.
Ano: 2009
URL: http://purl.umn.edu/56111

Production Cost and the Sequential Adoption of Precision Technology
Provedor de dados: 31
Autores: Ebel,   Robert M.; Schimmelpfennig,   David E.
Tipo: Presentation
Palavras-chave: Production cost; Precision agriculture; Technology adoption; Agribusiness; Crop Production/Industries; Farm Management; Production Economics; Research and Development/Tech Change/Emerging Technologies.
Ano: 2012
URL: http://purl.umn.edu/124393

A Strategic Approach to the Implementation of Precision Agriculture Principles in Cash Crop Farming
Provedor de dados: 31
Autores: Maine,   Ntsikane; Nell,   Wilhelm T.
Precision agriculture is one of the important agricultural technologies that can assist farmers and managers in promoting long-term success. Precision agriculture can help farm managers increase their management capacity, which is of utmost importance in the highly competitive modern agriculture. Increased yields and/or efficient input use can also be achieved with precision agriculture. Precision agriculture also involve a large capital outlay and requires skills in interpreting the masses of generated data. Modern farmers have to engage in pro-active thinking with regard to suitable agricultural systems that can enhance sustainable success of their farming businesses. Farm managers who are contemplating on getting involved in precision agriculture need...
Tipo: Conference Paper or Presentation
Palavras-chave: Precision agriculture; Strategic approach; Farming; Farming success; Crop Production/Industries; Research and Development/Tech Change/Emerging Technologies.
Ano: 2005
URL: http://purl.umn.edu/24259

A Whole Farm Analysis of the Influence of Auto-Steer Navigation on Net Returns, Risk, and Production Practices
Provedor de dados: 31
Autores: Shockley,   Jordan M.; Dillon,   Carl R.; Stombaugh,   Timothy S.
A whole farm economic analysis was conducted to provide a detailed assessment into the economic, risk, and production implications due to the adoption of auto-steer navigation. It was determined that auto-steer navigation was profitable for a grain farmer in Kentucky with net returns increasing up to 0.90% ($3.35/acre). Additionally, the technology could be used in reducing production risk. Adoption of the technology also alters production practices for optimal use.
Tipo: Journal Article
Palavras-chave: Economics; Farm management; Mean-variance; Precision agriculture; Simulation; Farm Management; Risk and Uncertainty; C61; C63; D81; Q12; Q16.
Ano: 2011
URL: http://purl.umn.edu/100640

AN ECONOMIC ASSESSMENT OF THE WHOLE-FARM IMPACT OF PRECISION AGRICULTURE
Provedor de dados: 31
Autores: Olson,   Kent D.; Elisabeth,   Pascal.
The full impact of an investment in a management information system (MIS), such as precision agriculture (PA), comes from improved managerial decision making throughout the whole farm and not just from improvements in a specific part of the farm.  This study was conducted to determine whether the adoption of PA had a positive impact on whole-farm profitability. To overcome problems of simultaneity and self-selection in the adoption decision of PA, this study used a two stage econometric model using data from farms in Southwest Minnesota. The PA adoption decision was evaluated in the first stage, and the impact of adopting PA was evaluated in the second stage. The whole farm rate of return to assets (ROA) was used to measure the impact of PA. For all 212...
Tipo: Conference Paper or Presentation
Palavras-chave: Precision agriculture; Economics; Adoption; Profitability; Agribusiness.
Ano: 2003
URL: http://purl.umn.edu/22119

The Value of Regional Annual Nitrogen Needs Information for Wheat Producers in Oklahoma
Provedor de dados: 31
Autores: Roberts,   David C.; Brorsen,   B. Wade; Raun,   William R.; Solie,   John B.
Crop producers are increasingly interested in reducing nitrogen use without sacrificing yield. Technology is available for precise application at the sub-field level, but adoption has been sluggish. This paper estimates the relative profitability of a field level annual predictor of mid-season N requirements and a regional predictor of the same.
Tipo: Conference Paper or Presentation
Palavras-chave: Nitrogen seeds; Nitrogen use efficiency; Precision agriculture; Wheat; Crop Production/Industries; Research and Development/Tech Change/Emerging Technologies.
Ano: 2008
URL: http://purl.umn.edu/6734

Farmers’ Perception of Precision Technology:  The Case of Autosteer Adoption by Cotton Farmers
Provedor de dados: 31
Autores: D'Antoni,   Jeremy M.; Mishra,   Ashok K.; Powell,   Rebekah R.; Martin,   Steven W.
Precision agriculture and autosteer technology are, overall, profitable investments for farmers, as previous literature has established. However, what has not been investigated is whether or not farmers perceive these technologies as such. This research postulates that cotton farmers must see potential for higher profits as a result of adopting precision technologies in order to adopt it. Using the 2009 Southern Cotton Precision Farming Survey  and multinomial logit model, this research investigates farmers’ perception of precision agriculture and how those perceptions impact adoption of the autosteer GPS guidance system. Autosteer adoption was found to be significant and positively related to the perceived future importance of precision agriculture as...
Tipo: Presentation
Palavras-chave: Farmers’ perception; Precision agriculture; Autosteer; Multinomial logit estimation; Technology adoption; Input cost saving.; Agribusiness; Agricultural Finance; Farm Management; Financial Economics; Labor and Human Capital; Production Economics; Risk and Uncertainty; Q12; Q16.
Ano: 2012
URL: http://purl.umn.edu/119734

SPATIOTEMPORAL MODELING OF AGRICULTURAL YIELD MONITOR DATA
Provedor de dados: 31
Autores: Nistor,   Adela P.; Florax,   Raymond J.G.M.; Lowenberg-DeBoer,   James; Brown,   Jason P.
Replaced with revised version of paper 03/06/08.
Tipo: Working or Discussion Paper
Palavras-chave: Corn; Drainage; Precision agriculture; Spatial panel model; Crop Production/Industries; Land Economics/Use; Research and Development/Tech Change/Emerging Technologies; Research Methods/ Statistical Methods; O18; Q18; R15; R38; R58.
Ano: 2008
URL: http://purl.umn.edu/6717

Why Don't Farmers Adopt Precision Farming Technologies in Cotton Production?
Provedor de dados: 31
Autores: Paudel,   Krishna P.; Pandit,   Mahesh; Mishra,   Ashok K.; Segarra,   Eduardo.
We used the 2009 Southern Cotton Precision Farming Survey data collected from farmers in twelve U.S. states (Alabama, Arkansas, Florida, Georgia, Louisiana, Missouri, Mississippi, North Carolina, South Carolina, Tennessee, Texas, and Virginia) to understand why farmers do not adopt seemingly profitable precision farming technology. Farmers provided cost, time constraint, satisfaction with the current practice and other as reasons for not adopting precision farming technology. Results from a multinomial logit regression model indicated that manure application on field, more formal education, larger farm size, participation in conservation easement or agricultural easement generally decreases the probability of nonadoption of precision agriculture in cotton...
Tipo: Conference Paper or Presentation
Palavras-chave: Precision agriculture; Technology adoption; Multinomial logit; Crop Production/Industries; Farm Management; Research and Development/Tech Change/Emerging Technologies; C25; Q16.
Ano: 2011
URL: http://purl.umn.edu/104828

Economic Analysis of Phosphorus Applications under Variable and Single-Rate Applications in the Bothaville District
Provedor de dados: 31
Autores: Maine,   Ntsikane; Nell,   Wilhelm T.; Lowenberg-DeBoer,   James; Alemu,   Zerihun Gudeta.
Variable-rate (VR) application of inputs in South African cash crop production is mainly concerned with fertilizer and lime, and this indicates the importance of these inputs in cash crop production. However, the profitability of VR application of inputs has not yet been investigated under South African conditions. This paper studies the maize yield response to variable-rate application of phosphorus (P) and the profitability thereof in South Africa, on the basis of data collected on a 104-hectare experimental field on a farm in the Bothaville district. The strip-plot design of 180 strips was used for this on-farm research experiment. This design involved treatments that run in the same direction across the field as planting and harvesting. The objective...
Tipo: Journal Article
Palavras-chave: Precision agriculture; Precision farming; Site-specific phosphorus management; Variable-rate application; Fertilizer; Yield response; South Africa; Crop Production/Industries.
Ano: 2007
URL: http://purl.umn.edu/7047

On the Economics of Precision Agriculture: Technical, Informational and Environmental Aspects
Provedor de dados: 31
Autores: Anvec,   Tihomir; Whelan,   Brett; McBratney,   Alex.
The paper presents an integrated framework of biophysical and economic modelling as a novel approach towards precision agriculture research. A theoretical economic model determining the optimal number of precision agriculture management units within a given field of land is presented. The model is expanded to account for the value of the research information provided be the precision agriculture researchers. Since the inherent environmental values associated with precision agriculture are often omitted from the economic analysis, an attempt is made to incorporate these values into the model. The versions of the model are empirically tested using the data available.
Tipo: Conference Paper or Presentation
Palavras-chave: Economics; Precision agriculture; Environment; Information; Agribusiness; Environmental Economics and Policy.
Ano: 2004
URL: http://purl.umn.edu/58362

Socioeconomic Profiles of Early Adopters of Precision Agriculture Technologies
Provedor de dados: 31
Autores: Daberkow,   Stan G.; McBride,   William D.
Corn producers are the largest users of cropland and agrichemicals in U.S. agriculture, and represent a major market for precision agriculture technologies. Based on a USDA survey of 950 corn-producing farms, approximately 9% utilized some aspect of precision agriculture for corn production in 1996. A logit analysis indicated that farmers were more likely to adopt precision technologies if they farmed a large number of corn acres, earned a sizable farm income, and had high expected corn yields. The probability of adoption was also higher for farm operators using a computerized farm record system, who were less than 50 years of age, and who relied on crop consultants for information on precision agriculture.
Tipo: Journal Article
Palavras-chave: Corn farms; Logit analysis; Precision agriculture; Precision farming; Technology adoption; Agribusiness; Research and Development/Tech Change/Emerging Technologies.
Ano: 1998
URL: http://purl.umn.edu/90442

2008 PRECISION AGRICULTURAL SERVICES DEALERSHIP SURVEY RESULTS
Provedor de dados: 31
Autores: Whipker,   Linda D.; Akridge,   Jay T.
Precision technologies are now well-integrated into the agricultural industry – both at the farm level and at the crop input dealer level.  No longer are crop input dealers only using the technologies to bring new services to their customers, they are also utilizing the technology in their own businesses to improve the efficiency and effectiveness of their operations.  In early 2008, Crop Life magazine and Purdue University’s Center for Food and Agricultural Business conducted a survey for the 13th consecutive year to assess the adoption of precision agriculture practices in the U.S. from the perspective of the retail crop input dealer.  The questionnaire was mailed to 2500 retail crop input dealerships across the U.S.  A total of 298 questionnaires were...
Tipo: Working or Discussion Paper
Palavras-chave: Precision agriculture; Geographic information systems (GIS); Crop input dealer; Variable rate application; Site-specific agriculture; Technology adoption.; Agribusiness; Crop Production/Industries; Research and Development/Tech Change/Emerging Technologies; Q13; O30; L84.
Ano: 2008
URL: http://purl.umn.edu/46427

Using Spatial Analysis to Study the Values of Variable Rate Technology and Information
Provedor de dados: 31
Autores: Bullock,   David S.; Lowenberg-DeBoer,   James.
We present a review of the last few years' literature on the economic feasibility of variable rate technology in agriculture.  Much of the research on this topic has involved the estimation of site-specific yield response functions.  Data used for such estimations most often inherently lend themselves to spatial analysis.  We discuss the different types of spatial analyses that may be appropriate in estimating various types yield response functions.  Then, we present a taxonomy for the discussion of the economics of precision agriculture technology and information.  We argue that precision agriculture technology and information must be studied together since they are by nature economic complements. We contend that longer-term, multi-location agronomic...
Tipo: Conference Paper or Presentation
Palavras-chave: Precision agriculture; Spatial econometrics; Variable rate technology; Research and Development/Tech Change/Emerging Technologies; C31; O33; Q16.
Ano: 2006
URL: http://purl.umn.edu/25393

Green Technologies for a More Sustainable Agriculture
Provedor de dados: 31
Autores: Hrubovcak,   James; Vasavada,   Utpal; Aldy,   Joseph E.
For U.S. agriculture to continue along a sustainable path of economic development, further production increases must be generated by technologies that are both profitable and more environmentally benign. In this context, we assess the role of these green or sustainable technologies in steering agriculture along a more sustainable path. However, the lack of markets for the environmental attributes associated with green technologies can limit their development. In addition, simply making a technology available does not mean it will be adopted. Experience with green technologies such as conservation tillage, integrated pest management, enhanced nutrient management, and precision agriculture demonstrates that even when technologies are profitable, barriers to...
Tipo: Report
Palavras-chave: Sustainable agriculture; Natural capital; Nonrenewable resources; Renewable resources; Environmental services; Green technology; Integrated pest management; Conservation tillage; Enhanced nutrient management; Precision agriculture; Environmental Economics and Policy; Farm Management.
Ano: 1999
URL: http://purl.umn.edu/33721

Economics of the Variable Rate Technology Investment Decision for Agricultural Sprayers
Provedor de dados: 31
Autores: Mooney,   Daniel F.; Larson,   James A.; Roberts,   Roland K.; English,   Burton C.
Producers lack information about the profitability of variable rate technology (VRT) for agricultural sprayers. An economic framework was developed to evaluate the returns required to pay for VRT investments. Payback variables included input savings, yield gains, and reduced application costs. We illustrate the framework with two example investment scenarios.
Tipo: Conference Paper or Presentation
Palavras-chave: Capital budgeting; Decision aid; Farm management; Precision agriculture; Map-based; Sensor-based; Site-specific management; Variable rate technology; Farm Management; Q10; Q16.
Ano: 2009
URL: http://purl.umn.edu/46860

Cost Sensitivity Analysis on the Optimal Location of Technology Providers In Kentucky
Provedor de dados: 31
Autores: Shockley,   Jordan M.; Saghaian,   Sayed H.; Dillon,   Carl R.
A warehouse location model was utilized in order to expand upon previous research.   The aim was to more accurately depicting the optimal location for an agribusiness firm providing precision agriculture technologies in the state of Kentucky. It was determined that the optimal solution was Muhlenberg County.
Tipo: Conference Paper or Presentation
Palavras-chave: Warehouse location model; Precision agriculture; Agribusiness; Agribusiness.
Ano: 2007
URL: http://purl.umn.edu/34875

Best fit model selection for spatial differences (regression) in the profitability analysis of precision phosphate (P) application to winter cereals in Precision Agriculture (PA)
Provedor de dados: 31
Autores: Hough,   Ella Christina; Nell,   Wilhelm T.; Maine,   Ntsikane; Groenewald,   Jan A.; van der Rijst,   M.
Phosphates (P) are an important nutrient required by every living plant and animal cell, and deficiencies in soils could cause limited crop production, thereby reducing profitability. Phosphates are also a primary nutrient essential for root development and crop production, and are needed in the tissues of a plant where cells rapidly divide and enlarge. Precision agriculture (PA) could assist the farmer in applying the correct amount of P to the part of the field where it is required most. Variable rate technology (VRT) is a potential tool that can help with the development of strategies for phosphate fertilizer management. On-field trials were conducted on a commercial farm in the Western Cape Province; As many as five soil types occur on each field...
Tipo: Journal Article
Palavras-chave: Precision agriculture; Variable-rate phosphate application; Single rate phosphate application; Profitability; Spatial differences; Restricted maximum-likelihood model (RELM); Spatial regression; Best fit model selection; South Africa; Crop Production/Industries.
Ano: 2010
URL: http://purl.umn.edu/96642

Estimating the Potential Value of Variable Rate Nitrogen Applications: A Comparison of Spatial Econometric and Geostatistical Models
Provedor de dados: 31
Autores: Hurley,   Terrance M.; Oishi,   Kikuo; Malzer,   Gary L.
Site-specific crop response functions (SSCRFs) are useful for estimating the value of variable rate nitrogen applications (VRA), but appropriate statistical models are necessary. Problems estimating SSCRFs using experimental field data include region, spatial, treatment, and strip dependent heteroskedasticity and correlation. We develop a spatial autoregressive error (SARE) model for dealing with these problems and compare results with previous analysis based on a geostatistical (GEO) model. VRA value estimates for the two models differ notably for 1995 data from Southern Minnesota. Furthermore, findings show that the results of a comparison of model performance are location specific.
Tipo: Journal Article
Palavras-chave: Geostatistics; Precision agriculture; Site-specific crop response functions; Spatial autoregressive error; Variable rate nitrogen application; Crop Production/Industries.
Ano: 2005
URL: http://purl.umn.edu/31210

New Precision Agriculture Technology Adoption for Dealers under Imperfect Market
Provedor de dados: 31
Autores: Jia,   Haili.
Replaced with revised version of paper 02/23/07.
Tipo: Conference Paper or Presentation
Palavras-chave: Precision agriculture; Real option; Demand uncertainty; New technique uncertainty; Noise; Research and Development/Tech Change/Emerging Technologies.
Ano: 2007
URL: http://purl.umn.edu/34951

Factors Affecting Perceived Improvements in Environmental Quality from Precision Farming
Provedor de dados: 31
Autores: Larkin,   Sherry L.; Perruso,   Larry; Marra,   Michele C.; Roberts,   Roland K.; English,   Burton C.; Larson,   James A.; Cochran,   Rebecca L.; Martin,   Steven W.
This study identified the factors that influenced whether farmers in the Southeastern United States perceived an improvement in environmental quality from adopting precision farming technologies (PFTs). Farmers with larger farms or higher yields were more likely to believe that they observed positive externalities associated with PFTs. Farmers who found PFTs profitable or who believed input reduction was important had higher probabilities whereas those with higher incomes or who were more dependent on farm income were less likely to perceive such benefits. Interestingly, the importance of environmental quality and length of time using PFTs were not found to affect the probability of perceiving an improvement in environmental quality.
Tipo: Journal Article
Palavras-chave: Precision agriculture; Site-specific farming; Variable rate application; C25; Q12; Q24.
Ano: 2005
URL: http://purl.umn.edu/42787

Precision livestock tools to improve products and processes in broiler production: a review
Provedor de dados: 89
Autores: Mollo,MN; Vendrametto,O; Okano,MT.
Economic growth and production process development require technological support. Technology changes production functions, enabling a higher number of goods to be produced using the same amount of input. In this review, we discuss research and development in information technology that has led to innovative actions, with the new generation of tools, known as precision agriculture tools, that can be applied in Brazilian poultry production. In this context, research and development have focused on producing technological innovations based on increasingly specialized tools that go beyond human mind power, and are related to the acquisition, access, and processing of a huge number of data. The technology generated to date has assimilated the knowledge of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agribusiness; Decision support system; Precision agriculture; Research and development; Technological innovation.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-635X2009000400001

Strategy of specification of management areas: rice grain yield as related to soil fertility
Provedor de dados: 90
Autores: Dalchiavon,Flávio Carlos; Carvalho,Morel de Passos e; Montanari,Rafael; Andreotti,Marcelo.
It is well-known nowadays that soil variability can influence crop yields. Therefore, to determine specific areas of soil management, we studied the Pearson and spatial correlations of rice grain yield with organic matter content and pH of an Oxisol (Typic Acrustox) under no- tillage, in the 2009/10 growing season, in Selvíria, State of Mato Grosso do Sul, in the Brazilian Cerrado (longitude 51º24' 21'' W, latitude 20º20' 56'' S). The upland rice cultivar IAC 202 was used as test plant. A geostatistical grid was installed for soil and plant data collection, with 120 sampling points in an area of 3.0 ha with a homogeneous slope of 0.055 m m-1. The properties rice grain yield and organic matter content, pH and potential acidity and aluminum content were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Soil fertility; Geostatistics; Spatial variability; Oryza sativa.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832013000100005

Multivariate analysis and geostatistics of the fertility of a humic rhodic hapludox under coffee cultivation
Provedor de dados: 90
Autores: Silva,Samuel de Assis; Lima,Julião Soares de Souza.
The spatial variability of soil and plant properties exerts great influence on the yeld of agricultural crops. This study analyzed the spatial variability of the fertility of a Humic Rhodic Hapludox with Arabic coffee, using principal component analysis, cluster analysis and geostatistics in combination. The experiment was carried out in an area under Coffea arabica L., variety Catucai 20/15 - 479. The soil was sampled at a depth 0.20 m, at 50 points of a sampling grid. The following chemical properties were determined: P, K+, Ca2+, Mg2+, Na+, S, Al3+, pH, H + Al, SB, t, T, V, m, OM, Na saturation index (SSI), remaining phosphorus (P-rem), and micronutrients (Zn, Fe, Mn, Cu and B). The data were analyzed with descriptive statistics, followed by principal...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffea arabica L; Precision agriculture; Principal components; Cluster analysis.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832012000200016

Cacao Crop Management Zones Determination Based on Soil Properties and Crop Yield
Provedor de dados: 90
Autores: Carvalho,Perla Silva Matos de; Franco,Laís Barreto; Silva,Samuel de Assis; Sodré,George Andrade; Queiroz,Daniel Marçal de; Lima,Julião Soares de Souza.
ABSTRACT: The use of management zones has ensured yield success for numerous agricultural crops. In spite of this potential, studies applying precision agricultural techniques to cacao plantations are scarce or almost nonexistent. The aim of the present study was to delineate management zones for cacao crop, create maps combining soil physical properties and cacao tree yield, and identify what combinations best fit within the soil chemical properties. The study was conducted in 2014 on a cacao plantation in a Nitossolo Háplico Eutrófico (Rhodic Paleudult) in Bahia, Brazil. Soil samples were collected in a regular sampling grid with 120 sampling points in the 0.00-0.20 m soil layer, and pH(H2O), P, K+, Ca2+, Mg2+, Na+, H+Al, Fe, Zn, Cu, Mn, SB, V, TOC,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Unsupervised classification; Soil fertility.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832016000100312

SPATIAL DEPENDENCE OF ELECTRICAL CONDUCTIVITY AND CHEMICAL PROPERTIES OF THE SOIL BY ELECTROMAGNETIC INDUCTION
Provedor de dados: 90
Autores: Machado,Flavia Cristina; Montanari,Rafael; Shiratsuchi,Luciano Shozo; Lovera,Lenon Henrique; Lima,Elizeu de Souza.
Brazilian soils have natural high chemical variability; thus, apparent electrical conductivity (ECa) can assist interpretation of crop yield variations. We aimed to select soil chemical properties with the best linear and spatial correlations to explain ECa variation in the soil using a Profiler sensor (EMP-400). The study was carried out in Sidrolândia, MS, Brazil. We analyzed the following variables: electrical conductivity - EC (2, 7, and 15 kHz), organic matter, available K, base saturation, and cation exchange capacity (CEC). Soil ECa was measured with the aid of an all-terrain vehicle, which crossed the entire area in strips spaced at 0.45 m. Soil samples were collected at the 0-20 cm depth with a total of 36 samples within about 70 ha. Classical...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Electrical conductivity; Management zones.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832015000401112

Spatial relationships between soil attributes and corn yield in no-tillage system
Provedor de dados: 90
Autores: Rodrigues,Marcos Sales; Corá,José Eduardo; Fernandes,Carolina.
Soil properties play an important role in spatial variability of crop yield. However, a low spatial correlation has generally been observed between maps of crop yield and of soil properties. The objectives of the present investigation were to assess the spatial pattern variability of soil properties and of corn yield at the same sampling intensity, and evaluate its cause-and-effect relationships. The experimental site was structured in a grid of 100 referenced points, spaced at 10 m intervals along four parallel 250 m long rows spaced 4.5 m apart. Thus, points formed a rectangle containing four columns and 25 rows. Therefore, each sampling cell encompassed an area of 45 m² and consisted of five 10 m long crop rows, in which the referenced points...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geostatistics; Precision agriculture; Soil sampling intensity; Spatial correlation; Zea mays.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832012000200029

Optical crop sensor for variable-rate nitrogen fertilization in corn: i - plant nutrition and dry matter production
Provedor de dados: 90
Autores: Bragagnolo,Jardes; Amado,Telmo Jorge Carneiro; Nicoloso,Rodrigo da Silveira; Jasper,Joerg; Kunz,Junior; Teixeira,Tiago de Gregori.
Variable-rate nitrogen fertilization (VRF) based on optical spectrometry sensors of crops is a technological innovation capable of improving the nutrient use efficiency (NUE) and mitigate environmental impacts. However, studies addressing fertilization based on crop sensors are still scarce in Brazilian agriculture. This study aims to evaluate the efficiency of an optical crop sensor to assess the nutritional status of corn and compare VRF with the standard strategy of traditional single-rate N fertilization (TSF) used by farmers. With this purpose, three experiments were conducted at different locations in Southern Brazil, in the growing seasons 2008/09 and 2010/11. The following crop properties were evaluated: above-ground dry matter production, nitrogen...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Site-specific management; Optical spectrometry; Precision agriculture; Soil fertility.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832013000500018

Model to estimate the sampling density for establishment of yield mapping
Provedor de dados: 91
Autores: Spezia,Graciele R.; Souza,Eduardo G. de; Nóbrega,Lúcia H. P.; Uribe-Opazo,Miguel A.; Milan,Marcos; Bazzi,Claudio L.
Yield mapping represents the spatial variability concerning the features of a productive area and allows intervening on the next year production, for example, on a site-specific input application. The trial aimed at verifying the influence of a sampling density and the type of interpolator on yield mapping precision to be produced by a manual sampling of grains. This solution is usually adopted when a combine with yield monitor can not be used. An yield map was developed using data obtained from a combine equipped with yield monitor during corn harvesting. From this map, 84 sample grids were established and through three interpolators: inverse of square distance, inverse of distance and ordinary kriging, 252 yield maps were created. Then they were compared...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Thematic map; Spatial variability.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662012000400016

Geostatistical analysis of Arabic coffee yield in two crop seasons
Provedor de dados: 91
Autores: Carvalho,Luis C. C.; Silva,Fabio M. da; Ferraz,Gabriel A. e S.; Stracieri,Juliana; Ferraz,Patrícia F. P.; Ambrosano,Lucas.
ABSTRACT To make the coffee activity competitive, some farmers use precision coffee farming. Thus, it is possible to create thematic maps that guide management practices for regions where there are limitation for the plant development. The objective of this study was to identify the spatial dependence of coffee crop yield, in 2012 and 2013. The experimental area is located in a Haplustox in Três Pontas, Minas Gerais. One hundred sampling points were georeferenced for the collection of yield data through manual harvest. The difference of yield between crop seasons was also evaluated. Data were processed using geostatistical analysis. It was possible to identify and characterize the spatial dependence of all variables, as well as to create contour maps....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffea arabica L.; Spatial variability; Biennuality; Maps; Precision agriculture.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017000600410

Spatial variability of soil fertility and its relation with cocoa yield
Provedor de dados: 91
Autores: Santos,Railton O. dos; Franco,Laís B.; Silva,Samuel A.; Sodré,George A.; Menezes,Agna A.
ABSTRACT The knowledge on the spatial variability of soil properties and crops is important for decision-making on agricultural management. The objective of this study was to evaluate the spatial variability of soil fertility and its relation with cocoa yield. The study was conducted over 14 months in an area cultivated with cocoa. A sampling grid was created to study soil chemical properties and cocoa yield (stratified in season, off-season and annual). The data were analyzed using descriptive and exploratory statistics, and geostatistics. The chemical attributes were classified using fuzzy logic to generate a soil fertility map, which was correlated with maps of crop yield. The soil of the area, except for the western region, showed possibilities ranging...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Cocoa; Spatial variability; Fuzzy logic.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017000200088

Performance of a variable-rate distribution system for simultaneous fertilizer application
Provedor de dados: 91
Autores: Barros,Murilo M. de; Volpato,Carlos E. S.; Silva,Fabio M. da; Conceição,Fagner G. da; Corrêa Júnior,Delorme; Ribeiro,Luiz F.
ABSTRACT The objective of this study was to evaluate the performance of a variable-rate fertilizer distribution system for coffee crop, simultaneously applying two products. Two types of tests were performed: transversal deposition and longitudinal deposition. The transversal deposition test, with tarps, aimed to quantify the variations between programmed and applied doses, using a completely randomized design (CRD), in a factorial scheme, and the Scott-Knott test at p &lt; 0.05. The longitudinal deposition test aimed to determine the distribution characteristics of the equipment along the displacement line, based on relative frequency values. In addition, the application rates on both sides of the distribution system were analysed using a CRD and the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffee production; Precision agriculture; Application at variable doses.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662016000200188

Effect of different conductor tubes on the longitudinal distribution of corn seeds
Provedor de dados: 91
Autores: Carpes,Dauto P.; Alonço,Airton dos S.; Rossato,Fernando P.; Veit,André A.; Souza,Lucas B. de; Francetto,Tiago R.
ABSTRACT The correct longitudinal distribution of seeds by the seeder machine is one of the features that most contributes to obtain an adequate plant stand and good crop yield. The objective of this study was to evaluate the longitudinal distribution of corn seeds by seed conductor tube types, combined with a horizontal perforated disc and a pneumatic meter, altering the seeding density rate. The experiment was conducted in a laboratory using a seed meter test bench. Treatments were a combination of two seed meters, six conductor tubes and four peripheral speeds for the meter disc, corresponding to densities of 60, 70, 80 and 90 thousand corn seeds per hectare and were organized in a three-factor scheme with four repetitions. By increasing the seeding...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural mechanization; Precision seeding; Precision agriculture; Row crop planter; Seed metering.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017000900657

Management zones in coffee cultivation
Provedor de dados: 91
Autores: Jacintho,João L.; Ferraz,Gabriel A. e S.; Silva,Fabio M. da; Santos,Sthéfany A.
ABSTRACT This study aimed to apply precision agriculture techniques in coffee production, using correlation analysis in the definition of management zones. This work was carried out in a 22-ha area of coffee (Coffea arabica L.), cv. ‘Topázio MG 1190’, which was sampled on a regular grid, using a topographic GPS, totaling 64 georeferenced samples (on average, 2.9 points per ha). Descriptive analysis was used in the data, followed by Pearson’s correlation analysis at 0.05 significance between soil chemical attributes, agronomic characteristics of the plants and altitude. It was possible to verify the correlation of soil chemical attributes, agronomic characteristics of the plants and altitude with coffee yield. Altitude was the variable most correlated with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffea arabica L.; Precision agriculture; Yield; Thematic mapping.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017000200094

Parallelism error in peanut sowing operation with auto-steer guidance
Provedor de dados: 91
Autores: Santos,Adão F. dos; Silva,Rouverson P. da; Tavares,Tiago O.; Ormond,Antonio T. S.; Rosalen,David L.; Assis,Leonardo C. de.
ABSTRACT GNSS positioning errors are certain, regardless of the adopted positioning method. In agriculture, these errors may represent higher or lower overlapping rates between passes of a mechanical assembly, affecting operation quality. Therefore, this study evaluated the main errors arising from peanut sowing operation performed with an auto-steer guidance system by an RTX signal, using the Statistical Process Control techniques. The errors evaluated were: in tractor lateral displacement, project execution, and parallelism between passes of tractor-seeder set. The average errors of project execution in all passes were within the range specified by the manufacturer, i.e. lower than 3.8 cm. The average error of tractor-seeder set was also within the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Autopilot; Precision agriculture; Electric auto-steering; RTX; GNSS.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017001000731

Spatial variability of soil attributes and sugarcane yield in relation to topographic location
Provedor de dados: 91
Autores: Souza,Zigomar M. de; Cerri,Domingos G. P.; Magalhães,Paulo S. G.; Siqueira,Diego S.
Soils submitted to the same management system in places with little variation of landscape, manifest differentiated spatial variability of their attributes and crop yield. The aim of this work was to investigate the correlation between spatial variability of the soil attributes and sugarcane yield as a result of soil topography. To achieve this objective, a test area of 42 ha located at the São João Sugar Mill, in Araras, in the State of São Paulo, Brazil, was selected. Sugarcane yield was measured with a yield monitor fitted in a sugarcane harvester and GPS signal. A total of 170 soil samples were taken at regular 50 m grid, at a depth of 0 - 0.2 m. The area under study was divided into two sites based on topography. The following soil attributes were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum sp; Geostatistics; Semivariogram; Curvature; Precision agriculture.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662010001200001

Spatial and temporal distribution of weeds in no-tillage system
Provedor de dados: 91
Autores: Bottega,Eduardo L.; Pegoraro,Camilo; Guerra,Naiara; Oliveira Neto,Antonio M. de; Queiroz,Daniel M. de.
ABSTRACT Brazil is one of the largest grain producers in the world, due to its extensive arable land and favorable climate for the cultivation of any species. The production could be higher, but problems such as competition between crops and weeds reduces crop yields. This study aimed to analyze the spatial distribution of weeds, especially milkweed (Sonchus oleraceus), horse weed (Conyza spp.) and ‘maria-mole’ (Senecio brasiliensis) in an area under no-tillage system for two harvests. The work was carried out during the 2013/14 and 2014/15 crop years in an area of 22.5 ha, where soybean is grown in the summer and oat in the winter. The weeds were mapped using a sampling grid of 85 points. The number of plants present in 0.25 m2 was recorded at each...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Spatial variability; Sonchus oleraceus; Conyza spp.; Senecio brasiliensis.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662016001201107

Performance evaluation of injection metering systems
Provedor de dados: 91
Autores: Antuniassi,Ulisses R.; Miller,Paul; Paice,Mark.
A method for measuring the performance of agricultural injection metering systems was developed and used to assess the characteristics of three commercial system designs. Steady-state characteristics were measured using both colored dyes and salt as tracers. Dynamic response characteristics were determined by measuring salt concentration downstream of the injection point by monitoring electrical conductivity of the spray solution. Salt added to a viscous test liquid changed viscosity slightly only at low shear rates and it is concluded that this liquid is appropriate for use in evaluation tests with injection systems. Results from tests with 2 systems specifically designed for operation with agricultural sprayers gave a linear response with both water and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Sprayers; Pesticides.
Ano: 2002
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662002000100028

Using a field radiometer to estimate instantaneous sky clearness
Provedor de dados: 91
Autores: Souza,Eduardo G.; Scharf,Peter; Sudduth,Ken A.; Hipple,James. D.
Reflectance measurements of crop plants and canopies show promise for guiding within-season, variable-rate nitrogen (N) application. Most research results have been obtained around solar noon with clear skies. However, for practical application, the system must work under cloudy skies or away from solar noon. The objective of this work was to assess the effect of cloud conditions on reflectance measurements of a corn canopy. The approach was to estimate an instantaneous sky clearness index (ICI) which could be used to correct field radiometer data for variations in cloud cover, such that the same reflectance reading would be obtained (and the same N recommendation made) for the same plants regardless of cloud conditions. Readings were taken from morning...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Nitrogen management; Reflectance; Cloud.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662006000200018

Sampling grid density and lime recommendation in an Oxisol
Provedor de dados: 91
Autores: Bottega,Eduardo L.; Queiroz,Daniel M. de; Pinto,Francisco A. C.; Oliveira Neto,Antonio M. de; Vilar,Cesar C.; Souza,Cristiano M. A. de.
The objective of this study was to evaluate the influence of different sampling grids density in the lime requirements in an Oxisol. The experiment was conducted at a rural property located in Sidrolândia city, Mato Grosso do Sul state, in the Brazilian ‘Cerrado’. In the soil attributes mapping, regular sampling grid was used consisting of 99 points, spread over an area of 90 ha. Other two grids (51 and 27 points) were derived by deleting lines or lines and points from the original one. Based on the results of soil analysis, the lime requirement at each sample point was calculated. Using geostatistical techniques the spatial variability of lime requirement was studied and grid configuration for each sample was tested. By kriging, maps were made. By...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Geostatistics; Spatial variability; Soil acidity correction.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662014001100008

Yield mapping, soil fertility and tree gaps in an orange orchard
Provedor de dados: 94
Autores: Molin,José Paulo; Colaço,André Freitas; Carlos,Eduardo Fermino; Mattos Junior,Dirceu de.
The current high competition on Citrus industry demands from growers new management technologies for superior efficiency and sustainability. In this context, precision agriculture (PA) has developed techniques based on yield mapping and management systems that recognize field spatial variability, which contribute to increase profitability of commercial crops. Because spatial variability is often not perceived the orange orchards are still managed as uniform and adoption of PA technology on citrus farms is low. Thus, the objective of the present study was to characterize the spatial variability of three factors: fruit yield, soil fertility and occurrence of plant gaps caused by either citrus blight or huanglongbing (HLB) in a commercial Valencia orchard in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Spatial variability; Citrus blight; Huanglongbing (HLB).
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-29452012000400035

Spatial variability of soil fertility and its relationship with seed physiological potential in a soybean production area
Provedor de dados: 95
Autores: Mondo,Vitor Henrique Vaz; Gomes Junior,Francisco Guilhien; Pinto,Taís Leite Ferreira; Marchi,José Luis de; Motomiya,Anamari Viegas de Araújo; Molin,José Paulo; Cicero,Silvio Moure.
The correlation of soil fertility x seed physiological potential is very important in the area of seed technology but results published with that theme are contradictory. For this reason, this study to evaluate the correlations between soil chemical properties and physiological potential of soybean seeds. On georeferenced points, both soil and seeds were sampled for analysis of soil fertility and seed physiological potential. Data were assessed by the following analyses: descriptive statistics; Pearson's linear correlation; and geostatistics. The adjusted parameters of the semivariograms were used to produce maps of spatial distribution for each variable. Organic matter content, Mn and Cu showed significant effects on seed germination. Most variables...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Glycine max; Precision agriculture; Seed quality.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0101-31222012000200002

Apparent soil electrical conductivity in two different soil types
Provedor de dados: 124
Autores: Medeiros,Wilker Nunes; Valente,Domingos Sárvio Magalhães; Queiroz,Daniel Marçal de; Pinto,Francisco de Assis de Carvalho; Assis,Igor Rodrigues de.
ABSTRACT  Mapping the apparent soil electrical conductivity (ECa) has become important for the characterization of the soil variability in precision agriculture systems. Could the ECa be used to locate the soil sampling points for mapping the chemical and physical soil attributes? The objective of this work was to examine the relations between ECa and soil attributes in two fields presenting different soil textures. In each field, 50 sampling points were chosen using a path that presented a high variability of ECa obtained from a preliminary ECa map. At each sampling point, the ECa was measured in soil depths of 0-20, 0-40 and 0-60 cm. In addition, at each point, soil samples were collected for the determination of physical and chemical attributes in the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Management zones; Soil sampling.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1806-66902018000100043

The relationship between apparent soil electrical conductivity and soil properties
Provedor de dados: 124
Autores: Valente,Domingos Sárvio Magalhães; Queiroz,Daniel Marçal de; Pinto,Francisco de Assis de Carvalho; Santos,Nerilson Terra; Santos,Fábio Lúcio.
Precision agriculture that is based on the physical and chemical properties of soil requires a dense sampling to evaluate spatial variability in the field. This dense sampling is often expensive and time consuming. One technique to reduce the number of samples is to define management zones based on information that is collected in the field. Some researchers have demonstrated the importance of the electrical properties of soil in defining management zones. Thus, the objective of this study was to evaluate the relationship between the apparent soil electrical conductivity and soil properties in mountainous areas of coffee production. The electrical conductivity of soil was evaluated at soil depths ranging from 0.00-0.20 m (EC20) and 0.00-0.40 m (EC40) using...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Management zone; Sensors.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1806-66902012000400009

Estimation of soil phosphorus availability via visible and near-infrared spectroscopy
Provedor de dados: 63
Autores: Souza,Micael Felipe de; Franco,Henrique Coutinho Junqueira; Amaral,Lucas Rios do.
ABSTRACT: Spectroscopic techniques have great potential to evaluate soil properties. However, there are still questions regarding the applicability of spectroscopy to analyze soil phosphorous (P) availability, especially in tropical soils with low nutrient contents. Therefore, this study evaluated the possibility to estimate P availability in soil and its pools (labile, moderately labile and non-labile) via Vis-NIR spectroscopy based on intra-field calibration. We used soils from two different locations, a plot experiment that received application of phosphate fertilizers (Field-A) and a cultivated field where a grid soil sampling was performed (Field-B). We used the technique of diffuse reflectance in the visible and near-infrared (Vis-NIR) to obtain the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Predictive modeling; Classification model; Precision agriculture; Fractionation of phosphorus; Soil fertility.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162020000501601

Spatial and temporal variability of soil electrical conductivity related to soil moisture
Provedor de dados: 63
Autores: Molin,José Paulo; Faulin,Gustavo Di Chiacchio.
Soil electrical conductivity (ECa) is a soil quality indicator associated to attributes interesting to site-specific soil management such as soil moisture and texture. Soil ECa provides information that helps guide soil management decisions, so we performed spatial evaluation of soil moisture in two experimental fields in two consecutive years and modeled its influence on soil ECa. Soil ECa, moisture and clay content were evaluated by statistical, geostatistical and regression analyses. Semivariogram models, adjusted for soil moisture, had strong spatial dependence, but the relationship between soil moisture and soil ECa was obtained only in one of the experimental fields, where soil moisture and clay content range was higher. In this same field,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Soil physics; Geostatistics; Soil sensors.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162013000100001

Methodology to filter out outliers in high spatial density data to improve maps reliability
Provedor de dados: 63
Autores: Maldaner,Leonardo Felipe; Molin,José Paulo; Spekken,Mark.
ABSTRACT The considerable volume of data generated by sensors in the field presents systematic errors; thus, it is extremely important to exclude these errors to ensure mapping quality. The objective of this research was to develop and test a methodology to identify and exclude outliers in high-density spatial data sets, determine whether the developed filter process could help decrease the nugget effect and improve the spatial variability characterization of high sampling data. We created a filter composed of a global, anisotropic, and an anisotropic local analysis of data, which considered the respective neighborhood values. For that purpose, we used the median to classify a given spatial point into the data set as the main statistical parameter and took...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Local analysis; Map accuracy.
Ano: 2022
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162022000100102

Establishing management zones using soil electrical conductivity and other soil properties by the fuzzy clustering technique
Provedor de dados: 63
Autores: Molin,José Paulo; Castro,Cesar Nunes de.
The design of site-specific management zones that can successfully define uniform regions of soil fertility attributes that are of importance to crop growth is one of the most challenging steps in precision agriculture. One important method of so proceeding is based solely on crop yield stability using information from yield maps; however, it is possible to accomplish this using soil information. In this study the soil was sampled for electrical conductivity and eleven other soil properties, aiming to define uniform site-specific management zones in relation to these variables. Principal component analysis was used to group variables and fuzzy logic classification was used for clustering the transformed variables. The importance of electrical conductivity...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Soil physical properties; Fuzziness.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162008000600001