Consulta: subjectFacets:"Processo kraft"
Registros recuperados: 1
Data/hora: 09/06/2024 17:09:49

Cellulose pulp produced from bulrush fiber
Provedor de dados: 65
Autores: Wille,Vania Karine Dick; Pedrazzi,Cristiane; Colodette,Jorge Luiz; Oliveira,Rubens Chaves de; Coldebella,Rodrigo; Giesbrecht,Bruna Mohr; Saccol,Angelo Fernando de Oliveira.
ABSTRACT: Brazil continues to use wood as the principal raw material source for the pulp industry; although, non-wood fibers have been revealed to be a competent substitute to produce paper with different and exceptional properties. Keeping this in focus, this study aimed to assess potential of Schoenoplectus californicus fibers (C. A. Mey.) Soják, commonly identified as bulrush or reed, in cellulosic pulp generation, as an alternative fiber source for the pulp and paper industry. On analyzing the chemical composition of reed fibers, extractives of lignin, carbohydrates, uronic acids and minerals were reported. Physico-chemical characteristics of reed-based cellulosic pulp were estimated including viscosity, hexenuronic acids, etc., as well as anatomical...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Schoenoplectus californicus; Caracterização química; Processo kraft.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782017000500403