Consulta: subjectFacets:"Shipboard experiments"
Registros recuperados: 1
Data/hora: 09/06/2024 06:48:46

First Steps of in Situ Surface-Enhanced Raman Scattering During Shipboard Experiments
Provedor de dados: 5
Autores: Peron, Olivier; Rinnert, Emmanuel; Colas, Florent; Lehaitre, Michel; Compere, Chantal.
It is shown that the surface-enhanced Raman scattering (SERS) technique can be applied to detect organic molecules during in situ experiments. To this purpose, we used trans-1,2-bis(4-pyridyl)ethylene (BPE) as a target molecule. Adsorbed on the SERS chemosensor surface and excited under laser, the vibration modes of the molecules can be identified. SERS chemosensors are based on quartz substrates functionalized by silanization and partially coated with gold nanoparticles. SERS measurements during shipboard experiments were made with a home-made in situ Raman spectrometer connected to a marinized micro-fluidic system. The device was designed to host chemosensors in order to ensure measurements with a flow cell. A theoretical limit of detection was estimated...
Tipo: Text
Palavras-chave: Surface-enhanced Raman scattering; SERS; Chemosensors; Flow cells; Shipboard experiments; In situ measurements; Freundlich isotherm.
Ano: 2010
URL: http://archimer.ifremer.fr/doc/00016/12691/9718.pdf