Consulta: subjectFacets:"SoiT consolidation"
Registros recuperados: 1
Data/hora: 15/06/2024 19:57:05

Modelling mud transport in a macrotidal estuary
Provedor de dados: 5
Autores: Le Hir, Pierre; Bassoullet, Philippe; L'Yavanc, Jacky.
In order to determine the fate of the fine particles and adsorbed contaminants in·a short macrotidal èstuary, a mathematical modelling system for cohesive suspended mater transport and bottom evolution, including a new consolidation algorithm, is developed. An analysis of successive erosion, transport and deposi~ion processes due to tidal forcing is given and comparisons with field data are provided. A description of mean-term bottom variations has been attempted and is partially validated by differential soundings.
Tipo: Text
Palavras-chave: Dynamique des sédiments cohésifs; Estuaire Morlaix; Tassement des vases; Modèle mathématique; Érosion; Dépôt; Cohesive sediment dynamics; Estuary; Erosion; Deposition; SoiT consolidation; Mathematical modelling.
Ano: 1988
URL: https://archimer.ifremer.fr/doc/00682/79379/81909.pdf