Consulta: subjectFacets:"Train de pêche"
Registros recuperados: 2
Data/hora: 12/06/2024 17:20:02

Etude numérique du train de pêche d'un chalutier (DEA)
Provedor de dados: 5
Autores: Theret, Francois.
IFREMER aims at digitalizing trawl gear in order to reach two goals: on the one hand, participating in the realisation of a computer assisted trawl conception software; on the other hand, being able to study quickly and easily the influence of different adjustment parameters on the shape of the trawl in order to indicate to the skipper, if possible in real time, the optimal adjustment for the conditions he's in. From an international point of view, there are only two strategies to approach this problem: - the first strategy is based on statistical studies on the existing nets (almost limited to their reproduction on different scales), but this approach does not leave much room for innovation as it can only be applied to the same type of nets as those that...
Tipo: Text
Palavras-chave: Experimentation; Optimization; Adjustment; Hydrodynamic; Modelization; Trawl gear; Trawl; Expérimentation; Maquette de chalut; Optimisation; Réglage; Hydrodynamique; Modèle numérique; Train de pêche; Chalut.
Ano: 1990
URL: http://archimer.ifremer.fr/doc/1990/these-3627.pdf

Etude dynamique d'un train de pêche complet
Provedor de dados: 5
Autores: Marichal, Dominique; Vincent, Benoit.
We present a complete numerical model of a full trawl gear and the vessel. The trawler is modelled by equations and hydrodynamic coefficients which are classically used for ship behaviour and ship manoeuvrability studies. It is submitted to the action of the warps. The warps and the net are part of a complex fluid-structure coupling problem. The net is a supple structure and its shape depends on the forces that are acting on it. Now, these forces themselves depend of the net meshes shape. The otter boards are most particular wings. We have studied one particular type. Then all these elements have been put together by writing their dynamics equations. A time step method enables the calculation of the shape, the forces and the motion of each element in the...
Tipo: Text
Palavras-chave: Obstruction; Fishing accident; Manoeuvrability; Trawl door; Net; Trawl gear; Croche; Accident de pêche; Manoeuvrabilité; Panneau; Filet; Chalut; Train de pêche.
Ano: 2007
URL: http://archimer.ifremer.fr/doc/2007/acte-4617.pdf