Consulta: subjectFacets:"Usinage"
Registros recuperados: 1
Data/hora: 10/06/2024 07:44:08

Contribution a l'usinage des materiaux composites
Provedor de dados: 5
Autores: Guegan, P; Lemaitre, F; Hamann, J.
While machining is generally to be avoided in the fabrication of components with composite materials, nevertheless many parts require some machining, drilling or milling after moulding. Machining of these materials involves the risk of damage in the machined region. It is therefore important to study the possible sources of damage and to quantify their extent for different drilling and milling operations.
Tipo: Text
Palavras-chave: Damage; Drilling; Ship technology; Composite materials; Usinage; Matériau composite.
Ano: 1992
URL: http://archimer.ifremer.fr/doc/1992/acte-1080.pdf