Consulta: subjectFacets:"Wheel soil interaction"
Registros recuperados: 1
Data/hora: 11/06/2024 06:44:58

Contact pressures and the impact of farm equipment on Latosol with the presence and absence of sugarcane straw
Provedor de dados: 64
Autores: Silva,Reginaldo Barboza da; Iori,Piero; Souza,Zigomar Menezes de; Pereira,Danilo de Moraes Gomes; Vischi Filho,Oswaldo Julio; Silva,Francisca Alcivania de Melo.
ABSTRACT High contact pressures applied to soil result in a greater degree of compaction, in addition to promoting other negative effects. The objective of this study was to quantify contact areas by using different methodologies, and pressures of farm equipment employed in production activity and evaluate structural changes caused in a Red Latosol with the presence and absence of straw cover. The design was completely randomized in a factorial scheme of type 4 (tire on front axle, tire on rear axle, tire on a sugarcane wagon and metallic track of sugar cane Harvester) x 2 (presence and absence of straw). The contact area (CA) of the run was obtained by three procedures: analytical measure of the area of an ellipse (CA1); digital measurement of area of an...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Farming traction tire; Farming trailer tire; Metal track; Wheel soil interaction.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1413-70542016000300265